<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Modules - Step Down Converter - MagI³C-VDRM &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Eagle Version 9, Library Revision 2020a, 2019-04-14&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="MAGI³C-VDRM_TO263-7EP">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module
&lt;br&gt;&lt;/b&gt;Size : TO263-7EP</description>
</package>
<package name="MAGI³C-VDRM_LGA-16EP">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module
&lt;br&gt;&lt;/b&gt;Size : LGA-16EP</description>
</package>
<package name="MAGI³C-VDRM_BQFN_1710X0302">
</package>
<package name="MAGI³C-VDRM_BQFN_171021501">
</package>
</packages>
<symbols>
<symbol name="MAGI³C-VDRM_TO263-7EP">
<pin name="VIN"/>
<pin name="RON"/>
<pin name="EN"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="SS"/>
<pin name="FB"/>
<pin name="VOUT"/>
</symbol>
<symbol name="MAGI³C-VDRM_LGA-16EP">
<pin name="13FB"/>
<pin name="16EN"/>
<pin name="VIN1"/>
<pin name="VIN2"/>
<pin name="VIN3"/>
<pin name="VIN4"/>
<pin name="GND"/>
<pin name="10VOUT"/>
<pin name="11VOUT"/>
<pin name="12VOUT"/>
<pin name="9VOUT"/>
</symbol>
<symbol name="MAGI³C-VDRM_BQFN_171021501">
<pin name="2COMP"/>
<pin name="3RCCOMP"/>
<pin name="4AGND"/>
<pin name="5AGND"/>
<pin name="6SW"/>
<pin name="7SW"/>
<pin name="8NC"/>
<pin name="9NC"/>
<pin name="10VOUT"/>
<pin name="20PGND"/>
<pin name="21SW"/>
<pin name="22SW"/>
<pin name="23SW"/>
<pin name="24SW"/>
<pin name="25BOOT"/>
<pin name="26VIN"/>
<pin name="27EN/UVLO"/>
<pin name="28SS/TRK"/>
<pin name="29INTSS"/>
<pin name="30INTRRT"/>
<pin name="31RT/CLK"/>
<pin name="32AGND"/>
<pin name="33AGND"/>
<pin name="34AGND"/>
<pin name="35PG"/>
<pin name="36FB"/>
<pin name="1RSETINT"/>
<pin name="12VOUT"/>
<pin name="13VOUT"/>
<pin name="14VOUT"/>
<pin name="15VOUT"/>
<pin name="16PGND"/>
<pin name="17PGND"/>
<pin name="18PGND"/>
<pin name="19PGND"/>
<pin name="40PGND"/>
<pin name="41SW"/>
<pin name="11VOUT"/>
<pin name="38SW"/>
<pin name="39VOUT"/>
<pin name="37AGND"/>
</symbol>
<symbol name="MAGI³C-VDRM_BQFN">
<pin name="2CCOMP"/>
<pin name="3COMP"/>
<pin name="4RT/CLK"/>
<pin name="5INTRRT"/>
<pin name="6SS/TR"/>
<pin name="7INTSS"/>
<pin name="8VOUT"/>
<pin name="9VOUT"/>
<pin name="10VOUT"/>
<pin name="20SW"/>
<pin name="21SW"/>
<pin name="22SW"/>
<pin name="23SW"/>
<pin name="24SW"/>
<pin name="25SW"/>
<pin name="26BOOT"/>
<pin name="27PG"/>
<pin name="28ENABLE"/>
<pin name="29UVLO"/>
<pin name="30VIN"/>
<pin name="32VIN"/>
<pin name="33AGND"/>
<pin name="34AGND"/>
<pin name="35FB"/>
<pin name="36VSENSE+"/>
<pin name="1RCOMP"/>
<pin name="12VOUT"/>
<pin name="13VOUT"/>
<pin name="14VOUT"/>
<pin name="15NC"/>
<pin name="16NC"/>
<pin name="17SW"/>
<pin name="18SW"/>
<pin name="19SW"/>
<pin name="11VOUT"/>
<pin name="38VOUT"/>
<pin name="39SW"/>
<pin name="37PGND"/>
<pin name="31VIN"/>
</symbol>
<symbol name="MAGI³C-VDRM_TO263-7EP_171050601">
<pin name="VIN"/>
<pin name="SYNC"/>
<pin name="EN"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="SS/TRK"/>
<pin name="FB"/>
<pin name="VOUT"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171032401" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171032401.pdf"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171032401 "/>
<attribute name="V-INPUT" value="6-42V"/>
<attribute name="V-OUTPUT" value="5-24V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171020601" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171020601.pdf"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171020601 "/>
<attribute name="V-INPUT" value="6-42V"/>
<attribute name="V-OUTPUT" value="0.8-6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171050601" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP_171050601"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="SS/TRK" pad="6"/>
<connect gate="G$1" pin="SYNC" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171050601.pdf"/>
<attribute name="I-OUTPUT" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171050601 "/>
<attribute name="V-INPUT" value="6-36V"/>
<attribute name="V-OUTPUT" value="0.8-6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171012401" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171012401.pdf"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171012401 "/>
<attribute name="V-INPUT" value="6-42V"/>
<attribute name="V-OUTPUT" value="5-24V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171030601" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171030601.pdf"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171030601 "/>
<attribute name="V-INPUT" value="6-42V"/>
<attribute name="V-OUTPUT" value="0.8-6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171012402" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171012402.pdf"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171012402 "/>
<attribute name="V-INPUT" value="6-42V"/>
<attribute name="V-OUTPUT" value="5-24V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_TO263-7EP_171010601" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_TO263-7EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_TO263-7EP">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="PGND" pad="EP"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171010601.pdf"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171010601 "/>
<attribute name="V-INPUT" value="6-42V"/>
<attribute name="V-OUTPUT" value="0.8-6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_LGA-16EP_171031801" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_LGA-16EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_LGA-16EP">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13FB" pad="13"/>
<connect gate="G$1" pin="16EN" pad="16"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP1 EP2 EP3 EP4"/>
<connect gate="G$1" pin="VIN1" pad="1"/>
<connect gate="G$1" pin="VIN2" pad="2"/>
<connect gate="G$1" pin="VIN3" pad="3"/>
<connect gate="G$1" pin="VIN4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171031801.pdf"/>
<attribute name="I-OUTPUT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171031801 "/>
<attribute name="V-INPUT" value="4-18V"/>
<attribute name="V-OUTPUT" value="0.8-17V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_LGA-16EP_171011801" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_LGA-16EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_LGA-16EP">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13FB" pad="13"/>
<connect gate="G$1" pin="16EN" pad="16"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP1 EP2 EP3 EP4"/>
<connect gate="G$1" pin="VIN1" pad="1"/>
<connect gate="G$1" pin="VIN2" pad="2"/>
<connect gate="G$1" pin="VIN3" pad="3"/>
<connect gate="G$1" pin="VIN4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171011801.pdf"/>
<attribute name="I-OUTPUT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171011801 "/>
<attribute name="V-INPUT" value="4-18V"/>
<attribute name="V-OUTPUT" value="0.8-17V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_BQFN_171060302" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_BQFN"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_BQFN_1710X0302">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13VOUT" pad="13"/>
<connect gate="G$1" pin="14VOUT" pad="14"/>
<connect gate="G$1" pin="15NC" pad="15"/>
<connect gate="G$1" pin="16NC" pad="16"/>
<connect gate="G$1" pin="17SW" pad="17"/>
<connect gate="G$1" pin="18SW" pad="18"/>
<connect gate="G$1" pin="19SW" pad="19"/>
<connect gate="G$1" pin="1RCOMP" pad="1"/>
<connect gate="G$1" pin="20SW" pad="20"/>
<connect gate="G$1" pin="21SW" pad="21"/>
<connect gate="G$1" pin="22SW" pad="22"/>
<connect gate="G$1" pin="23SW" pad="23"/>
<connect gate="G$1" pin="24SW" pad="24"/>
<connect gate="G$1" pin="25SW" pad="25"/>
<connect gate="G$1" pin="26BOOT" pad="26"/>
<connect gate="G$1" pin="27PG" pad="27"/>
<connect gate="G$1" pin="28ENABLE" pad="28"/>
<connect gate="G$1" pin="29UVLO" pad="29"/>
<connect gate="G$1" pin="2CCOMP" pad="2"/>
<connect gate="G$1" pin="30VIN" pad="30"/>
<connect gate="G$1" pin="31VIN" pad="31"/>
<connect gate="G$1" pin="32VIN" pad="32"/>
<connect gate="G$1" pin="33AGND" pad="33"/>
<connect gate="G$1" pin="34AGND" pad="34"/>
<connect gate="G$1" pin="35FB" pad="35"/>
<connect gate="G$1" pin="36VSENSE+" pad="36"/>
<connect gate="G$1" pin="37PGND" pad="37"/>
<connect gate="G$1" pin="38VOUT" pad="38"/>
<connect gate="G$1" pin="39SW" pad="39"/>
<connect gate="G$1" pin="3COMP" pad="3"/>
<connect gate="G$1" pin="4RT/CLK" pad="4"/>
<connect gate="G$1" pin="5INTRRT" pad="5"/>
<connect gate="G$1" pin="6SS/TR" pad="6"/>
<connect gate="G$1" pin="7INTSS" pad="7"/>
<connect gate="G$1" pin="8VOUT" pad="8"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171060302.pdf"/>
<attribute name="I-OUTPUT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171060302 "/>
<attribute name="V-INPUT" value="2.95-6V"/>
<attribute name="V-OUTPUT" value="0.8-3.6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_LGA-16EP_171021801" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_LGA-16EP"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_LGA-16EP">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13FB" pad="13"/>
<connect gate="G$1" pin="16EN" pad="16"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP1 EP2 EP3 EP4"/>
<connect gate="G$1" pin="VIN1" pad="1"/>
<connect gate="G$1" pin="VIN2" pad="2"/>
<connect gate="G$1" pin="VIN3" pad="3"/>
<connect gate="G$1" pin="VIN4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171021801.pdf"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171021801 "/>
<attribute name="V-INPUT" value="4-18V"/>
<attribute name="V-OUTPUT" value="0.8-17V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_BQFN_171020302" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_BQFN"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_BQFN_1710X0302">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13VOUT" pad="13"/>
<connect gate="G$1" pin="14VOUT" pad="14"/>
<connect gate="G$1" pin="15NC" pad="15"/>
<connect gate="G$1" pin="16NC" pad="16"/>
<connect gate="G$1" pin="17SW" pad="17"/>
<connect gate="G$1" pin="18SW" pad="18"/>
<connect gate="G$1" pin="19SW" pad="19"/>
<connect gate="G$1" pin="1RCOMP" pad="1"/>
<connect gate="G$1" pin="20SW" pad="20"/>
<connect gate="G$1" pin="21SW" pad="21"/>
<connect gate="G$1" pin="22SW" pad="22"/>
<connect gate="G$1" pin="23SW" pad="23"/>
<connect gate="G$1" pin="24SW" pad="24"/>
<connect gate="G$1" pin="25SW" pad="25"/>
<connect gate="G$1" pin="26BOOT" pad="26"/>
<connect gate="G$1" pin="27PG" pad="27"/>
<connect gate="G$1" pin="28ENABLE" pad="28"/>
<connect gate="G$1" pin="29UVLO" pad="29"/>
<connect gate="G$1" pin="2CCOMP" pad="2"/>
<connect gate="G$1" pin="30VIN" pad="30"/>
<connect gate="G$1" pin="31VIN" pad="31"/>
<connect gate="G$1" pin="32VIN" pad="32"/>
<connect gate="G$1" pin="33AGND" pad="33"/>
<connect gate="G$1" pin="34AGND" pad="34"/>
<connect gate="G$1" pin="35FB" pad="35"/>
<connect gate="G$1" pin="36VSENSE+" pad="36"/>
<connect gate="G$1" pin="37PGND" pad="37"/>
<connect gate="G$1" pin="38VOUT" pad="38"/>
<connect gate="G$1" pin="39SW" pad="39"/>
<connect gate="G$1" pin="3COMP" pad="3"/>
<connect gate="G$1" pin="4RT/CLK" pad="4"/>
<connect gate="G$1" pin="5INTRRT" pad="5"/>
<connect gate="G$1" pin="6SS/TR" pad="6"/>
<connect gate="G$1" pin="7INTSS" pad="7"/>
<connect gate="G$1" pin="8VOUT" pad="8"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171020302.pdf"/>
<attribute name="I-OUTPUT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171020302 "/>
<attribute name="V-INPUT" value="2.95-6V"/>
<attribute name="V-OUTPUT" value="0.8-3.6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_BQFN_171040302" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_BQFN"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_BQFN_1710X0302">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13VOUT" pad="13"/>
<connect gate="G$1" pin="14VOUT" pad="14"/>
<connect gate="G$1" pin="15NC" pad="15"/>
<connect gate="G$1" pin="16NC" pad="16"/>
<connect gate="G$1" pin="17SW" pad="17"/>
<connect gate="G$1" pin="18SW" pad="18"/>
<connect gate="G$1" pin="19SW" pad="19"/>
<connect gate="G$1" pin="1RCOMP" pad="1"/>
<connect gate="G$1" pin="20SW" pad="20"/>
<connect gate="G$1" pin="21SW" pad="21"/>
<connect gate="G$1" pin="22SW" pad="22"/>
<connect gate="G$1" pin="23SW" pad="23"/>
<connect gate="G$1" pin="24SW" pad="24"/>
<connect gate="G$1" pin="25SW" pad="25"/>
<connect gate="G$1" pin="26BOOT" pad="26"/>
<connect gate="G$1" pin="27PG" pad="27"/>
<connect gate="G$1" pin="28ENABLE" pad="28"/>
<connect gate="G$1" pin="29UVLO" pad="29"/>
<connect gate="G$1" pin="2CCOMP" pad="2"/>
<connect gate="G$1" pin="30VIN" pad="30"/>
<connect gate="G$1" pin="31VIN" pad="31"/>
<connect gate="G$1" pin="32VIN" pad="32"/>
<connect gate="G$1" pin="33AGND" pad="33"/>
<connect gate="G$1" pin="34AGND" pad="34"/>
<connect gate="G$1" pin="35FB" pad="35"/>
<connect gate="G$1" pin="36VSENSE+" pad="36"/>
<connect gate="G$1" pin="37PGND" pad="37"/>
<connect gate="G$1" pin="38VOUT" pad="38"/>
<connect gate="G$1" pin="39SW" pad="39"/>
<connect gate="G$1" pin="3COMP" pad="3"/>
<connect gate="G$1" pin="4RT/CLK" pad="4"/>
<connect gate="G$1" pin="5INTRRT" pad="5"/>
<connect gate="G$1" pin="6SS/TR" pad="6"/>
<connect gate="G$1" pin="7INTSS" pad="7"/>
<connect gate="G$1" pin="8VOUT" pad="8"/>
<connect gate="G$1" pin="9VOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171040302.pdf"/>
<attribute name="I-OUTPUT" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171040302 "/>
<attribute name="V-INPUT" value="2.95-6V"/>
<attribute name="V-OUTPUT" value="0.8-3.6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGI³C-VDRM_BQFN_171021501" prefix="U" uservalue="yes">
<description>&lt;b&gt;MagI³C-VDRM Variable Step Down Regulator Module&lt;/b&gt;&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
 Low conducted and radiated EMI (compliant to EN55022 class B / CISPR-22)
&lt;br&gt;
&lt;br&gt;&lt;b&gt;TO263-7EP&lt;/b&gt;&lt;br&gt;
Leaded package for easy manufacturing and prototyping
&lt;br&gt;Simple layout
&lt;br&gt;Wide input voltage range for input transient capability
&lt;br&gt;Support ambient temperatures up to + 105 °C
&lt;br&gt;2 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;QFN&lt;/b&gt;&lt;br&gt;
Low profile package
&lt;br&gt;Simple application circuit (only 4 external components required)
&lt;br&gt;Optional multiple features (adj.frequency, adj.softstart, power good, sequencing, tracking, synchronization to external clock, adjustable undervoltage lockout)
&lt;br&gt;Wide input voltage range QFN41 type
&lt;br&gt;3 solder cycles supported
&lt;br&gt;
&lt;br&gt;&lt;b&gt;LGA-16EP&lt;/b&gt;&lt;br&gt;
Low profile LGA-package
&lt;br&gt;Stand alone solution (CIN and COUT integrated, 2 external components to set VOUT)
&lt;br&gt;Ideal for space constrained applications
&lt;br&gt;2 solder cycles supported
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;

&lt;br&gt;Point-of-Load DC-DC applications from 24V, 18V, 15V, 12V, 9V, 5V industrial rails
&lt;br&gt;Industrial, Test &amp; Measurement, Medical applications
&lt;br&gt;System power supplies
&lt;br&gt;I/O interface power supply
&lt;br&gt;DSPs, FPGAs, MCUs and MPUs supply
&lt;br&gt;High density distributed power systems
&lt;br&gt;Telecommunication applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o33388v209%20MagIC_VDRM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pm/MAGIC-VDRM"&gt;https://katalog.we-online.com/en/pm/MAGIC-VDRM&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-09-19&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="MAGI³C-VDRM_BQFN_171021501"/>
</gates>
<devices>
<device name="" package="MAGI³C-VDRM_BQFN_171021501">
<connects>
<connect gate="G$1" pin="10VOUT" pad="10"/>
<connect gate="G$1" pin="11VOUT" pad="11"/>
<connect gate="G$1" pin="12VOUT" pad="12"/>
<connect gate="G$1" pin="13VOUT" pad="13"/>
<connect gate="G$1" pin="14VOUT" pad="14"/>
<connect gate="G$1" pin="15VOUT" pad="15"/>
<connect gate="G$1" pin="16PGND" pad="16"/>
<connect gate="G$1" pin="17PGND" pad="17"/>
<connect gate="G$1" pin="18PGND" pad="18"/>
<connect gate="G$1" pin="19PGND" pad="19"/>
<connect gate="G$1" pin="1RSETINT" pad="1"/>
<connect gate="G$1" pin="20PGND" pad="20"/>
<connect gate="G$1" pin="21SW" pad="21"/>
<connect gate="G$1" pin="22SW" pad="22"/>
<connect gate="G$1" pin="23SW" pad="23"/>
<connect gate="G$1" pin="24SW" pad="24"/>
<connect gate="G$1" pin="25BOOT" pad="25"/>
<connect gate="G$1" pin="26VIN" pad="26"/>
<connect gate="G$1" pin="27EN/UVLO" pad="27"/>
<connect gate="G$1" pin="28SS/TRK" pad="28"/>
<connect gate="G$1" pin="29INTSS" pad="29"/>
<connect gate="G$1" pin="2COMP" pad="2"/>
<connect gate="G$1" pin="30INTRRT" pad="30"/>
<connect gate="G$1" pin="31RT/CLK" pad="31"/>
<connect gate="G$1" pin="32AGND" pad="32"/>
<connect gate="G$1" pin="33AGND" pad="33"/>
<connect gate="G$1" pin="34AGND" pad="34"/>
<connect gate="G$1" pin="35PG" pad="35"/>
<connect gate="G$1" pin="36FB" pad="36"/>
<connect gate="G$1" pin="37AGND" pad="37"/>
<connect gate="G$1" pin="38SW" pad="38"/>
<connect gate="G$1" pin="39VOUT" pad="39"/>
<connect gate="G$1" pin="3RCCOMP" pad="3"/>
<connect gate="G$1" pin="40PGND" pad="40"/>
<connect gate="G$1" pin="41SW" pad="41"/>
<connect gate="G$1" pin="4AGND" pad="4"/>
<connect gate="G$1" pin="5AGND" pad="5"/>
<connect gate="G$1" pin="6SW" pad="6"/>
<connect gate="G$1" pin="7SW" pad="7"/>
<connect gate="G$1" pin="8NC" pad="8"/>
<connect gate="G$1" pin="9NC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/pm/datasheet/171021501.pdf"/>
<attribute name="I-OUTPUT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 171021501 "/>
<attribute name="V-INPUT" value="7-50V"/>
<attribute name="V-OUTPUT" value="2.5-15V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
