<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Aluminum Electrolytic Capacitors - WCAP-ASLI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-12-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-ASLL_10X10.5(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,10X10.5X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLL_6.3X7.7(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X7.7X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLL_5X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,5X5.5X1.4(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLL_4X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,4X5.5X1(DiameterXLengthXPitch)</description>
</package>
<package name="WCAP-ASLL_8X10.5(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,8X10.5X3.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLL_12.5X14(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,12.5X14X4.5(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLL_6.3X5.5(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,6.3X5.5X2.1(DiameterXLengthXP)</description>
</package>
<package name="WCAP-ASLL_16X17(DXL)">
<description>&lt;B&gt;WCAP-ASLL&lt;/B&gt;&lt;BR&gt; Aluminium Electrolytic Capacitors,16X17X6.6(DiameterXLengthXP)</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-ASLL_12.5X14" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_12.5X14(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060162012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060162012?ae"/>
<attribute name="DF" value="26%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="207.9uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060162012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140332M6R3DVCTGE000"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060262011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060262011?ae"/>
<attribute name="DF" value="21%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="220uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060262011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140222M010DVCTGE000"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060362011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060362011?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="240uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060362011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140152M016DVCTGE000"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060462010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060462010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="250uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060462010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140102M025DVCTGE000"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060562009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060562009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="164.5uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060562009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140471M035DVCTGE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060562010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060562010?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="238uA"/>
<attribute name="I-RIPPLE" value="1150mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060562010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140681M035DVCTGE000"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060762008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060762008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="800mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060762008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140151M063DVCTGE000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="180mohm"/>
</technology>
<technology name="_865060762009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060762009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="138.6uA"/>
<attribute name="I-RIPPLE" value="830mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060762009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140221M063DVCTGE000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="160mohm"/>
</technology>
<technology name="_865060862006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060862006?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060862006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEH140680M100DVCTGE000"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="100V (DC)"/>
<attribute name="Z" value="700mohm"/>
</technology>
<technology name="_865061462002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865061462002?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="121.15uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865061462002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDH1404R7M450DVCTGE000"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="450V (DC)"/>
<attribute name="Z" value="6600mohm"/>
</technology>
<technology name="_865061462003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865061462003?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="130.6uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865061462003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDH1406R8M450DVCTGE000"/>
<attribute name="VALUE" value="6.8 µF"/>
<attribute name="VR" value="450V (DC)"/>
<attribute name="Z" value="5600mohm"/>
</technology>
<technology name="_865061462004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865061462004?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="12.5mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="145uA"/>
<attribute name="I-RIPPLE" value="70mA"/>
<attribute name="L" value="14mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865061462004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDH140100M450DVCTGE000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="450V (DC)"/>
<attribute name="Z" value="5000mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_8X10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_8X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060153007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060153007?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060153007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M6R3DVCTEE000"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060153008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060153008?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060153008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105471M6R3DVCTEE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060153009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060153009?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060153009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105681M6R3DVCTEE000"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060153010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060153010?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060153010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105102M6R3DVCTEE000"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060253007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060253007?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060253007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M010DVCTEE000"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060253008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060253008?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060253008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105471M010DVCTEE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060353008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060353008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060353008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M016DVCTEE000"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060353009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060353009?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060353009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105471M016DVCTEE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060453006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060453006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="37.5uA"/>
<attribute name="I-RIPPLE" value="500mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060453006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105151M025DVCTEE000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060453007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060453007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060453007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105221M025DVCTEE000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060453008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060453008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060453008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105331M025DVCTEE000"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060553006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060553006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="35uA"/>
<attribute name="I-RIPPLE" value="450mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060553006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105101M035DVCTEE000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060553007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060553007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="52.5uA"/>
<attribute name="I-RIPPLE" value="550mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060553007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105151M035DVCTEE000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060553014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060553014?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="590mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value=""/>
<attribute name="PART-NUMBER" value=" 865060553014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105221M035DVCTEE000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="170mohm"/>
</technology>
<technology name="_865060653009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060653009?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060653009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105680M050DVCTEE000"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="340mohm"/>
</technology>
<technology name="_865060653010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060653010?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="350mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060653010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105101M050DVCTEE000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="340mohm"/>
</technology>
<technology name="_865060753004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060753004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="20.79uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060753004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105330M063DVCTEE000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="700mohm"/>
</technology>
<technology name="_865060753005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060753005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="29.61uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060753005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105470M063DVCTEE000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="650mohm"/>
</technology>
<technology name="_865060853003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060853003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="130mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060853003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEE105220M100DVCTEE000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="100V (DC)"/>
<attribute name="Z" value="1900mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_10X10.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_10X10.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060157011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060157011?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="94.5uA"/>
<attribute name="I-RIPPLE" value="690mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060157011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105152M6R3DVCTEE000"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="90mohm"/>
</technology>
<technology name="_865060257009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060257009?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="68uA"/>
<attribute name="I-RIPPLE" value="690mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060257009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105681M010DVCTEE000"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="90mohm"/>
</technology>
<technology name="_865060257010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060257010?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="100uA"/>
<attribute name="I-RIPPLE" value="690mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060257010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105102M010DVCTEE000"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="90mohm"/>
</technology>
<technology name="_865060357010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060357010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="108.8uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060357010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105681M016DVCTEE000"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="90mohm"/>
</technology>
<technology name="_865060457009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060457009?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="670mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060457009 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105471M025DVCTEE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="90mohm"/>
</technology>
<technology name="_865060557008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060557008?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="77uA"/>
<attribute name="I-RIPPLE" value="670mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060557008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105221M035DVCTEE000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="90mohm"/>
</technology>
<technology name="_865060657011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060657011?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="75uA"/>
<attribute name="I-RIPPLE" value="555mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060657011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105151M050DVCTEE000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="250mohm"/>
</technology>
<technology name="_865060657012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060657012?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="110uA"/>
<attribute name="I-RIPPLE" value="600mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060657012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105221M050DVCTEE000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="230mohm"/>
</technology>
<technology name="_865060757006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060757006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="42.84uA"/>
<attribute name="I-RIPPLE" value="400mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060757006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105680M063DVCTEE000"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="380mohm"/>
</technology>
<technology name="_865060757007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060757007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="63uA"/>
<attribute name="I-RIPPLE" value="420mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060757007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105101M063DVCTEE000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="240mohm"/>
</technology>
<technology name="_865060857004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060857004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="200mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060857004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105330M100DVCTEE000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="100V (DC)"/>
<attribute name="Z" value="1250mohm"/>
</technology>
<technology name="_865060857005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060857005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="47uA"/>
<attribute name="I-RIPPLE" value="390mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060857005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEF105470M100DVCTEE000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="100V (DC)"/>
<attribute name="Z" value="950mohm"/>
</technology>
<technology name="_865061457001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865061457001?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="114.85uA"/>
<attribute name="I-RIPPLE" value="40mA"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865061457001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDF1053R3M450DVCTEE000"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="450V (DC)"/>
<attribute name="Z" value="7200mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_4X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_4X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060140001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060140001?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060140001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055220M6R3DVCTAB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="1500mohm"/>
</technology>
<technology name="_865060140002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060140002?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060140002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055330M6R3DVCTAB000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="1350mohm"/>
</technology>
<technology name="_865060240001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060240001?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060240001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055220M010DVCTAB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="1350mohm"/>
</technology>
<technology name="_865060340001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060340001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060340001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055100M016DVCTAB000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="1350mohm"/>
</technology>
<technology name="_865060440001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060440001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060440001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055100M025DVCTAB000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="2100mohm"/>
</technology>
<technology name="_865060540001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060540001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="90mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060540001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0554R7M035DVCTAB000"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="1900mohm"/>
</technology>
<technology name="_865060640001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060640001?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060640001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB055010M050DVCTAB000"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="4400mohm"/>
</technology>
<technology name="_865060640002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060640002?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060640002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0552R2M050DVCTAB000"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="3900mohm"/>
</technology>
<technology name="_865060640003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060640003?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="4mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="60mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060640003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEB0553R3M050DVCTAB000"/>
<attribute name="VALUE" value="3.3 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="3900mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_6.3X7.7" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_6.3X7.7(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060145006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060145006?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060145006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077221M6R3DVCTCB000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865060245006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060245006?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060245006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077221M010DVCTCB000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865060345006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060345006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060345006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077151M016DVCTCB000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865060345007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060345007?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="280mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060345007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077221M016DVCTCB000"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865060445005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060445005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="300mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060445005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077101M025DVCTCB000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="360mohm"/>
</technology>
<technology name="_865060645007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060645007?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="185mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060645007 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077330M050DVCTCB000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="680mohm"/>
</technology>
<technology name="_865060645008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060645008?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="23.5uA"/>
<attribute name="I-RIPPLE" value="185mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060645008 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077470M050DVCTCB000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="680mohm"/>
</technology>
<technology name="_865060745003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060745003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="13.86uA"/>
<attribute name="I-RIPPLE" value="120mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060745003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077220M063DVCTCB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="1000mohm"/>
</technology>
<technology name="_865060845002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060845002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060845002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077100M100DVCTCB000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="100V (DC)"/>
<attribute name="Z" value="3900mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_6.3X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_6.3X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060143004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060143004?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060143004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055101M6R3DVCTBB000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060143005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060143005?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="9.45uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060143005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055151M6R3DVCTBB000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060243003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060243003?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="4.7uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060243003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055470M010DVCTBB000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060243004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060243004?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060243004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055101M010DVCTBB000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="500mohm"/>
</technology>
<technology name="_865060243005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060243005?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="15uA"/>
<attribute name="I-RIPPLE" value="250mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060243005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055151M010DVCTBB000"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060343003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060343003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5.28uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060343003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055330M016DVCTBB000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060343004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060343004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="7.52uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060343004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055470M016DVCTBB000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060343005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060343005?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="255mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060343005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055101M016DVCTBB000"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060443003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060443003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="8.25uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060443003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055330M025DVCTBB000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060443004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060443004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11.75uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060443004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055470M025DVCTBB000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060543003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060543003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="7.7uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060543003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055220M035DVCTBB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060543004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060543004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11.55uA"/>
<attribute name="I-RIPPLE" value="230mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060543004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055330M035DVCTBB000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060543005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060543005?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="16.45uA"/>
<attribute name="I-RIPPLE" value="240mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060543005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055470M035DVCTBB000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="440mohm"/>
</technology>
<technology name="_865060643005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060643005?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="165mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060643005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055100M050DVCTBB000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="1400mohm"/>
</technology>
<technology name="_865060643006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060643006?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="165mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060643006 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055220M050DVCTBB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="1200mohm"/>
</technology>
<technology name="_865060743002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060743002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="80mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060743002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED055100M063DVCTBB000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="1500mohm"/>
</technology>
<technology name="_865060845002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/865060845002.pdf"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="ENDURANCE" value=""/>
<attribute name="I-LEAK" value="10uA"/>
<attribute name="I-RIPPLE" value="65mA"/>
<attribute name="L" value="7.7mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060845002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASED077100M100DVCTCB000"/>
<attribute name="VALUE" value="10  µF "/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="Z" value="3.9Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_5X5.5" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_5X5.5(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060142003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060142003?ae"/>
<attribute name="DF" value="22%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060142003 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055470M6R3DVCTBB000"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="800mohm"/>
</technology>
<technology name="_865060242002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060242002?ae"/>
<attribute name="DF" value="19%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.3uA"/>
<attribute name="I-RIPPLE" value="160mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060242002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055330M010DVCTBB000"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="800mohm"/>
</technology>
<technology name="_865060342002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060342002?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.52uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060342002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055220M016DVCTBB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="800mohm"/>
</technology>
<technology name="_865060442002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060442002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="5.5uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060442002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055220M025DVCTBB000"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="800mohm"/>
</technology>
<technology name="_865060542002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060542002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3.5uA"/>
<attribute name="I-RIPPLE" value="150mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060542002 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC055100M035DVCTBB000"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="800mohm"/>
</technology>
<technology name="_865060642004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060642004?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="85mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060642004 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC0554R7M050DVCTBB000"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="1520mohm"/>
</technology>
<technology name="_865060742001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060742001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="ENDURANCE" value="2000h"/>
<attribute name="I-LEAK" value="3uA"/>
<attribute name="I-RIPPLE" value="50mA"/>
<attribute name="L" value="5.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060742001 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEC0554R7M063DVCTBB000"/>
<attribute name="VALUE" value="4.7 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="3000mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-ASLL_16X17" prefix="C">
<description>&lt;b&gt;WCAP-ASLL Aluminium Electrolytic Capacitors  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Low Impedance &amp; Long Life +105 °C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Low impedance and long life product series 
&lt;BR&gt;Mounting style: V-Chip SMT 
&lt;BR&gt;Capacitance range: 1 µF ‒ 6800 µF 
&lt;BR&gt;Capacitance tolerance: ±20 % 
&lt;BR&gt;Voltage range (UR): 6.3 ‒ 450 V(DC) 
&lt;BR&gt;Operating temperature: 
&lt;BR&gt;-55 °C up to +105 °C for UR ≤ 100 V(DC) 
&lt;BR&gt;-40 °C up to +105 °C for UR &gt; 100 V(DC) 
&lt;BR&gt;Endurance: 2000 ‒ 5000 h @ +105 °C 
&lt;BR&gt;Dimensions (DxL) in mm: 4.0 x 5.5 up to 16.0 x 17.0 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Long life application &amp; low impedance 
&lt;BR&gt;Input and output capacitor for switched-mode power supply 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. DC/DC converter, AC/DC converter, satellite receiver, control panel 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14724v209%20family-wcap-asll-5x5.5x1.4.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-ASLL/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WCAP-ASLL&lt;/a&gt;&lt;p&gt;

Updated by Ella 2022-12-06&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-ASLL_16X17(DXL)">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_865060163013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060163013?ae"/>
<attribute name="DF" value="32%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="428.4uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060163013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170682M6R3DVCTHE000"/>
<attribute name="VALUE" value="6800 µF"/>
<attribute name="VR" value="6.3V (DC)"/>
<attribute name="Z" value="35mohm"/>
</technology>
<technology name="_865060263012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060263012?ae"/>
<attribute name="DF" value="25%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="470uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060263012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170472M010DVCTHE000"/>
<attribute name="VALUE" value="4700 µF"/>
<attribute name="VR" value="10V (DC)"/>
<attribute name="Z" value="35mohm"/>
</technology>
<technology name="_865060363012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060363012?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="528uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060363012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170332M016DVCTHE000"/>
<attribute name="VALUE" value="3300 µF"/>
<attribute name="VR" value="16V (DC)"/>
<attribute name="Z" value="35mohm"/>
</technology>
<technology name="_865060463011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060463011?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="550uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060463011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170222M025DVCTHE000"/>
<attribute name="VALUE" value="2200 µF"/>
<attribute name="VR" value="25V (DC)"/>
<attribute name="Z" value="35mohm"/>
</technology>
<technology name="_865060563011">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060563011?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="350uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060563011 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170102M035DVCTHE000"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060563012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060563012?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="525uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060563012 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170152M035DVCTHE000"/>
<attribute name="VALUE" value="1500 µF"/>
<attribute name="VR" value="35V (DC)"/>
<attribute name="Z" value="66mohm"/>
</technology>
<technology name="_865060663013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060663013?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="235uA"/>
<attribute name="I-RIPPLE" value="1610mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060663013 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170471M050DVCTHE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="73mohm"/>
</technology>
<technology name="_865060663014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060663014?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="340uA"/>
<attribute name="I-RIPPLE" value="1610mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060663014 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170681M050DVCTHE000"/>
<attribute name="VALUE" value="680 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="73mohm"/>
</technology>
<technology name="_865060663015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060663015?ae"/>
<attribute name="DF" value="12%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="500uA"/>
<attribute name="I-RIPPLE" value="1610mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060663015 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170102M050DVCTHE000"/>
<attribute name="VALUE" value="1000 µF"/>
<attribute name="VR" value="50V (DC)"/>
<attribute name="Z" value="73mohm"/>
</technology>
<technology name="_865060763010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865060763010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="296.1uA"/>
<attribute name="I-RIPPLE" value="1410mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865060763010 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASEK170471M063DVCTHE000"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="63V (DC)"/>
<attribute name="Z" value="82mohm"/>
</technology>
<technology name="_865061463005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/865061463005?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="DIAMETER" value="16mm"/>
<attribute name="ENDURANCE" value="5000h"/>
<attribute name="I-LEAK" value="167.5uA"/>
<attribute name="I-RIPPLE" value="100mA"/>
<attribute name="L" value="17mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value=" 865061463005 "/>
<attribute name="TECHNICAL-REFERENCE" value="ASDK170150M450DVCTHE000"/>
<attribute name="VALUE" value="15 µF"/>
<attribute name="VR" value="450V (DC)"/>
<attribute name="Z" value="3500mohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
