<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - MLCCs-Multilayer Ceramic Chip Capacitors - WCAP-CSGP&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024d, 2024-10-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-CSGP_0805_H0.8_W">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805&lt;/b&gt;&lt;br&gt;Solder type: Wave,2 x 1.25x0.8( LxWxH) ;</description>
</package>
<package name="WCAP-CSGP_0805_H0.8_R">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805&lt;/b&gt;&lt;br&gt;Solder type: Reflow,2 x 1.25x0.8( LxWxH) ;</description>
</package>
<package name="WCAP-CSGP_0603_FI0.35_R">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0603&lt;/b&gt;&lt;br&gt;Solder type: Reflow, 1.6 x 0.8 (LxW)</description>
</package>
<package name="WCAP-CSGP_2220_H2.5">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812&lt;/b&gt;&lt;br&gt;4.5X3.2X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSGP_0603_FI0.35_W">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0603&lt;/b&gt;&lt;br&gt;Solder type: Wave, 1.6 x 0.8 (LxW)</description>
</package>
<package name="WCAP-CSGP_1206_H0.8">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206&lt;/b&gt;&lt;br&gt;3.2X1.6X0.8(LXWXH) ;</description>
</package>
<package name="WCAP-CSGP_1206_H1.15">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206&lt;/b&gt;&lt;br&gt;3.2X1.6X1.15(LXWXH) ;</description>
</package>
<package name="WCAP-CSGP_1210_H1.25">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210&lt;/b&gt;&lt;br&gt;3.2x2.5x1.25(LXWXH);</description>
</package>
<package name="WCAP-CSGP_0805_H0.6_W">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805&lt;/b&gt;&lt;br&gt;Solder type: Wave,2 x 1.25x0.6( LxWxH) ;</description>
</package>
<package name="WCAP-CSGP_1210_H1.6">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210&lt;/b&gt;&lt;br&gt;3.2x2.5x1.6(LXWXH);</description>
</package>
<package name="WCAP-CSGP_0805_H0.6_R">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805&lt;/b&gt;&lt;br&gt;Solder type: Reflow,2 x 1.25x0.6( LxWxH) ;</description>
</package>
<package name="WCAP-CSGP_1210_H2.0">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210&lt;/b&gt;&lt;br&gt;3.2x2.5x2.0LXWXH);</description>
</package>
<package name="WCAP-CSGP_0201">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0201
&lt;/B&gt;&lt;BR&gt;0.6X0.3X0.3(LXWXH)</description>
</package>
<package name="WCAP-CSGP_1206_H1.6">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206&lt;/b&gt;&lt;br&gt;3.2X1.6X1.6(LXWXH) ;</description>
</package>
<package name="WCAP-CSGP_0603_R">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0603&lt;/b&gt;&lt;br&gt;Solder type: Reflow, 1.6 x 0.8 (LxW)</description>
</package>
<package name="WCAP-CSGP_0603_W">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0603&lt;/b&gt;&lt;br&gt;Solder type: Wave, 1.6 x 0.8 (LxW)</description>
</package>
<package name="WCAP-CSGP_1206_H0.95">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206&lt;/b&gt;&lt;br&gt;3.2X1.6X0.95(LXWXH) ;</description>
</package>
<package name="WCAP-CSGP_2220_H2.8">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812&lt;/b&gt;&lt;br&gt;4.5X3.2X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSGP_2220_H2.0">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812&lt;/b&gt;&lt;br&gt;4.5X3.2X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSGP_1812_H2.0">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812&lt;/b&gt;&lt;br&gt;4.5X3.2X2.0(LXWXH)</description>
</package>
<package name="WCAP-CSGP_1210_H0.95">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210&lt;/b&gt;&lt;br&gt;3.2x2.5x0.95(LXWXH);</description>
</package>
<package name="WCAP-CSGP_1812_H1.25">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812&lt;/b&gt;&lt;br&gt;4.5X3.2X1.25(LXWXH)</description>
</package>
<package name="WCAP-CSGP_1206_H1.25">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206&lt;/b&gt;&lt;br&gt;3.2X1.6X1.25(LXWXH) ;</description>
</package>
<package name="WCAP-CSGP_0805_H1.25_R">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805&lt;/b&gt;&lt;br&gt;Solder type: Reflow,2 x 1.25x1.25( LxWxH) ;</description>
</package>
<package name="WCAP-CSGP_1210_H2.5">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210&lt;/b&gt;&lt;br&gt;3.2x2.5x2.5(LXWXH);</description>
</package>
<package name="WCAP-CSGP_1812_H2.5">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812&lt;/b&gt;&lt;br&gt;4.5X3.2X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSGP_0402">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0402
&lt;/B&gt;&lt;BR&gt;1X0.5X0.5(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-CSGP_0805_H0.8" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2022-02-15
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_10V(DC)_R" package="WCAP-CSGP_0805_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007007 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207007?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207016?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)_R" package="WCAP-CSGP_0805_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007020 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007021 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007022 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007023 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207027?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207028?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207029?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207030?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207032?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207033?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207034?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207035?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207036?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207037?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207038?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207039?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207040?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207041?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207042?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207043?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207044?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207045?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)_R" package="WCAP-CSGP_0805_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007038">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007038?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007038 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007039">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007039?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007039 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007040">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007040?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007040 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007041">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007041?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007041 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007042">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007042?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007042 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207054">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207054?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207054 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207055">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207055?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207055 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207056">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207056?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207056 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207057">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207057?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207057 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207058">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207058?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207058 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207059">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207059?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207059 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207060">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207060?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207060 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207061">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207061?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207061 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207062">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207062?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207062 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207063">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207063?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207063 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207064">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207064?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207064 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207065">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207065?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207065 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207066">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207066?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207066 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207067">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207067?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207067 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207068">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207068?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207068 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207069">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207069?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207069 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207070">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207070?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207070 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207071">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207071?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207071 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207072">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207072?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207072 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_R" package="WCAP-CSGP_0805_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007061">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007061?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007061 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007062">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007062?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007062 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007063">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007063?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007063 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007064">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007064?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007064 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007065">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007065?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007065 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207080">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207080?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207080 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207081">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207081?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207081 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207082">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207082?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207082 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207083">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207083?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207083 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207084">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207084?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207084 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207085">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207085?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207085 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207086">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207086?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207086 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207087">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207087?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207087 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207088">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207088?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207088 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207089">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207089?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207089 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207090">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207090?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207090 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207091">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207091?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207091 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207092">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207092?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207092 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207093">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207093?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207093 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207094">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207094?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207094 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207095">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207095?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207095 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207096">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207096?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207096 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207097">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207097?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207097 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207098">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207098?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207098 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207098R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207098R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012207098R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)_R" package="WCAP-CSGP_0805_H0.8_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007086">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007086?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007086 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007087">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007087?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007087 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007088">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007088?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007088 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007089">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007089?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007089 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207110">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207110?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207110 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207111">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207111 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207113">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207113?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207113 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207114">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207114?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207114 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207115">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207115?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207115 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207116">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207116?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207116 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207117">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207117?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207117 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207119">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207119?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207119 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207120">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207120?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207120 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207121">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207121?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207121 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207122">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207122?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207122 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207123">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207123?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207123 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="6.7GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207124">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207124?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207124 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)_W" package="WCAP-CSGP_0805_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007007 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207007?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207016?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)_W" package="WCAP-CSGP_0805_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007020 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007021 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007022 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007023 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207027?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207028?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207029?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207030?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207032?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207033?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207034?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207035?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207036?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207037?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207038?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207039?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207040?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207041?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207042?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207043?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207044?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207045?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)_W" package="WCAP-CSGP_0805_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007038">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007038?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007038 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007039">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007039?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007039 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007040">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007040?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007040 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007041">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007041?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007041 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007042">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007042?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007042 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207054">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207054?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207054 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207055">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207055?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207055 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207056">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207056?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207056 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207057">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207057?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207057 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207058">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207058?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207058 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207059">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207059?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207059 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207060">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207060?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207060 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207061">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207061?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207061 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207062">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207062?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207062 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207063">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207063?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207063 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207064">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207064?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207064 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207065">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207065?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207065 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207066">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207066?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207066 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207067">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207067?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207067 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207068">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207068?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207068 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207069">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207069?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207069 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207070">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207070?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207070 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207071">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207071?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207071 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207072">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207072?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207072 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_W" package="WCAP-CSGP_0805_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007061">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007061?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007061 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007062">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007062?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007062 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007063">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007063?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007063 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007064">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007064?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007064 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007065">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007065?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007065 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207080">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207080?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207080 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207081">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207081?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207081 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207082">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207082?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207082 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207083">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207083?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207083 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207084">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207084?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207084 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207085">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207085?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207085 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207086">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207086?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207086 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207087">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207087?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207087 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207088">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207088?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207088 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207089">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207089?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207089 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207090">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207090?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207090 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207091">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207091?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207091 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207092">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207092?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207092 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207093">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207093?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207093 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207094">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207094?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207094 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207095">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207095?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207095 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207096">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207096?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207096 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207097">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207097?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207097 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207098">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207098?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207098 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207098R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207098R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012207098R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)_W" package="WCAP-CSGP_0805_H0.8_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007086">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007086?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007086 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007087">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007087?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007087 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007088">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007088?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007088 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007089">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007089?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007089 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207110">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207110?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207110 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207111">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207111 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207113">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207113?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207113 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207114">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207114?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207114 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207115">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207115?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207115 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207116">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207116?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207116 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207117">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207117?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207117 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207119">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207119?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207119 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207120">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207120?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207120 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207121">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207121?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207121 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207122">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207122?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207122 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207123">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207123?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207123 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="6.7GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207124">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207124?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207124 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="4.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_0603_FI0.35" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0603 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2024-02-05
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_50V(DC)_R" package="WCAP-CSGP_0603_FI0.35_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012206126">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206126?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206126 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_W" package="WCAP-CSGP_0603_FI0.35_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012206126">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206126?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206126 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)_R" package="WCAP-CSGP_0603_FI0.35_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012106032">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106032?ae"/>
<attribute name="DF" value=" 0.2 "/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)_W" package="WCAP-CSGP_0603_FI0.35_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012106032">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106032?ae"/>
<attribute name="DF" value=" 0.2 "/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_2220_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 2220 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2022-08-01
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_100V(DC)" package="WCAP-CSGP_2220_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012214003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012214003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012214003 "/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value=" 2220 "/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1206_H0.8" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;

&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_10V(DC)" package="WCAP-CSGP_1206_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008001 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008002 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008003 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008004 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208007?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1206_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008011 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208020?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208021?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208022?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208023?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208024?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208025?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208026?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208027?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208028?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208029?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208030?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1206_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008018 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008019 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008020 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008021 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008022 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008023 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008024?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008024 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008025">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008025?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008025 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008026">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008026?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008026 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008027">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008027?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008027 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008028">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008028?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008028 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208042?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208043?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208044?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208045?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208046">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208046?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208046 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208047">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208047?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208047 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208048">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208048?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208048 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208049">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208049?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208049 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208050">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208050?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208050 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208051">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208051?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208051 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208052">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208052?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208052 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208053">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208053?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208053 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208054">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208054?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208054 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208055">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208055?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208055 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208056">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208056?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208056 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208057">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208057?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208057 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208058">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208058?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208058 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1206_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008031">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008031?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008031 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008032?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008032 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008033">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008033?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008033 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008034?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008034 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008035">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008035?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008035 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008036">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008036?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008036 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008037?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008037 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008038">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008038?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008038 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008039">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008039?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008039 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008040">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008040?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008040 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008041">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008041?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008041 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008042">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008042?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008042 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008043">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008043?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008043 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008044">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008044?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008044 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008045">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008045?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008045 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008046">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008046?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008046 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008047?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008047 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008048">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008048?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008048 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008049">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008049?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008049 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008050">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008050?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008050 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008051?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008051 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008052">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008052?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008052 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008053">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008053?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008053 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208070">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208070?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208070 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208071">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208071?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208071 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208072">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208072?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208072 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208073">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208073?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208073 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208074">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208074?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208074 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208075">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208075?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208075 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208076">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208076?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208076 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208077">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208077?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208077 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208078">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208078?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208078 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208079">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208079?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208079 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208080">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208080?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208080 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208081">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208081?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208081 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208082">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208082?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208082 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208083">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208083?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208083 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208084">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208084?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208084 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208085">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208085?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208085 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208086">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208086?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208086 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208087">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208087?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208087 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_1206_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008061">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008061?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008061 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008062">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008062?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008062 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008065">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008065?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008065 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008067">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008067?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008067 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008068">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008068?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008068 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008070">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008070?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008070 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008071">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008071?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008071 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008072">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008072?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008072 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008073">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008073?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008073 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008074">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008074?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008074 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008076">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008076?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008076 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208101">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208101?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208101 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208103">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208103?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208103 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208104">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208104?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208104 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208105">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208105?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208105 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208106">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208106?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208106 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208107">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208107?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208107 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208109">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208109?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208109 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208110">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208110?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208110 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208111">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208111 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208112">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208112?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208112 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208113">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208113?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208113 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="6.7GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208115">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208115?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208115 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208116">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208116?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208116 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208117">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208117?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208117 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1210_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2022-02-15
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_10V(DC)" package="WCAP-CSGP_1210_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012009001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/885012009001.pdf"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value=""/>
<attribute name="LENGTH" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009001 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10G Ohm"/>
<attribute name="SIZE" value=""/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value=""/>
</technology>
<technology name="_885012009006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/885012009006.pdf"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value=""/>
<attribute name="LENGTH" value=""/>
<attribute name="MOUNT" value=""/>
<attribute name="OPERATING-TEMPERATURE" value="-55 °C up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10G Ohm"/>
<attribute name="SIZE" value=""/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value=""/>
</technology>
<technology name="_885012209003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209003?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1210_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012009001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009001 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209010?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209011?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1210_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012009006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209023?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209024?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1210_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012009024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009024?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009024 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209044?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209045?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209046">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209046?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209046 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209047">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209047?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209047 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209047R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209047R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012209047R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1206_H1.15" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)" package="WCAP-CSGP_1206_H1.15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012208001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1206_H1.15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012108006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208015?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1206_H1.15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012108013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108013?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208034?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208035?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208036?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208037?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208038?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1206_H1.15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012208062">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208062?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208062 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208063">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208063?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208063 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208064">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208064?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208064 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1210_H1.6" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_25V(DC)" package="WCAP-CSGP_1210_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012209025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209025?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209026?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_0805_H0.6" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2021-02-03
&lt;br&gt;2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_10V(DC)_R" package="WCAP-CSGP_0805_H0.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007001 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007002 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007003 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007004 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007010 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)_R" package="WCAP-CSGP_0805_H0.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007011 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007012 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007017 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007018 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007019 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)_R" package="WCAP-CSGP_0805_H0.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007026">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007026?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007026 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007027">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007027?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007027 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007028">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007028?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007028 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007029">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007029?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007029 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007030?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007030 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007031">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007031?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007031 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007032?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007032 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007033">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007033?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007033 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007034?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007034 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007035">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007035?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007035 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007036">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007036?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007036 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007037?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007037 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_R" package="WCAP-CSGP_0805_H0.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007045">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007045?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007045 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007046">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007046?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007046 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007047?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007047 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007048">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007048?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007048 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007049">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007049?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007049 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007050">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007050?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007050 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007051?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007051 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007052">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007052?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007052 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007053">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007053?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007053 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007054">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007054?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007054 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007055">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007055?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007055 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007056">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007056?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007056 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007057">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007057?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007057 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007058">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007058?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007058 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007059">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007059?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007059 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007060">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007060?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007060 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)_W" package="WCAP-CSGP_0805_H0.6_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007001 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007002 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007003 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007004 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)_W" package="WCAP-CSGP_0805_H0.6_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007011 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007017 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007018 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007019 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)_W" package="WCAP-CSGP_0805_H0.6_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007026">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007026?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007026 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007027">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007027?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007027 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007028">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007028?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007028 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007029">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007029?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007029 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007030?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007030 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007031">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007031?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007031 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007032?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007032 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007033">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007033?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007033 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007034?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007034 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007035">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007035?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007035 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007036">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007036?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007036 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007037?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007037 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_W" package="WCAP-CSGP_0805_H0.6_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007045">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007045?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007045 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007046">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007046?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007046 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007047?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007047 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007048">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007048?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007048 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007049">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007049?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007049 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007050">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007050?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007050 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007051?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007051 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007052">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007052?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007052 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007053">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007053?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007053 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007054">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007054?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007054 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007055">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007055?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007055 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007056">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007056?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007056 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007057">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007057?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007057 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007058">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007058?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007058 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007059">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007059?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007059 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007060">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007060?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007060 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)_R" package="WCAP-CSGP_0805_H0.6_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007076">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007076?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007076 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007077">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007077?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007077 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007079">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007079?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007079 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007080">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007080?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007080 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007081">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007081?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007081 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007082">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007082?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007082 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007083">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007083?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007083 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007085">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007085?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007085 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007094">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007094?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007094 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007095">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007095?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007095 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007096">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007096?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007096 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007097">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007097?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007097 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007098">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007098?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007098 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="8.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007099">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007099?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007099 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007100">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007100?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007100 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007101">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007101?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007101 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)_W" package="WCAP-CSGP_0805_H0.6_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007076">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007076?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007076 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007077">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007077?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007077 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007079">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007079?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007079 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007080">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007080?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007080 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007081">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007081?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007081 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007082">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007082?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007082 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007083">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007083?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007083 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007085">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007085?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007085 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007094">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007094?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007094 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007095">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007095?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007095 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007096">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007096?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007096 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007097">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007097?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007097 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007098">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007098?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007098 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="8.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007099">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007099?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007099 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="0.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007100">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007100?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007100 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007101">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007101?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007101 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1210_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)" package="WCAP-CSGP_1210_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1210_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1210_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209012?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1210_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109012?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209027?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209028?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_1210_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012209069">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209069?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209069 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1206_H1.6" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella 2024-08-09
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)" package="WCAP-CSGP_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012108001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.001GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.60mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008009 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012008010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.60mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208016?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208019?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012108015">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108016">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108016?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108017">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108018">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208039?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208040?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208041?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012108019">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108019?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108020">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108020?ae"/>
<attribute name="DF" value="7%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012108021">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108021?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208065">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208065?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208065 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1.5uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208066">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208066?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208066 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208067">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208067?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208067 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208068">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208068?ae"/>
<attribute name="DF" value="7%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208068 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208069">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208069?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208069 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012108022">
<attribute name="CERAMIC-TYPE" value="X5R Class II "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012108022?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012108022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208091">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208091?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208091 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208092">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208092?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208092 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208093">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208093?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208093 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208094">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208094?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208094 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012208119">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208119?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208119 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208124">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208124?ae"/>
<attribute name="DF" value=" 0.05 "/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208124 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_0201" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0201 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2022-08-01
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)" package="WCAP-CSGP_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012104003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104010?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104011?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012104002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012204005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012204005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012204005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012104001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104007?ae"/>
<attribute name="DF" value="20%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012004001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004001 "/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004003 "/>
<attribute name="QMIN" value="430"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004004 "/>
<attribute name="QMIN" value="600"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004005 "/>
<attribute name="QMIN" value="640"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="12pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004006 "/>
<attribute name="QMIN" value="700"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004007 "/>
<attribute name="QMIN" value="760"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="18pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004008 "/>
<attribute name="QMIN" value="840"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004009 "/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004010 "/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104008?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012104014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012104014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012104014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012204004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012204004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012204004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012204006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012204006?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012204006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012004002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004002 "/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004011 "/>
<attribute name="QMIN" value="600"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004012 "/>
<attribute name="QMIN" value="840"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004013 "/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012004014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012004014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012004014 "/>
<attribute name="QMIN" value="1000"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012204001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012204001?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012204001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012204002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012204002?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012204002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
<technology name="_885012204003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012204003?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LENGTH" value="0.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012204003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0201"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1206_H0.95" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_100V(DC)" package="WCAP-CSGP_1206_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008078">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008078?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008078 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1206_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008007 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1206_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208032?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208033?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1206_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008029">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008029?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008029 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208059">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208059?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208059 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208060">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208060?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208060 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208061">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208061?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208061 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1206_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008054">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008054?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008054 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208088">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208088?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208088 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208089">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208089?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208089 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_2220_H2.8" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 2220 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2022-08-01
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_25V(DC)" package="WCAP-CSGP_2220_H2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012214004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012214004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012214004 "/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value=" 2220 "/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_2220_H2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012214005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012214005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012214005 "/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value=" 2220 "/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_2220_H2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012214001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012214001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012214001 "/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value=" 2220 "/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_885012214006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012214006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012214006 "/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value=" 2220 "/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1812_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_50V(DC)" package="WCAP-CSGP_1812_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012210030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210030?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210031?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.0mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_2220_H2.0" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 2220 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2022-08-01
&lt;br&gt;2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_100V(DC)" package="WCAP-CSGP_2220_H2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012214002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012214002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="LENGTH" value="5.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012214002 "/>
<attribute name="RISO" value="0.03GOhm"/>
<attribute name="SIZE" value=" 2220 "/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_0603" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0603 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2024-10-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)_R" package="WCAP-CSGP_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012106001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106001 "/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106002 "/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106003 "/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106004 "/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106005 "/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012106006"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206001 "/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206002 "/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)_R" package="WCAP-CSGP_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006001 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006002 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006003 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006004 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006007 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006009 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006011 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206003?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206007?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206016?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206017?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206018?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206019?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206020?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206021?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206022?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206023?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206024?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206025?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206026?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206027?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)_R" package="WCAP-CSGP_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006017 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006018 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006019 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006020 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006021 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006022 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006023 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006024?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006024 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006025">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006025?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006025 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006026">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006026?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006026 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006027">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006027?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006027 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006028">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006028?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006028 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006029">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006029?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006029 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106015">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106016">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106016?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106017">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106018">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106029">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106029?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206028?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206029?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206030?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206032?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206033?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206034?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206035?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206036?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206037?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206038?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206039?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206040?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206041?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206042?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206043?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206044?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206045?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206046">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206046?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206046 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206047">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206047?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206047 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206048">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206048?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206048 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206049">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206049?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206049 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206050">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206050?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206050 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206051">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206051?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206051 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206052">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206052?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206052 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)_R" package="WCAP-CSGP_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006030?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006030 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006031">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006031?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006031 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006032?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006032 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006033">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006033?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006033 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006034?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006034 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006035">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006035?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006035 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006036">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006036?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006036 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006037?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006037 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006038">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006038?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006038 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006039">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006039?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006039 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006040">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006040?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006040 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006041">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006041?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006041 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006042">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006042?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006042 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006043">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006043?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006043 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006044">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006044?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006044 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106019">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106019?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106020">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106020?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106021">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106021?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106022">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106022?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106030">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106030?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106031">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206053">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206053?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206053 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206054">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206054?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206054 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206055">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206055?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206055 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206056">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206056?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206056 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206057">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206057?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206057 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206058">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206058?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206058 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206059">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206059?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206059 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206060">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206060?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206060 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206061">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206061?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206061 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206062">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206062?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206062 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206063">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206063?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206063 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206064">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206064?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206064 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206065">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206065?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206065 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206066">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206066?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206066 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206067">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206067?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206067 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206068">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206068?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206068 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206069">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206069?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206069 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206070">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206070?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206070 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206071">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206071?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206071 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206071R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206071R?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206071R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206072">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206072?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206072 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206073">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206073?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206073 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206074">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206074?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206074 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206075">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206075?ae"/>
<attribute name="DF" value="7%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206075 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206075R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206075R?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206075R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206076">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206076?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206076 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_R" package="WCAP-CSGP_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006045">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006045?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006045 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006046">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006046?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006046 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006047?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006047 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006048">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006048?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006048 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006049">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006049?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006049 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006050">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006050?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006050 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006051?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006051 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006052">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006052?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006052 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006053">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006053?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006053 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006054">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006054?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006054 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006055">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006055?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006055 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006056">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006056?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006056 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006057">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006057?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006057 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006058">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006058?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006058 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006059">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006059?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006059 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006060">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006060?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006060 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006061">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006061?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006061 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006062">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006062?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006062 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006063">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006063?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006063 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206077">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206077?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206077 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206078">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206078?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206078 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206079">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206079?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206079 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206080">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206080?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206080 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206081">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206081?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206081 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206082">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206082?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206082 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206083">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206083?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206083 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206083R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206083R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206083R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206084">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206084?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206084 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206085">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206085?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206085 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206086">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206086?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206086 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206087">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206087?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206087 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206088">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206088?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206088 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206089">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206089?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206089 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206089R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206089R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206089R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10000pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206090">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206090?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206090 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206091">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206091?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206091 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206092">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206092?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206092 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206093">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206093?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206093 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206094">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206094?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206094 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206095">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206095?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206095 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206095R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206095R?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206095R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206121">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206121?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206121 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206125">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206125?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206125 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)_R" package="WCAP-CSGP_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006073">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006073?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006073 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006074">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006074?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006074 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006076">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006076?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006076 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006077">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006077?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006077 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006078">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006078?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006078 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006079">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006079?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006079 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006080">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006080?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006080 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006082">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006082?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006082 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006083">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006083?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006083 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006084">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006084?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006084 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006085">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006085?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006085 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006086">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006086?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006086 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006087">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006087?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006087 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006088">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006088?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006088 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006089">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006089?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006089 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006090">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006090?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006090 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006091">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006091?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006091 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006092">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006092?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006092 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="5.6pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006093">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006093?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006093 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="8.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206102">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206102?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206102 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206103">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206103?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206103 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206105">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206105?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206105 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206106">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206106?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206106 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206107">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206107?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206107 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206108">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206108?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206108 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206109">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206109?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206109 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206111">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206111 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206112">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206112?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206112 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206113">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206113?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206113 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206114">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206114?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206114 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206114R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206114R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206114R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206118">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206118?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206118 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206120">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206120?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206120 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_6.3V(DC)_W" package="WCAP-CSGP_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012106001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)_W" package="WCAP-CSGP_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006001 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006002 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006003 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006004 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006007 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006009 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006011 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206003?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206007?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206016?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206017?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206018?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206019?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206020?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206021?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206022?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206023?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206024?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206025?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206026?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206027?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)_W" package="WCAP-CSGP_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006017 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006018 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006019 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006020 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006021 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006022 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006023 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006024?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006024 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006025">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006025?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006025 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006026">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006026?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006026 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006027">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006027?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006027 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006028">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006028?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006028 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006029">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006029?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006029 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106015">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106016">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106016?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106017">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106018">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106029">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106029?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206028?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206029?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206030?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206032?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206033?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206034?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206035?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206036?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206037?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206038?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206039?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206040?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206041?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206042?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206043?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206044?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206045?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206046">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206046?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206046 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206047">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206047?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206047 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206048">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206048?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206048 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206049">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206049?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206049 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206050">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206050?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206050 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206051">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206051?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206051 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206052">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206052?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206052 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)_W" package="WCAP-CSGP_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006030?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006030 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006031">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006031?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006031 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006032?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006032 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006033">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006033?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006033 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006034?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006034 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006035">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006035?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006035 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006036">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006036?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006036 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006037?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006037 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006038">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006038?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006038 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006039">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006039?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006039 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006040">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006040?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006040 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006041">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006041?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006041 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006042">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006042?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006042 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006043">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006043?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006043 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006044">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006044?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006044 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106019">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106019?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106020">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106020?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106021">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106021?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106022">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106022?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106030">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106030?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012106031">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012106031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012106031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206053">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206053?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206053 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206054">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206054?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206054 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206055">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206055?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206055 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206056">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206056?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206056 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206057">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206057?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206057 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206058">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206058?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206058 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206059">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206059?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206059 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206060">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206060?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206060 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206061">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206061?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206061 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206062">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206062?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206062 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206063">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206063?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206063 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206064">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206064?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206064 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206065">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206065?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206065 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206066">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206066?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206066 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206067">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206067?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206067 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206068">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206068?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206068 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206069">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206069?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206069 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206070">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206070?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206070 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206071">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206071?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206071 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206071R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206071R?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206071R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206072">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206072?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206072 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206073">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206073?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206073 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206074">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206074?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206074 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206075">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206075?ae"/>
<attribute name="DF" value="7%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206075 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206075R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206075R?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206075R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206076">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206076?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206076 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)_W" package="WCAP-CSGP_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006045">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006045?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006045 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006046">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006046?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006046 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006047?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006047 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006048">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006048?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006048 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006049">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006049?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006049 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006050">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006050?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006050 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006051?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006051 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006052">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006052?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006052 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006053">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006053?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006053 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006054">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006054?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006054 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006055">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006055?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006055 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006056">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006056?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006056 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006057">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006057?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006057 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006058">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006058?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006058 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006059">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006059?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006059 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006060">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006060?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006060 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006061">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006061?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006061 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006062">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006062?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006062 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006063">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006063?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006063 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206077">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206077?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206077 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206078">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206078?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206078 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206079">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206079?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206079 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206080">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206080?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206080 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206081">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206081?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206081 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206082">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206082?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206082 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206083">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206083?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206083 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206083R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206083R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206083R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206084">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206084?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206084 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206085">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206085?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206085 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206086">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206086?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206086 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206087">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206087?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206087 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206088">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206088?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206088 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206089">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206089?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206089 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206089R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206089R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206089R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10000pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206090">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206090?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206090 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206091">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206091?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206091 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206092">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206092?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206092 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206093">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206093?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206093 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206094">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206094?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206094 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206095">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206095?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206095 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206095R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206095R?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206095R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206121">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206121?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206121 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206125">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206125?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206125 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)_W" package="WCAP-CSGP_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012006073">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006073?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006073 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006074">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006074?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006074 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006076">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006076?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006076 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006077">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006077?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006077 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006078">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006078?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006078 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006079">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006079?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006079 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006080">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006080?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006080 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006082">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006082?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006082 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006083">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006083?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006083 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006084">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006084?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006084 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006085">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006085?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006085 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006086">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006086?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006086 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006087">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006087?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006087 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006088">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006088?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006088 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006089">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006089?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006089 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006090">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006090?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006090 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006091">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006091?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006091 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006092">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006092?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006092 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="5.6pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012006093">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012006093?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012006093 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="8.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206102">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206102?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206102 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206103">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206103?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206103 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206105">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206105?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206105 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206106">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206106?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206106 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206107">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206107?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206107 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206108">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206108?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206108 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206109">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206109?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206109 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206111">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206111?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206111 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206112">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206112?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206112 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206113">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206113?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206113 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206114">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206114?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206114 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206114R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206114R?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012206114R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206118">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206118?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206118 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885012206120">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012206120?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012206120 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1210_H0.95" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_25V(DC)" package="WCAP-CSGP_1210_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012009002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009002 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009003 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009004 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209015?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209016?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209017?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209018?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209019?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209020?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209021?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209022?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1210_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012209001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209001?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209002?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1210_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012209007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209007?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209008?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209009?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1210_H0.95">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012009007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009007 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009009 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009011 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009017 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009018 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009019 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009020 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009021 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009022 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012009023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012009023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012009023 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209029?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209030?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209031?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209032?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209033?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209034?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209035?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209036?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209037?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209038?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209039?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209040?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209041?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209042?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209043?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1812_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_16V(DC)" package="WCAP-CSGP_1812_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012010001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010001 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010002 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210001?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210002?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210003?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210004?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_1812_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012010003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010003 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010004 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210005?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210006?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210007?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210008?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210009?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210010?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210011?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210012?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1812_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012010005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010005 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010006 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010007 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010009 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010011 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012010016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012010016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012010016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210013?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210014?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210015?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210016?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210017?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210018?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210019?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210020?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210021?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210022?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210023?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210024?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210025?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210026?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210027?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210028?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_885012210029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210029?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1206_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1206  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_25V(DC)" package="WCAP-CSGP_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008030?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008030 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008008 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008017 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008055">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008055?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008055 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208090">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208090?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208090 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012008079">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012008079?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012008079 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885012208118">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012208118?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012208118 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_0805_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0805  &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2024-10-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)" package="WCAP-CSGP_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012107001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.03GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107004?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107005?ae"/>
<attribute name="DF" value=" 0.15 "/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012107005"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107006?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107019">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107019?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107027">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107027?ae"/>
<attribute name="DF" value=" 0.125 "/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207002?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207003?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007009 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107008?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.03GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107009?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107010?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207017?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207018?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207019?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207020?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207021?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207022?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207023?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.3GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1.5uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207024?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207025?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207026?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007024?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007024 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007025">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007025?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007025 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107012?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107014?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207046">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207046?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207046 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207047">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207047?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207047 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3.3GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207048">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207048?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207048 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207049">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207049?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207049 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207050">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207050?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207050 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.1GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207051">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207051?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207051 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.7GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207052">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207052?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207052 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207053">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207053?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207053 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007043">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007043?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007043 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007044">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007044?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007044 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107015">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107016">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107016?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107017">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107018">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107019">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107019?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012107027">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012107027?ae"/>
<attribute name="DF" value=" 0.125 "/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012107027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207073">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207073?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207073 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207074">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207074?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207074 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207075">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207075?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207075 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207076">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207076?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207076 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207077">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207077?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207077 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207078">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207078?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207078 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207079">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207079?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207079 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007066">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007066?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007066 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007067">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007067?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007067 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207099">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207099?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207099 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="150nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207100">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207100?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207100 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207101">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207101?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207101 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207102">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207102?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207102 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207103">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207103?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207103 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="-"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207103R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207103R?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012207103R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_0805_H1.25_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012007091">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007091?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007091 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012007092">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012007092?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012007092 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207125">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207125?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207125 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="3GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207126">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207126?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207126 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.1GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207127">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207127?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207127 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1.5GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207128">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207128?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207128 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885012207130">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012207130?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012207130 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1210_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1210 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2024-10-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_25V(DC)" package="WCAP-CSGP_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109014?ae"/>
<attribute name="DF" value=" 0.1 "/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012109014"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109015">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109015?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012109015"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="20uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209074">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209074?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209074 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109006?ae"/>
<attribute name="DF" value=" 0.1 "/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012109006"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109010?ae"/>
<attribute name="DF" value=" 0.1 "/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012109010"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109011?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012209048">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209048?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209048 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012209073">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209073?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209073 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_6.3V(DC)" package="WCAP-CSGP_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012109002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109002?ae"/>
<attribute name="DF" value=" 0.1 "/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012109002"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.005GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.002GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_885012109004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012109004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012109004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.001GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="100uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012209071">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012209071?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012209071 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_0402" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 0402 &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;General Purpose &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Ella Wu 2024-10-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_6.3V(DC)" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012105001">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105001 "/>
<attribute name="RISO" value="1GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105002">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105002 "/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105003">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105003 "/>
<attribute name="RISO" value="0.3GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105004">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105004 "/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105005">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105005 "/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="680nF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105006">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105006?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105006 "/>
<attribute name="RISO" value="0.1GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105007">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105007?ae"/>
<attribute name="DF" value=" 0.2 "/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012105007"/>
<attribute name="RISO" value="0.02GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105008">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105008?ae"/>
<attribute name="DF" value=" 0.2 "/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value="885012105008"/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105020">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105020?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105020 "/>
<attribute name="RISO" value="0.01GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10uF"/>
<attribute name="VR" value="6.3V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
<device name="_10V(DC)" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012005001">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005001?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005001 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005002">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005002?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005002 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005003">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005003?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005003 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005004">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005004?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005004 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005005">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005005?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005005 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005006">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005006?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005006 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005007">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005007?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005007 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005008">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005008?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005008 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005009">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005009?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005009 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005010">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005010?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005010 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005011">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005011?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005011 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005012">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005012?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005012 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005013">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005013?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005013 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005014">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005014?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005014 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005015">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005015?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005015 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005016">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005016?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005016 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005017">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005017?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005017 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005018">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005018?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005018 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105009">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105010">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105011">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="2.3GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105012">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105012?ae"/>
<attribute name="DF" value="15%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105013">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105013?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.05GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205001?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205001 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205002?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205002 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205003?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205003 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205004?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205004 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205005?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205005 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205006?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205006 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205007?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205007 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205008?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205008 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205009?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205009 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205010?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205010 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205011?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205011 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205012?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205012 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205013?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205013 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205015">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205016">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205016?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205017">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205017?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205018">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205018?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="10V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
<device name="_16V(DC)" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012005019">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005019?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005019 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005020">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005020?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005020 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005021">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005021?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005021 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005022">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005022?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005022 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005023">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005023?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005023 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005024">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005024?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005024 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005025">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005025?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005025 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005026">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005026?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005026 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005027">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005027?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005027 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005028">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005028?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005028 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005029">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005029?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005029 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005030">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005030?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005030 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005031">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005031?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005031 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005032">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005032?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005032 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005033">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005033?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005033 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105014">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105014?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105014 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105015">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105015?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105015 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105016">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105016?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105016 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105017">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105017?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105017 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205019">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205019?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205019 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205020">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205020?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205020 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205021">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205021?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205021 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205022">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205022?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205022 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205023">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205023?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205023 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205024">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205024?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205024 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205025">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205025?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205025 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205026">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205026?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205026 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205027">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205027?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205027 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205028">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205028?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205028 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205029">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205029?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205029 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205030">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205030?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205030 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205031">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205031?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205031 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205032?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205033">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205033?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205033 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205034">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205034?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205034 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205035">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205035?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205035 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205036">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205036?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205036 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="7.4GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205037">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205037?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205037 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205037R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205037R?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012205037R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="16V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
<device name="_25V(DC)" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012005034">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005034?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005034 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005035">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005035?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005035 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005036">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005036?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005036 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005037">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005037?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005037 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005038">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005038?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005038 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005039">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005039?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005039 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005040">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005040?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005040 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005041">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005041?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005041 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005042">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005042?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005042 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005043">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005043?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005043 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005044">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005044?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005044 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005045">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005045?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005045 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005046">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005046?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005046 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005047">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005047?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005047 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005048">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005048?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005048 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012105018">
<attribute name="CERAMIC-TYPE" value="X5R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012105018?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +85 °C"/>
<attribute name="PART-NUMBER" value=" 885012105018 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205038">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205038?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205038 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205039">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205039?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205039 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205040">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205040?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205040 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205041">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205041?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205041 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205042">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205042?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205042 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205043">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205043?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205043 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205044">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205044?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205044 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205045">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205045?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205045 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205046">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205046?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205046 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205047">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205047?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205047 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205048">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205048?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205048 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205049">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205049?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205049 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205050">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205050?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205050 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205051">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205051?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205051 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205052">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205052?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205052 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205053">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205053?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205053 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205054">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205054?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205054 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205085">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205085?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205085 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205085R">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205085R?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value="885012205085R"/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="25V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
<device name="_50V(DC)" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012005049">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005049?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005049 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005050">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005050?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005050 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005051">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005051?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005051 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005052">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005052?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005052 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005053">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005053?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005053 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005054">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005054?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005054 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005055">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005055?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005055 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005056">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005056?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005056 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="15pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005057">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005057?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005057 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="22pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005058">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005058?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005058 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005059">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005059?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005059 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005060">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005060?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005060 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005061">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005061?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005061 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005062">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005062?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005062 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005063">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005063?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005063 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005067">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005067?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.25mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005067 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205055">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205055?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205055 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205056">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205056?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205056 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205057">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205057?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205057 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205058">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205058?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205058 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205059">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205059?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205059 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205060">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205060?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205060 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="680pF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205061">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205061?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205061 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205062">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205062?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205062 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1.5nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205063">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205063?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205063 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205064">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205064?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205064 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="3.3nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205065">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205065?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205065 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205066">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205066?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205066 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="6.8nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205067">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205067?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205067 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205086">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205086?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205086 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205092">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205092?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205092 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.5GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
<device name="_100V(DC)" package="WCAP-CSGP_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012005074">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005074?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005074 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="10pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005077">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005077?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005077 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005078">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005078?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005078 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="47pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005079">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005079?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005079 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="68pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005080">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005080?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005080 "/>
<attribute name="QMIN" value=" 1000 "/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005083">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005083?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005083 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="2.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005084">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005084?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005084 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012005085">
<attribute name="CERAMIC-TYPE" value="NP0 Class I"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012005085?ae"/>
<attribute name="DF" value="-"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012005085 "/>
<attribute name="QMIN" value="400+20C"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="8.2pF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205080">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205080?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205080 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="1nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
<technology name="_885012205084">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012205084?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012205084 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="10GOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="4.7nF"/>
<attribute name="VR" value="100V(DC)"/>
<attribute name="WIDTH" value="0.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSGP_1812_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSGP MLCCs 1812 &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;


&lt;B&gt;Characteristics&lt;BR&gt;
&lt;BR&gt;General purpose product series&lt;/B&gt;
&lt;BR&gt; High performance ceramic
&lt;BR&gt; High electrical precision and stability ceramic especially for NP0
&lt;BR&gt; Minimal aging especially for NP0
&lt;BR&gt; Mounting style: SMT-Chip
&lt;BR&gt; Ceramic: NP0 (Class I), X5R (Class II), X7R (Class II)
&lt;BR&gt; Temperature coefficient: 
&lt;BR&gt; ±30 ppm/°C; ±0.54 % for NP0 
&lt;BR&gt; ±15 % for X5R and X7R
&lt;BR&gt; Operating temperature: 
&lt;BR&gt;-55 °C up to + 125 °C for NP0 and X7R 
&lt;BR&gt;-55 °C up to + 85 °C for X5R
&lt;BR&gt; Termination: Cu/Ni/Sn
&lt;BR&gt; Recommended soldering: Reflow soldering
&lt;BR&gt; Wave soldering for size 0603
&lt;BR&gt; Wave soldering for size 0805 (only valid for the thickness ≤0.85 mm)

&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Temperature compensation (NP0)
&lt;BR&gt;Coupling
&lt;BR&gt; Decoupling
&lt;BR&gt; Bypass
&lt;BR&gt; Smoothing
&lt;BR&gt; Filtering
&lt;BR&gt; Resonant circuit

&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o177837v209%20MLCC_GRP_all.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose"&gt;https://www.we-online.com/catalog/en/pbs/capacitors/multilayer_ceramic_chip_capacitors/mlcc_general_purpose&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-09
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_50V(DC)" package="WCAP-CSGP_1812_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885012210032">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885012210032?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885012210032 "/>
<attribute name="QMIN" value="-"/>
<attribute name="RISO" value="0.2GOhm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.2uF"/>
<attribute name="VR" value="50V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
