<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - MLCCs-Multilayer Ceramic Chip Capacitors - WCAP-CSST&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-01-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-CSST_1210_H2.5">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x2.5(LXWXH);</description>
</package>
<package name="WCAP-CSST_0603_R">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,size code LxW:1,6 x 0,8 ;</description>
</package>
<package name="WCAP-CSST_1210_H1.6">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;3.2x2.5x1.6(LXWXH);</description>
</package>
<package name="WCAP-CSST_0805">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Reflow,2 x 1.25x1.25( LxWxH) ;</description>
</package>
<package name="WCAP-CSST_1812_H2.5">
<description>&lt;b&gt;WCAP-CSST Soft Termination
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size: 1812, SMT, 2pins
&lt;br&gt;4.5X3.2X2.5(LXWXH)</description>
</package>
<package name="WCAP-CSST_0603_W">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;Solder type: Wave,size code LxW:1,6 x 0,8 ;</description>
</package>
<package name="WCAP-CSST_1206_H1.6">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;3.2X1.6X1.6(LXWXH) ;</description>
</package>
<package name="WCAP-CSST_1206_H1.25">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/b&gt;&lt;br&gt;3.2X1.6X1.25(LXWXH) ;</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-CSST_1210_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSST_1210_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382209002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382209002?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382209002 "/>
<attribute name="RISO" value="0.05 Gohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="100 V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSST_1210_H1.6" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSST_1210_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382209001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382209001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.75mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382209001 "/>
<attribute name="RISO" value="3 Gohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="500 V(DC)"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSST_0805" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSST_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382207001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207001?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207001 "/>
<attribute name="RISO" value="0.5 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="16 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207002?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207002 "/>
<attribute name="RISO" value="1.5 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="330 nF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207003?ae"/>
<attribute name="DF" value="5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207003 "/>
<attribute name="RISO" value="0.5 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207004?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207004 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207005 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="2.2 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207006 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207007 "/>
<attribute name="RISO" value="5 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207008?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207008 "/>
<attribute name="RISO" value="2.3 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="220 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207009 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="100 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
<technology name="_885382207010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382207010?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382207010 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="VALUE" value="270 pF"/>
<attribute name="VR" value="500 V(DC)"/>
<attribute name="WIDTH" value="1.25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSST_1812_H2.5" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSST_1812_H2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382211002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382211002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.5mm"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382211002 "/>
<attribute name="RISO" value="1 Gohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="1000 V(DC)"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSST_0603" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_R" package="WCAP-CSST_0603_R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382206001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206001 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206002 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206003 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206004?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206004 "/>
<attribute name="RISO" value="5 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206005 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="200 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_W" package="WCAP-CSST_0603_W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382206001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206001?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206001 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="220 pF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206002 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206003 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206004?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206004 "/>
<attribute name="RISO" value="5 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_885382206005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382206005?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.4mm"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382206005 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1 nF"/>
<attribute name="VR" value="200 V(DC)"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSST_1206_H1.6" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSST_1206_H1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382208001">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208001?ae"/>
<attribute name="DF" value="3.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208001 "/>
<attribute name="RISO" value="0.2 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="2.2 µF"/>
<attribute name="VR" value="25 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208004">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208004?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208004 "/>
<attribute name="RISO" value="1 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208005">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208005?ae"/>
<attribute name="DF" value="3%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208005 "/>
<attribute name="RISO" value="0.5 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="1 µF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208007">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208007?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208007 "/>
<attribute name="RISO" value="1 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="250 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208010">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208010?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208010 "/>
<attribute name="RISO" value="4.5 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="22 nF"/>
<attribute name="VR" value="500 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208011">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208011?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208011 "/>
<attribute name="RISO" value="3 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="33 nF"/>
<attribute name="VR" value="500 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-CSST_1206_H1.25" prefix="C">
<description>&lt;b&gt;WCAP-CSST MLCCs &lt;/B&gt;&lt;BR&gt;
&lt;B&gt;Soft Termination  &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Product series with high absorbtion of mechanical stress 
&lt;BR&gt;Mounting style: SMT-Chip 
&lt;BR&gt;Capacitance range: 220 pF - 2.2 µF 
&lt;BR&gt;Temperature Coefficient: ± 15 % 
&lt;BR&gt;Voltage range (UR): 16 V(DC) - 2 kV(DC) 
&lt;BR&gt;Operating temperature: -55 °C up to + 125 °C 
&lt;BR&gt;Sizes: 0603 / 0805 / 1206 / 1210 
&lt;BR&gt;Termination: Ag-Polymer/Ni/Sn 
&lt;BR&gt;Recommended soldering: Reflow soldering 
&lt;BR&gt;Wave soldering (only valid for the thickness ≤0.85 mm) 
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Application with high mechanical stress 
&lt;BR&gt;Power supply 
&lt;BR&gt;Lighting 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o164343v209%20Family_WE-MLCC_1210.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="www.we-online.com/catalog/WCAP-CSST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WCAP-CSST&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-01-18
&lt;br&gt;2024(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="WCAP-CSST_1206_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_885382208002">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208002?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208002 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208003">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208003?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208003 "/>
<attribute name="RISO" value="5 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="50 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208006">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208006?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208006 "/>
<attribute name="RISO" value="1 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="100 nF"/>
<attribute name="VR" value="100 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208008">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208008?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208008 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="270 pF"/>
<attribute name="VR" value="500 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208009">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208009?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208009 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="10 nF"/>
<attribute name="VR" value="500 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208012">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208012?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208012 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="4.7 nF"/>
<attribute name="VR" value="1000 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208013">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208013?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208013 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="470 pF"/>
<attribute name="VR" value="2000 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_885382208014">
<attribute name="CERAMIC-TYPE" value="X7R Class II"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/885382208014?ae"/>
<attribute name="DF" value="2.5%"/>
<attribute name="FI" value="0.6mm"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-55 up to +125 °C"/>
<attribute name="PART-NUMBER" value=" 885382208014 "/>
<attribute name="RISO" value="10 Gohm"/>
<attribute name="SIZE" value="1206"/>
<attribute name="VALUE" value="680 pF"/>
<attribute name="VR" value="2000 V(DC)"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
