<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Capacitors - Film Capacitors - WCAP-FTBP&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-FTBP_27.5X31X10X19(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X10X19(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_27.5X31X15X24.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X15X24.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_27.5X31X13X22(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X13X22(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_22.5X26X6X15(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X6X15(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_22.5X26X8.5X17(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X8.5X17(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_22.5X26X9X18(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X9X18(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_15X18X10X16.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X10X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_27.5X31X16X25.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X16X25.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_27.5X31X18X26(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X18X26(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_27.5X31X14X23.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,27.5X31X14X23.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_15X18X5X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_15X18X6X12(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_15X18X8X14(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X8X14(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_7.5X10.5X6X12(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,7.5X10.5X6X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_22.5X26X7X16.5(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,22.5X26X7X16.5(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_7.5X10.5X5X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,7.5X10.5X5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_15X18X7X13(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,15X18X7X13(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_10X13X5.5X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X5.5X11(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_10X13X6X12(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X6.0X12(PitchXLXWXH)</description>
</package>
<package name="WCAP-FTBP_10X13X5.0X11(PXLXWXH)">
<description>&lt;B&gt;WCAP-FTBP&lt;/B&gt;&lt;BR&gt; Film Capacitors,10X13X5.0X11(PitchXLXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-FTBP_P27.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBP Film Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polypropylene &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Stable frequency and temperature behavior 
&lt;BR&gt;No voltage derating 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 33 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±5 % 
&lt;BR&gt;Voltage range (UR): 160 ‒ 630 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Stable demanding applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P27.5=Pitch 27.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBP/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-10
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W10.0" package="WCAP-FTBP_27.5X31X10X19(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283327004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283327004CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.39%@10kHz"/>
<attribute name="DF3" value="3.3%@100kHz"/>
<attribute name="H" value="19mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283327004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="90V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP275105J400DCPP35004"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_W13.0" package="WCAP-FTBP_27.5X31X13X22(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890443327007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890443327007CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.75%@10kHz"/>
<attribute name="DF3" value="5.9%@100kHz"/>
<attribute name="H" value="22mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890443327007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="46V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP275685J160DCPP35004"/>
<attribute name="VALUE" value="6.8  µF "/>
<attribute name="VR" value="160V(DC)"/>
<attribute name="W" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_W14.0" package="WCAP-FTBP_27.5X31X14X23.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273327007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273327007CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.57%@10kHz"/>
<attribute name="DF3" value="4.6%@100kHz"/>
<attribute name="H" value="23.5mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273327007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="64V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP275475J250DCPP35004"/>
<attribute name="VALUE" value="4.7  µF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="14mm"/>
</technology>
</technologies>
</device>
<device name="_W15.0" package="WCAP-FTBP_27.5X31X15X24.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283327008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283327008CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.4%@10kHz"/>
<attribute name="DF3" value="3.4%@100kHz"/>
<attribute name="H" value="24.5mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283327008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="98V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP275225J400DCPP25004"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_W16.0" package="WCAP-FTBP_27.5X31X16X25.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303327008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303327008CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.34%@10kHz"/>
<attribute name="DF3" value="2.3%@100kHz"/>
<attribute name="H" value="25.5mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303327008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP275155J630DCPP25004"/>
<attribute name="VALUE" value="1.5  µF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="16mm"/>
</technology>
</technologies>
</device>
<device name="_W18.0" package="WCAP-FTBP_27.5X31X18X26(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283327010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283327010CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.4%@10kHz"/>
<attribute name="DF3" value="3.4%@100kHz"/>
<attribute name="H" value="26mm"/>
<attribute name="L" value="31mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283327010CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="100V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP275335J400DCPP25004"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="18mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBP_P22.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBP Film Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polypropylene &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Stable frequency and temperature behavior 
&lt;BR&gt;No voltage derating 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 33 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±5 % 
&lt;BR&gt;Voltage range (UR): 160 ‒ 630 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Stable demanding applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P22.5=Pitch 22.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBP/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-10
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W6.0" package="WCAP-FTBP_22.5X26X6X15(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273326003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273326003CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.36%@10kHz"/>
<attribute name="DF3" value="3.1%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273326003CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="60V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225684J250DCPP45004"/>
<attribute name="VALUE" value="680  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890283326003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283326003CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.3%@10kHz"/>
<attribute name="DF3" value="1.9%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283326003CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="97V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225334J400DCPP45004"/>
<attribute name="VALUE" value="330  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890303326003CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303326003CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.26%@10kHz"/>
<attribute name="DF3" value="1.3%@100kHz"/>
<attribute name="H" value="15mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303326003CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="120V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225154J630DCPP45004"/>
<attribute name="VALUE" value="150  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_W7.0" package="WCAP-FTBP_22.5X26X7X16.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273326007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273326007CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.4%@10kHz"/>
<attribute name="DF3" value="3.4%@100kHz"/>
<attribute name="H" value="16.5mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273326007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="61V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225155J250DCPP35004"/>
<attribute name="VALUE" value="1.5  µF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_W8.5" package="WCAP-FTBP_22.5X26X8.5X17(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283326009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283326009CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.32%@10kHz"/>
<attribute name="DF3" value="2.2%@100kHz"/>
<attribute name="H" value="17mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283326009CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="95V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225105J400DCPP35004"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_W9.0" package="WCAP-FTBP_22.5X26X9X18(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303326009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303326009CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.28%@10kHz"/>
<attribute name="DF3" value="1.5%@100kHz"/>
<attribute name="H" value="18mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303326009CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="130V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225474J630DCPP35004"/>
<attribute name="VALUE" value="470  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="9mm"/>
</technology>
<technology name="_890443326007CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890443326007CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.44%@10kHz"/>
<attribute name="DF3" value="3.9%@100kHz"/>
<attribute name="H" value="18mm"/>
<attribute name="L" value="26mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890443326007CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="57V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP225335J160DCPP35004"/>
<attribute name="VALUE" value="3.3  µF "/>
<attribute name="VR" value="160V(DC)"/>
<attribute name="W" value="9mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBP_P7.5" prefix="C">
<description>&lt;b&gt;WCAP-FTBP Film Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polypropylene &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Stable frequency and temperature behavior 
&lt;BR&gt;No voltage derating 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 33 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±5 % 
&lt;BR&gt;Voltage range (UR): 160 ‒ 630 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Stable demanding applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P7.5=Pitch 7.5&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBP/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-10
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W5.0" package="WCAP-FTBP_7.5X10.5X5X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273322005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273322005CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.26%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273322005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="340V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP075154J250DCPP45004"/>
<attribute name="VALUE" value="150  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890303322005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303322005CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.15%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303322005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="700V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP075333J630DCPP45004"/>
<attribute name="VALUE" value="33  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890443322001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890443322001CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.26%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890443322001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP075104J160DCPP45004"/>
<attribute name="VALUE" value="100nF"/>
<attribute name="VR" value="160V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_W6.0" package="WCAP-FTBP_7.5X10.5X6X12(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283322006CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283322006CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.15%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="10.5mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283322006CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="610V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP075683J400DCPP45004"/>
<attribute name="VALUE" value="68  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBP_P15" prefix="C">
<description>&lt;b&gt;WCAP-FTBP Film Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polypropylene &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Stable frequency and temperature behavior 
&lt;BR&gt;No voltage derating 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 33 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±5 % 
&lt;BR&gt;Voltage range (UR): 160 ‒ 630 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Stable demanding applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P15=Pitch 15&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBP/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-10
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W10.0" package="WCAP-FTBP_15X18X10X16.5(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890443325010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890443325010CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.28%@10kHz"/>
<attribute name="DF3" value="1.6%@100kHz"/>
<attribute name="H" value="16.5mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890443325010CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="98V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015225J160DCPP45004"/>
<attribute name="VALUE" value="2.2  µF "/>
<attribute name="VR" value="160V(DC)"/>
<attribute name="W" value="10mm"/>
</technology>
</technologies>
</device>
<device name="_W5.0" package="WCAP-FTBP_15X18X5X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273325005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273325005CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.28%@10kHz"/>
<attribute name="DF3" value="1.5%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273325005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="59V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015474J250DCPP45004"/>
<attribute name="VALUE" value="470  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
<technology name="_890283325002CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283325002CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.15%@10kHz"/>
<attribute name="DF3" value="0.8%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283325002CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="120V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015104J400DCPP45004"/>
<attribute name="VALUE" value="100  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_W6.0" package="WCAP-FTBP_15X18X6X12(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303325004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303325004CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.15%@10kHz"/>
<attribute name="DF3" value="0.57%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303325004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="240V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015683J630DCPP45004"/>
<attribute name="VALUE" value="68  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_W7.0" package="WCAP-FTBP_15X18X7X13(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273325009CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273325009CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.28%@10kHz"/>
<attribute name="DF3" value="1.5%@100kHz"/>
<attribute name="H" value="13mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273325009CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="85V/us"/>
<attribute name="RISO" value="10000  Ohm x F "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015105J250DCPP45004"/>
<attribute name="VALUE" value="1  µF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="7mm"/>
</technology>
<technology name="_890283325008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283325008CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.15%@10kHz"/>
<attribute name="DF3" value="0.92%@100kHz"/>
<attribute name="H" value="13mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283325008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="140V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015334J400DCPP45004"/>
<attribute name="VALUE" value="330  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="7mm"/>
</technology>
<technology name="_890303325008CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303325008CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.15%@10kHz"/>
<attribute name="DF3" value="0.68%@100kHz"/>
<attribute name="H" value="13mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303325008CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="200V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015154J630DCPP45004"/>
<attribute name="VALUE" value="150  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="7mm"/>
</technology>
</technologies>
</device>
<device name="_W8.0" package="WCAP-FTBP_15X18X8X14(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890303325010CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303325010CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.15%@10kHz"/>
<attribute name="DF3" value="0.68%@100kHz"/>
<attribute name="H" value="14mm"/>
<attribute name="L" value="18mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303325010CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="220V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP015224J630DCPP45004"/>
<attribute name="VALUE" value="220  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-FTBP_P10" prefix="C">
<description>&lt;b&gt;WCAP-FTBP Film Capacitors &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Boxed Type Metallized Polypropylene &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series with max. operating temperature of +105 °C 
&lt;BR&gt;Self-healing properties 
&lt;BR&gt;Stable frequency and temperature behavior 
&lt;BR&gt;No voltage derating 
&lt;BR&gt;Mounting style: Boxed THT 
&lt;BR&gt;Dielectric: Polypropylene 
&lt;BR&gt;Capacitance range: 33 nF ‒ 6.8 µF 
&lt;BR&gt;Capacitance tolerance: ±5 % 
&lt;BR&gt;Voltage range (UR): 160 ‒ 630 V(DC) 
&lt;BR&gt;Operating temperature: -40 °C up to + 105 °C 
&lt;BR&gt;Pitch: 7.5 / 10.0 / 15.0 / 22.5 / 27.5 mm 
&lt;BR&gt;Recommended soldering: Wave soldering  
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Stable demanding applications 
&lt;BR&gt;Filtering 
&lt;BR&gt;Smoothing 
&lt;BR&gt;e.g. Monitor, electrical ballast 
&lt;BR&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;P10=Pitch 10&lt;/B&gt;
&lt;BR&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o85133v209%20Family_WE_WCAP-FTBP_4mm+Original.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/WCAP-FTBP/"&gt;https://www.we-online.com/catalog/en/WCAP-FTBP/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-03-10
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="_W5.0" package="WCAP-FTBP_10X13X5.0X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283323001CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283323001CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.31%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283323001CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="340V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP010473J400DCPP55004"/>
<attribute name="VALUE" value="47  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="5mm"/>
</technology>
</technologies>
</device>
<device name="_W5.5" package="WCAP-FTBP_10X13X5.5X11(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890283323005CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890283323005CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.35%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890283323005CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="300V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP010104J400DCPP55004"/>
<attribute name="VALUE" value="100  nF "/>
<attribute name="VR" value="400V(DC)"/>
<attribute name="W" value="5.5mm"/>
</technology>
<technology name="_890303323004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890303323004CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="10%@10kHz"/>
<attribute name="DF3" value="0.29%@100kHz"/>
<attribute name="H" value="11mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890303323004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="430V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP010473J630DCPP55004"/>
<attribute name="VALUE" value="47  nF "/>
<attribute name="VR" value="630V(DC)"/>
<attribute name="W" value="5.5mm"/>
</technology>
</technologies>
</device>
<device name="_W6.0" package="WCAP-FTBP_10X13X6X12(PXLXWXH)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_890273323004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890273323004CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.1%@10kHz"/>
<attribute name="DF3" value="0.4%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890273323004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="250V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP010224J250DCPP45004"/>
<attribute name="VALUE" value="220  nF "/>
<attribute name="VR" value="250V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
<technology name="_890443323004CS">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/890443323004CS.pdf"/>
<attribute name="DF1" value="0.1%@1kHz"/>
<attribute name="DF2" value="0.15%@10kHz"/>
<attribute name="DF3" value="0.54%@100kHz"/>
<attribute name="H" value="12mm"/>
<attribute name="L" value="13mm"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="PART-NUMBER" value="890443323004CS"/>
<attribute name="RATE-OF-VOLTAGE-RISE" value="180V/us"/>
<attribute name="RISO" value="30000  MOhm "/>
<attribute name="TECHNICAL-REFERENCE" value="MPPP010334J160DCPP45004"/>
<attribute name="VALUE" value="330  nF "/>
<attribute name="VR" value="160V(DC)"/>
<attribute name="W" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
