<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Capacitors - Aluminium Hybrid Polymer Capacitors - WCAP-HSG5&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-04-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WCAP-HSG5_D6.3H7.7P2.2">
<description>&lt;b&gt;WCAP-HSG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch = 6.3mmX7.7mmX2.2mm, SMT, 2pins</description>
</package>
<package name="WCAP-HSG5_D6.3H5.8P2.2">
<description>&lt;b&gt;WCAP-HSG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch = 6.3mmX5.8mmX2.2mm, SMT, 2pins</description>
</package>
<package name="WCAP-HSG5_D10H10.5P4.5">
<description>&lt;b&gt;WCAP-HSG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch = 10mmX10.5mmX4.5mm, SMT, 2pins</description>
</package>
<package name="WCAP-HSG5_D10H12.4P4.5">
<description>&lt;b&gt;WCAP-HSG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch = 10mmX12.4mmX4.5mm, SMT, 2pins</description>
</package>
<package name="WCAP-HSG5_D8H10.5P3.1">
<description>&lt;b&gt;WCAP-HSG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch = 8mmX10.5mmX3.1mm, SMT, 2pins</description>
</package>
<package name="WCAP-HSG5_D5H5.8P1.4">
<description>&lt;b&gt;WCAP-HSG5 Polymer Electrolytic Capacitor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Diameter X Length X Pitch = 5mmX5.8mmX1.4mm, SMT, 2pins</description>
</package>
</packages>
<symbols>
<symbol name="C_POLAR">
<description>C_POLARIZED</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WCAP-HSG5_D10H10.5P4.5" prefix="C">
<description>&lt;b&gt;WCAP-HSG5 General Purpose 105°C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Endurance: 10000h @ +105 °C
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HSG5"&gt;https://www.we-online.com/en/components/products/WCAP-HSG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HSG5_D10H10.5P4.5">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875575357006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575357006?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="52.8uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575357006 "/>
<attribute name="RESR" value="20mohm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875575357008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575357008?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="75.2uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575357008 "/>
<attribute name="RESR" value="20mohm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875575357010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575357010?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="89.6uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575357010 "/>
<attribute name="RESR" value="20mohm"/>
<attribute name="VALUE" value="560 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875575557006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575557006?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="82.5uA"/>
<attribute name="I-RIPPLE" value="2500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575557006 "/>
<attribute name="RESR" value="20mohm"/>
<attribute name="VALUE" value="330 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875575757004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575757004?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="28uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575757004 "/>
<attribute name="RESR" value="28mohm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875575757007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575757007?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="50uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575757007 "/>
<attribute name="RESR" value="28mohm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875575857006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575857006?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="35.3uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575857006 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875575857007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575857007?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="42.8uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575857007 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875575957003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575957003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="22uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575957003 "/>
<attribute name="RESR" value="45mohm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HSG5_D6.3H7.7P2.2" prefix="C">
<description>&lt;b&gt;WCAP-HSG5 General Purpose 105°C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Endurance: 10000h @ +105 °C
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HSG5"&gt;https://www.we-online.com/en/components/products/WCAP-HSG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HSG5_D6.3H7.7P2.2">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875575345004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575345004?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="35.2uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value=" 875575345004 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875575545003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575545003?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="25uA"/>
<attribute name="I-RIPPLE" value="2000mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value=" 875575545003 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875575745003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575745003?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16.5uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value=" 875575745003 "/>
<attribute name="RESR" value="40mohm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875575845002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575845002?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="13.9uA"/>
<attribute name="I-RIPPLE" value="1500mA"/>
<attribute name="LENGTH" value="7.7mm"/>
<attribute name="PART-NUMBER" value=" 875575845002 "/>
<attribute name="RESR" value="80mohm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HSG5_D10H12.4P4.5" prefix="C">
<description>&lt;b&gt;WCAP-HSG5 General Purpose 105°C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Endurance: 10000h @ +105 °C
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HSG5"&gt;https://www.we-online.com/en/components/products/WCAP-HSG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HSG5_D10H12.4P4.5">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875575561007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575561007?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="117.5uA"/>
<attribute name="I-RIPPLE" value="2800mA"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="PART-NUMBER" value=" 875575561007 "/>
<attribute name="RESR" value="16mohm"/>
<attribute name="VALUE" value="470 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875575961005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575961005?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="10mm"/>
<attribute name="I-LEAK" value="33uA"/>
<attribute name="I-RIPPLE" value="1600mA"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="PART-NUMBER" value=" 875575961005 "/>
<attribute name="RESR" value="40mohm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="100V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HSG5_D8H10.5P3.1" prefix="C">
<description>&lt;b&gt;WCAP-HSG5 General Purpose 105°C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Endurance: 10000h @ +105 °C
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HSG5"&gt;https://www.we-online.com/en/components/products/WCAP-HSG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HSG5_D8H10.5P3.1">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875575553004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575553004?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="55uA"/>
<attribute name="I-RIPPLE" value="2300mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575553004 "/>
<attribute name="RESR" value="27mohm"/>
<attribute name="VALUE" value="220 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875575753005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575753005?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="34uA"/>
<attribute name="I-RIPPLE" value="1800mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575753005 "/>
<attribute name="RESR" value="30mohm"/>
<attribute name="VALUE" value="68 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875575853003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575853003?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="20.8uA"/>
<attribute name="I-RIPPLE" value="1700mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575853003 "/>
<attribute name="RESR" value="40mohm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
<technology name="_875575853004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575853004?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="8mm"/>
<attribute name="I-LEAK" value="29.6uA"/>
<attribute name="I-RIPPLE" value="1700mA"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="PART-NUMBER" value=" 875575853004 "/>
<attribute name="RESR" value="40mohm"/>
<attribute name="VALUE" value="47 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HSG5_D6.3H5.8P2.2" prefix="C">
<description>&lt;b&gt;WCAP-HSG5 General Purpose 105°C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Endurance: 10000h @ +105 °C
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HSG5"&gt;https://www.we-online.com/en/components/products/WCAP-HSG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HSG5_D6.3H5.8P2.2">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875575344001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575344001?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="16uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575344001 "/>
<attribute name="RESR" value="50mohm"/>
<attribute name="VALUE" value="100 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875575344003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575344003?ae"/>
<attribute name="DF" value="16%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="24uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575344003 "/>
<attribute name="RESR" value="50mohm"/>
<attribute name="VALUE" value="150 µF"/>
<attribute name="VR" value="16V(DC)"/>
</technology>
<technology name="_875575544002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575544002?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="14uA"/>
<attribute name="I-RIPPLE" value="1300mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575544002 "/>
<attribute name="RESR" value="50mohm"/>
<attribute name="VALUE" value="56 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875575744002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575744002?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="11uA"/>
<attribute name="I-RIPPLE" value="1100mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575744002 "/>
<attribute name="RESR" value="80mohm"/>
<attribute name="VALUE" value="22 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
<technology name="_875575844001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575844001?ae"/>
<attribute name="DF" value="8%"/>
<attribute name="DIAMETER" value="6.3mm"/>
<attribute name="I-LEAK" value="6.3uA"/>
<attribute name="I-RIPPLE" value="1000mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575844001 "/>
<attribute name="RESR" value="120mohm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="63V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WCAP-HSG5_D5H5.8P1.4" prefix="C">
<description>&lt;b&gt;WCAP-HSG5 General Purpose 105°C &lt;/B&gt;&lt;BR&gt;&lt;BR&gt;

&lt;B&gt;Characteristics&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;General purpose product series
&lt;BR&gt;Low ESR
&lt;BR&gt;High ripple current characteristics
&lt;BR&gt;High stability over the temperature range
&lt;BR&gt;Low leakage current
&lt;BR&gt;Endurance: 10000h @ +105 °C
&lt;BR&gt;Operating temperature: -55 °C up to +105 °C
&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Industry and telecommunication
&lt;BR&gt;Smoothing
&lt;BR&gt;e.g. Servo inverter, air conditioner, industrial power supply, security camera, base station
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o696140v209%20multi-WCAP-HSG5-875575344001.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WCAP-HSG5"&gt;https://www.we-online.com/en/components/products/WCAP-HSG5&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-26&lt;br&gt;
2023(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="C_POLAR"/>
</gates>
<devices>
<device name="" package="WCAP-HSG5_D5H5.8P1.4">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_875575559001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575559001?ae"/>
<attribute name="DF" value="14%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="8.3uA"/>
<attribute name="I-RIPPLE" value="900mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575559001 "/>
<attribute name="RESR" value="80mohm"/>
<attribute name="VALUE" value="33 µF"/>
<attribute name="VR" value="25V(DC)"/>
</technology>
<technology name="_875575759001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/875575759001?ae"/>
<attribute name="DF" value="10%"/>
<attribute name="DIAMETER" value="5mm"/>
<attribute name="I-LEAK" value="5uA"/>
<attribute name="I-RIPPLE" value="750mA"/>
<attribute name="LENGTH" value="5.8mm"/>
<attribute name="PART-NUMBER" value=" 875575759001 "/>
<attribute name="RESR" value="120mohm"/>
<attribute name="VALUE" value="10 µF"/>
<attribute name="VR" value="50V(DC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
