<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-HCFT&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-05-15&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCFT_2012_1.2WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 2012, SMT</description>
</package>
<package name="WE-HCFT_2012_1.5WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 2012, SMT</description>
</package>
<package name="WE-HCFT_3540_2.0WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3540, SMT</description>
</package>
<package name="WE-HCFT_3533_1.8WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3533, SMT</description>
</package>
<package name="WE-HCFT_3533_2.0WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3533, SMT</description>
</package>
<package name="WE-HCFT_3540_1.3WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3540, SMT</description>
</package>
<package name="WE-HCFT_3521">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3521, SMT</description>
</package>
<package name="WE-HCFT_2504_PIN0.5MM">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 2504, SMT
&lt;br&gt;Pad width=0.5mm</description>
</package>
<package name="WE-HCFT_3540_0.8WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3540, SMT</description>
</package>
<package name="WE-HCFT_3540_1.5WIRE">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 3540, SMT</description>
</package>
<package name="WE-HCFT_2504_PIN1.0MM">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 2504, SMT
&lt;br&gt;Pad width=1.0mm</description>
</package>
<package name="WE-HCFT_2504_PIN0.6MM">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 2504, SMT
&lt;br&gt;Pad width=0.6mm</description>
</package>
<package name="WE-HCFT_2504_PIN0.7MM">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
Size: 2504, SMT
&lt;br&gt;Pad width=0.6mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCFT_2012" prefix="L">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor
&lt;br&gt;&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; THT version to assure the mechanical stability
&lt;br&gt;Inductance ranging from 1.5 µH up to 65 µH
&lt;br&gt;Current capability up to 75 A (Saturation &gt;125 A)
&lt;br&gt;Extremely low DCR
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters
&lt;br&gt;High current Power Supplies
&lt;br&gt;Battery chargers
&lt;br&gt;Solar inverter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCFT"&gt;www.we-online.com/en/components/products/WE-HCFT&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2020-11-03&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="_1.2WIRE" package="WE-HCFT_2012_1.2WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443782012068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443782012068?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="20.6A"/>
<attribute name="ISAT" value="30.6A"/>
<attribute name="PART-NUMBER" value=" 7443782012068 "/>
<attribute name="RDC-MAX" value="5mOhm"/>
<attribute name="RDC-TYPE" value="4.55mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443782012082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443782012082?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="20.6A"/>
<attribute name="ISAT" value="25.6A"/>
<attribute name="PART-NUMBER" value=" 7443782012082 "/>
<attribute name="RDC-MAX" value="5mOhm"/>
<attribute name="RDC-TYPE" value="4.55mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7443782012100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443782012100?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="20.6A"/>
<attribute name="ISAT" value="20.6A"/>
<attribute name="PART-NUMBER" value=" 7443782012100 "/>
<attribute name="RDC-MAX" value="5mOhm"/>
<attribute name="RDC-TYPE" value="4.55mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7443782012150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443782012150?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="20.6A"/>
<attribute name="ISAT" value="12.9A"/>
<attribute name="PART-NUMBER" value=" 7443782012150 "/>
<attribute name="RDC-MAX" value="5mOhm"/>
<attribute name="RDC-TYPE" value="4.55mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
<device name="_1.5WIRE" package="WE-HCFT_2012_1.5WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443782012033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443782012033?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="28.7A"/>
<attribute name="ISAT" value="43A"/>
<attribute name="PART-NUMBER" value=" 7443782012033 "/>
<attribute name="RDC-MAX" value="2.4mOhm"/>
<attribute name="RDC-TYPE" value="2.2mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7443782012047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443782012047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="28.7A"/>
<attribute name="ISAT" value="29.8A"/>
<attribute name="PART-NUMBER" value=" 7443782012047 "/>
<attribute name="RDC-MAX" value="2.4mOhm"/>
<attribute name="RDC-TYPE" value="2.2mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCFT_3533" prefix="L">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor
&lt;br&gt;&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; THT version to assure the mechanical stability
&lt;br&gt;Inductance ranging from 1.5 µH up to 65 µH
&lt;br&gt;Current capability up to 75 A (Saturation &gt;125 A)
&lt;br&gt;Extremely low DCR
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters
&lt;br&gt;High current Power Supplies
&lt;br&gt;Battery chargers
&lt;br&gt;Solar inverter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCFT"&gt;www.we-online.com/en/components/products/WE-HCFT&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2020-11-03&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="_2.0WIRE" package="WE-HCFT_3533_2.0WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443783533220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443783533220?ae"/>
<attribute name="FRES" value="8.15MHz"/>
<attribute name="IR" value="23.2A"/>
<attribute name="ISAT" value="49.4A"/>
<attribute name="PART-NUMBER" value=" 7443783533220 "/>
<attribute name="RDC-MAX" value="8.8mOhm"/>
<attribute name="RDC-TYPE" value="8mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7443783533330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443783533330?ae"/>
<attribute name="FRES" value="6.08MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="39.2A"/>
<attribute name="PART-NUMBER" value=" 7443783533330 "/>
<attribute name="RDC-MAX" value="9.9mOhm"/>
<attribute name="RDC-TYPE" value="9mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
<device name="_1.8WIRE" package="WE-HCFT_3533_1.8WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443783533470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443783533470?ae"/>
<attribute name="FRES" value="5.1MHz"/>
<attribute name="IR" value="19.3A"/>
<attribute name="ISAT" value="32.3A"/>
<attribute name="PART-NUMBER" value=" 7443783533470 "/>
<attribute name="RDC-MAX" value="12.98mOhm"/>
<attribute name="RDC-TYPE" value="11.8mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_7443783533650">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443783533650?ae"/>
<attribute name="FRES" value="4.28MHz"/>
<attribute name="IR" value="17.2A"/>
<attribute name="ISAT" value="26.6A"/>
<attribute name="PART-NUMBER" value=" 7443783533650 "/>
<attribute name="RDC-MAX" value="14.44mOhm"/>
<attribute name="RDC-TYPE" value="13.13mOhm"/>
<attribute name="VALUE" value="65uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCFT_3521" prefix="L">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor
&lt;br&gt;&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; THT version to assure the mechanical stability
&lt;br&gt;Inductance ranging from 1.5 µH up to 65 µH
&lt;br&gt;Current capability up to 75 A (Saturation &gt;125 A)
&lt;br&gt;Extremely low DCR
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters
&lt;br&gt;High current Power Supplies
&lt;br&gt;Battery chargers
&lt;br&gt;Solar inverter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCFT"&gt;www.we-online.com/en/components/products/WE-HCFT&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2020-11-03&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-HCFT_3521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443763521015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763521015?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="75A"/>
<attribute name="ISAT" value="125A"/>
<attribute name="PART-NUMBER" value=" 7443763521015 "/>
<attribute name="RDC-MAX" value="0.4mOhm"/>
<attribute name="RDC-TYPE" value="0.34mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443763521022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763521022?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="75A"/>
<attribute name="ISAT" value="120A"/>
<attribute name="PART-NUMBER" value=" 7443763521022 "/>
<attribute name="RDC-MAX" value="0.4mOhm"/>
<attribute name="RDC-TYPE" value="0.34mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7443763521033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763521033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="75A"/>
<attribute name="ISAT" value="91A"/>
<attribute name="PART-NUMBER" value=" 7443763521033 "/>
<attribute name="RDC-MAX" value="0.4mOhm"/>
<attribute name="RDC-TYPE" value="0.34mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCFT_2504" prefix="L">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor
&lt;br&gt;&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; THT version to assure the mechanical stability
&lt;br&gt;Inductance ranging from 1.5 µH up to 65 µH
&lt;br&gt;Current capability up to 75 A (Saturation &gt;125 A)
&lt;br&gt;Extremely low DCR
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters
&lt;br&gt;High current Power Supplies
&lt;br&gt;Battery chargers
&lt;br&gt;Solar inverter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCFT"&gt;www.we-online.com/en/components/products/WE-HCFT&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2020-11-03&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="_PIN0.5MM" package="WE-HCFT_2504_PIN0.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443762504068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443762504068?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="12.6A"/>
<attribute name="PART-NUMBER" value=" 7443762504068 "/>
<attribute name="RDC-MAX" value="4.63mOhm"/>
<attribute name="RDC-TYPE" value="4.21mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443762504100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443762504100?ae"/>
<attribute name="FRES" value="8.4MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="8.8A"/>
<attribute name="PART-NUMBER" value=" 7443762504100 "/>
<attribute name="RDC-MAX" value="4.63mOhm"/>
<attribute name="RDC-TYPE" value="4.21mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_PIN0.6MM" package="WE-HCFT_2504_PIN0.6MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443762504047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443762504047?ae"/>
<attribute name="FRES" value="14.5MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="PART-NUMBER" value=" 7443762504047 "/>
<attribute name="RDC-MAX" value="3.05mOhm"/>
<attribute name="RDC-TYPE" value="2.77mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
<device name="_PIN1.0MM" package="WE-HCFT_2504_PIN1.0MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443762504010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443762504010?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="39A"/>
<attribute name="ISAT" value="33A"/>
<attribute name="PART-NUMBER" value=" 7443762504010 "/>
<attribute name="RDC-MAX" value="0.95mOhm"/>
<attribute name="RDC-TYPE" value="0.86mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
</technologies>
</device>
<device name="_PIN0.7MM" package="WE-HCFT_2504_PIN0.7MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443762504022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443762504022?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="23.8A"/>
<attribute name="PART-NUMBER" value=" 7443762504022 "/>
<attribute name="RDC-MAX" value="1.96mOhm"/>
<attribute name="RDC-TYPE" value="1.78mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCFT_3540" prefix="L">
<description>&lt;b&gt;WE-HCFT THT High Current Inductor
&lt;br&gt;&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; THT version to assure the mechanical stability
&lt;br&gt;Inductance ranging from 1.5 µH up to 65 µH
&lt;br&gt;Current capability up to 75 A (Saturation &gt;125 A)
&lt;br&gt;Extremely low DCR
&lt;br&gt;Low core losses (MnZn)
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature -40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Storage inductor for high efficiency DC/DC converters
&lt;br&gt;High current Power Supplies
&lt;br&gt;Battery chargers
&lt;br&gt;Solar inverter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o133807v209%20Family_WE-HCFT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-HCFT"&gt;www.we-online.com/en/components/products/WE-HCFT&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2020-11-03&lt;br&gt;
2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="_2.0WIRE" package="WE-HCFT_3540_2.0WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443763540068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763540068?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="56.7A"/>
<attribute name="ISAT" value="76.5A"/>
<attribute name="PART-NUMBER" value=" 7443763540068 "/>
<attribute name="RDC-MAX" value="1.2mOhm"/>
<attribute name="RDC-TYPE" value="1.01mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7443763540100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763540100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="56.7A"/>
<attribute name="ISAT" value="62A"/>
<attribute name="PART-NUMBER" value=" 7443763540100 "/>
<attribute name="RDC-MAX" value="1.2mOhm"/>
<attribute name="RDC-TYPE" value="1.01mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_0.8WIRE" package="WE-HCFT_3540_0.8WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443763540330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763540330?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="32A"/>
<attribute name="ISAT" value="38.9A"/>
<attribute name="PART-NUMBER" value=" 7443763540330 "/>
<attribute name="RDC-MAX" value="6.38mOhm"/>
<attribute name="RDC-TYPE" value="5.67mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7443763540470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763540470?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="32A"/>
<attribute name="ISAT" value="31A"/>
<attribute name="PART-NUMBER" value=" 7443763540470 "/>
<attribute name="RDC-MAX" value="6.38mOhm"/>
<attribute name="RDC-TYPE" value="5.67mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
<device name="_1.3WIRE" package="WE-HCFT_3540_1.3WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443763540220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763540220?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="40.6A"/>
<attribute name="ISAT" value="42A"/>
<attribute name="PART-NUMBER" value=" 7443763540220 "/>
<attribute name="RDC-MAX" value="3.2mOhm"/>
<attribute name="RDC-TYPE" value="2.63mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
<device name="_1.5WIRE" package="WE-HCFT_3540_1.5WIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443763540150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443763540150?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="45.3A"/>
<attribute name="ISAT" value="51.6A"/>
<attribute name="PART-NUMBER" value=" 7443763540150 "/>
<attribute name="RDC-MAX" value="2.16mOhm"/>
<attribute name="RDC-TYPE" value="1.77mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
