<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-HCM&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-04-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCM_4035_74434035007">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 4035, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 5X3.1X3.5X1.55mm</description>
</package>
<package name="WE-HCM_4035_74434035010">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 4035, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 5X3.1X3.5X1.55mm</description>
</package>
<package name="WE-HCM_7070">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7070, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 7X7X7X2mm</description>
</package>
<package name="WE-HCM_1323">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1323, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 13X10.5X2.3X6.9mm</description>
</package>
<package name="WE-HCM_1078">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1078, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 9.4X6.2X7.8X1.8mm</description>
</package>
<package name="WE-HCM_1820_TWO-TURNS">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1820, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 16.4X13.6X2X3mm</description>
</package>
<package name="WE-HCM_1435">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1435, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 13.5X13.65X3.5X9.6mm</description>
</package>
<package name="WE-HCM_1070">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1070, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10.1X7X6.8X2.6mm</description>
</package>
<package name="WE-HCM_1390">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1390, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 14X13X9X1.8mm</description>
</package>
<package name="WE-HCM_4030">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 4030, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 4.1X3.1X3X4.8mm</description>
</package>
<package name="WE-HCM_1411">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1411, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 14.5X13.5X10.7X2.7mm</description>
</package>
<package name="WE-HCM_1350">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1350, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 13.5X13.3X5X2mm</description>
</package>
<package name="WE-HCM_1820_PARALLEL">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1820, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 16.4X13.6X2X3mm</description>
</package>
<package name="WE-HCM_1088B">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1088B, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10.8X8.2X8.5X2.8mm</description>
</package>
<package name="WE-HCM_1050">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1050, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10.2X7X5X2.5mm</description>
</package>
<package name="WE-HCM_1088A">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1088A, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10.2X8.1X8X2.5mm</description>
</package>
<package name="WE-HCM_1820">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1820, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 16.4X13.6X2X3mm</description>
</package>
<package name="WE-HCM_1190">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1190, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 11.3X11X8.9X2.2mm</description>
</package>
<package name="WE-HCM_1088">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1088, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10.2X8X8.1X2.5mm</description>
</package>
<package name="WE-HCM_9065">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 9065, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 8.64X6.35X4.5X2.7mm</description>
</package>
<package name="WE-HCM_1820_THREE-TURNS">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1820, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 16.4X13.6X2X3mm</description>
</package>
<package name="WE-HCM_1012">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1012, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10X6X12X2.4mm</description>
</package>
<package name="WE-HCM_5030">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 5030, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 5X3.1X3X5.6mm</description>
</package>
<package name="WE-HCM_1052">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1052, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 10.5X10.3X5X2mm</description>
</package>
<package name="WE-HCM_7050">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7050, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 7.15X7X5X2.5mm</description>
</package>
<package name="WE-HCM_1240">
<description>&lt;b&gt;WE-HCM SMD High Current Flat Wire Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1240, SMT, 2Pins
&lt;br&gt;LXWXHXFI = 11.5X11.8X3.8X1.75mm</description>
</package>
</packages>
<symbols>
<symbol name="L_POINT_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820_TWO-TURNS">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820_PARALLEL">
<pin name="IN" direction="pas"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820_THREE-TURNS">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-HCM_1820">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCM_4035" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="_74434035007" package="WE-HCM_4035_74434035007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74434035007?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="29A"/>
<attribute name="ISAT" value="17A@10%"/>
<attribute name="ISAT2" value="18.1A@30%"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="LR" value="0.01uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.55mm"/>
<attribute name="PART-NUMBER" value="74434035007"/>
<attribute name="RDC" value="0.38mOhm"/>
<attribute name="SIZE" value="4035"/>
<attribute name="VALUE" value="0.07uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
</technologies>
</device>
<device name="_74434035010" package="WE-HCM_4035_74434035010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74434035010?ae"/>
<attribute name="FRES" value="69MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="29A"/>
<attribute name="ISAT" value="18.1A@10%"/>
<attribute name="ISAT2" value="19.1A@30%"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="LR" value="0.016uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.55mm"/>
<attribute name="PART-NUMBER" value="74434035010"/>
<attribute name="RDC" value="0.38mOhm"/>
<attribute name="SIZE" value="4035"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_7070" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_7070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744307012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744307012?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="HEIGHT" value="7mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="43.3A@10%"/>
<attribute name="ISAT2" value="48.5A@30%"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LR" value="0.118uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744307012"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744307016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744307016?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="7mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="40A@10%"/>
<attribute name="ISAT2" value="51.7A@30%"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LR" value="0.155uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744307016"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744307022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744307022?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="7mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="26.8A@10%"/>
<attribute name="ISAT2" value="29.9A@30%"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="LR" value="0.174uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744307022"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="7070"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1323" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1323">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74431323012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431323012?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="2.3mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="40.1A@10%"/>
<attribute name="ISAT2" value="47.8A@30%"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="LR" value="0.117uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="6.9mm"/>
<attribute name="PART-NUMBER" value="74431323012"/>
<attribute name="RDC" value="0.7mOhm"/>
<attribute name="SIZE" value="1323"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
<technology name="_74431323016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431323016?ae"/>
<attribute name="FRES" value="113MHz"/>
<attribute name="HEIGHT" value="2.3mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="28.9A@10%"/>
<attribute name="ISAT2" value="35.1A@30%"/>
<attribute name="LENGTH" value="13mm"/>
<attribute name="LR" value="0.149uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="6.9mm"/>
<attribute name="PART-NUMBER" value="74431323016"/>
<attribute name="RDC" value="0.7mOhm"/>
<attribute name="SIZE" value="1323"/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="10.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1078" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1078">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443081010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081010?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="91.3A@10%"/>
<attribute name="ISAT2" value="104.4A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081010"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
<technology name="_7443081012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081012?ae"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="78.2A@10%"/>
<attribute name="ISAT2" value="88.5A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.12uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081012"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
<technology name="_7443081015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="67A@10%"/>
<attribute name="ISAT2" value="75A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081015"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
<technology name="_7443081018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081018?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="55.6A@10%"/>
<attribute name="ISAT2" value="63.4A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.176uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081018"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
<technology name="_7443081022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081022?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="39.1A@10%"/>
<attribute name="ISAT2" value="48.4A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.2uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081022"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
<technology name="_7443081030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081030?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="28.9A@10%"/>
<attribute name="ISAT2" value="34.6A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.14uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081030"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
<technology name="_7443081040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443081040?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="7.8mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="20.1A@10%"/>
<attribute name="ISAT2" value="24.1A@30%"/>
<attribute name="LENGTH" value="9.4mm"/>
<attribute name="LR" value="0.05uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="7443081040"/>
<attribute name="RDC" value="0.29mOhm"/>
<attribute name="SIZE" value="1078"/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="6.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820_TWO-TURNS" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820_TWO-TURNS"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820_TWO-TURNS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431821100?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="21A"/>
<attribute name="ISAT" value="6.6A@10%"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="3mm"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="SIZE" value="1820"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="13.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1435" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1435">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74431435010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431435010?ae"/>
<attribute name="FRES" value="87MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="72.5A@10%"/>
<attribute name="ISAT2" value="82.6A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.099uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="9.6mm"/>
<attribute name="PART-NUMBER" value="74431435010"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="SIZE" value="1435"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="13.65mm"/>
</technology>
<technology name="_74431435012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431435012?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="62.7A@10%"/>
<attribute name="ISAT2" value="71.3A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.119uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="9.6mm"/>
<attribute name="PART-NUMBER" value="74431435012"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="SIZE" value="1435"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="13.65mm"/>
</technology>
<technology name="_74431435015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431435015?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="55.8A@10%"/>
<attribute name="ISAT2" value="64.8A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.147uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="9.6mm"/>
<attribute name="PART-NUMBER" value="74431435015"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="SIZE" value="1435"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="13.65mm"/>
</technology>
<technology name="_74431435018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431435018?ae"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="49.7A@10%"/>
<attribute name="ISAT2" value="58.4A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.175uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="9.6mm"/>
<attribute name="PART-NUMBER" value="74431435018"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="SIZE" value="1435"/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="13.65mm"/>
</technology>
<technology name="_74431435022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431435022?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="3.5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="37.6A@10%"/>
<attribute name="ISAT2" value="43A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.211uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="9.6mm"/>
<attribute name="PART-NUMBER" value="74431435022"/>
<attribute name="RDC" value="0.28mOhm"/>
<attribute name="SIZE" value="1435"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="13.65mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1070" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744308015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744308015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="6.8mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="53.8A@10%"/>
<attribute name="ISAT2" value="60.7A@30%"/>
<attribute name="LENGTH" value="10.1mm"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.6mm"/>
<attribute name="PART-NUMBER" value="744308015"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="SIZE" value="1070"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744308020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744308020?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="6.8mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="44A@10%"/>
<attribute name="ISAT2" value="50.4A@30%"/>
<attribute name="LENGTH" value="10.1mm"/>
<attribute name="LR" value="0.198uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.6mm"/>
<attribute name="PART-NUMBER" value="744308020"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="SIZE" value="1070"/>
<attribute name="VALUE" value="0.2uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744308025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744308025?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="6.8mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="41.6A@10%"/>
<attribute name="ISAT2" value="46.5A@30%"/>
<attribute name="LENGTH" value="10.1mm"/>
<attribute name="LR" value="0.246uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.6mm"/>
<attribute name="PART-NUMBER" value="744308025"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="SIZE" value="1070"/>
<attribute name="VALUE" value="0.25uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744308033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744308033?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="6.8mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="27.3A@10%"/>
<attribute name="ISAT2" value="32A@30%"/>
<attribute name="LENGTH" value="10.1mm"/>
<attribute name="LR" value="0.305uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.6mm"/>
<attribute name="PART-NUMBER" value="744308033"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="SIZE" value="1070"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744308040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744308040?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="6.8mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="23.8A@10%"/>
<attribute name="ISAT2" value="28.3A@30%"/>
<attribute name="LENGTH" value="10.1mm"/>
<attribute name="LR" value="0.345uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.6mm"/>
<attribute name="PART-NUMBER" value="744308040"/>
<attribute name="RDC" value="0.37mOhm"/>
<attribute name="SIZE" value="1070"/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1390" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1390">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744309012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744309012?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="125A@10%"/>
<attribute name="ISAT2" value="125A@30%"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="LR" value="0.12uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="744309012"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="SIZE" value="1390"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
<technology name="_744309025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744309025?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="75.6A@10%"/>
<attribute name="ISAT2" value="88.5A@30%"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="LR" value="0.245uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="744309025"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="SIZE" value="1390"/>
<attribute name="VALUE" value="0.25uH"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
<technology name="_744309033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744309033?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="58A@10%"/>
<attribute name="ISAT2" value="65.7A@30%"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="LR" value="0.31uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="744309033"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="SIZE" value="1390"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
<technology name="_744309047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744309047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="9mm"/>
<attribute name="IR" value="47.5A"/>
<attribute name="ISAT" value="35.1A@10%"/>
<attribute name="ISAT2" value="46.8A@30%"/>
<attribute name="LENGTH" value="14mm"/>
<attribute name="LR" value="0.2uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.8mm"/>
<attribute name="PART-NUMBER" value="744309047"/>
<attribute name="RDC" value="0.165mOhm"/>
<attribute name="SIZE" value="1390"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="13mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_4030" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744340300025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744340300025?ae"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="48.9A@10%"/>
<attribute name="ISAT2" value="51A@30%"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="LR" value="0.025uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="4.8mm"/>
<attribute name="PART-NUMBER" value="744340300025"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.025uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
<technology name="_744340300030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744340300030?ae"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="47.3A@10%"/>
<attribute name="ISAT2" value="50.6A@30%"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="LR" value="0.029uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="4.8mm"/>
<attribute name="PART-NUMBER" value="744340300030"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.03uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
<technology name="_744340300055">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744340300055?ae"/>
<attribute name="FRES" value="123MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="23.6A@10%"/>
<attribute name="ISAT2" value="25.2A@30%"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="LR" value="0.055uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="4.8mm"/>
<attribute name="PART-NUMBER" value="744340300055"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.055uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
<technology name="_744340300075">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744340300075?ae"/>
<attribute name="FRES" value="106MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="18.7A@10%"/>
<attribute name="ISAT2" value="23.5A@30%"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="LR" value="0.075uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="4.8mm"/>
<attribute name="PART-NUMBER" value="744340300075"/>
<attribute name="RDC" value="0.27mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.075uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1411" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1411">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443091062">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443091062?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="10.7mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="68.4A@10%"/>
<attribute name="ISAT2" value="74A@30%"/>
<attribute name="LENGTH" value="14.5mm"/>
<attribute name="LR" value="0.62uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="7443091062"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="SIZE" value="1411"/>
<attribute name="VALUE" value="0.62uH"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7443091080">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443091080?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="10.7mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="53.1A@10%"/>
<attribute name="ISAT2" value="58.5A@30%"/>
<attribute name="LENGTH" value="14.5mm"/>
<attribute name="LR" value="0.78uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="7443091080"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="SIZE" value="1411"/>
<attribute name="VALUE" value="0.8uH"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7443091100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443091100?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="10.7mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="38.5A@10%"/>
<attribute name="ISAT2" value="43.5A@30%"/>
<attribute name="LENGTH" value="14.5mm"/>
<attribute name="LR" value="0.95uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="7443091100"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="SIZE" value="1411"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7443091120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443091120?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="10.7mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="32.2A@10%"/>
<attribute name="ISAT2" value="38.3A@30%"/>
<attribute name="LENGTH" value="14.5mm"/>
<attribute name="LR" value="1.02uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="7443091120"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="SIZE" value="1411"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7443091150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443091150?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="10.7mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="22.5A@10%"/>
<attribute name="ISAT2" value="27.1A@30%"/>
<attribute name="LENGTH" value="14.5mm"/>
<attribute name="LR" value="0.18uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="7443091150"/>
<attribute name="RDC" value="0.42mOhm"/>
<attribute name="SIZE" value="1411"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1088B" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-04-23&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1088B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443082010B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082010B?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="103A@10%"/>
<attribute name="ISAT2" value="117A@30%"/>
<attribute name="LENGTH" value="10.8mm"/>
<attribute name="LR" value="0.104uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.8mm"/>
<attribute name="PART-NUMBER" value="7443082010B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="SIZE" value="1088B"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="8.2mm"/>
</technology>
<technology name="_7443082012B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082012B?ae"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="93.6A@10%"/>
<attribute name="ISAT2" value="100.9A@30%"/>
<attribute name="LENGTH" value="10.8mm"/>
<attribute name="LR" value="0.117uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.8mm"/>
<attribute name="PART-NUMBER" value="7443082012B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="SIZE" value="1088B"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="8.2mm"/>
</technology>
<technology name="_7443082015B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082015B?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="8.5mm"/>
<attribute name="IR" value="70A"/>
<attribute name="ISAT" value="80.7A@10%"/>
<attribute name="ISAT2" value="88.4A@30%"/>
<attribute name="LENGTH" value="10.8mm"/>
<attribute name="LR" value="0.143uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.8mm"/>
<attribute name="PART-NUMBER" value="7443082015B"/>
<attribute name="RDC" value="0.114mOhm"/>
<attribute name="SIZE" value="1088B"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="8.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820_PARALLEL" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820_PARALLEL">
<connects>
<connect gate="G$1" pin="IN" pad="1 2 3" route="any"/>
<connect gate="G$1" pin="OUT" pad="4 5 6" route="any"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431821100?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="6.6A@10%"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="3mm"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="SIZE" value="1820"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="13.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1088A" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-04-23&lt;br&gt;
2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1088A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443082015A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082015A?ae"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="65A"/>
<attribute name="ISAT" value="68.5A@10%"/>
<attribute name="ISAT2" value="76.9A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.136uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082015A"/>
<attribute name="RDC" value="0.15mOhm"/>
<attribute name="SIZE" value="1088A"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
<technology name="_7443082018A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082018A?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="65A"/>
<attribute name="ISAT" value="63.9A@10%"/>
<attribute name="ISAT2" value="72.7A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.157uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082018A"/>
<attribute name="RDC" value="0.15mOhm"/>
<attribute name="SIZE" value="1088A"/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="8.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1350" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1350">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744305022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744305022?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="39.9A@10%"/>
<attribute name="ISAT2" value="42A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.215uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744305022"/>
<attribute name="RDC" value="0.155mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="13.3mm"/>
</technology>
<technology name="_744305033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744305033?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="23.6A@10%"/>
<attribute name="ISAT2" value="27.7A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.27uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744305033"/>
<attribute name="RDC" value="0.155mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="13.3mm"/>
</technology>
<technology name="_744305040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744305040?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="16.8A@10%"/>
<attribute name="ISAT2" value="21.7A@30%"/>
<attribute name="LENGTH" value="13.5mm"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744305040"/>
<attribute name="RDC" value="0.155mOhm"/>
<attribute name="SIZE" value="1350"/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="13.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431821100?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="34A"/>
<attribute name="ISAT" value="6.6A@10%"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="3mm"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="SIZE" value="1820"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="13.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1190" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1190">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744301025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744301025?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="54.4A@10%"/>
<attribute name="ISAT2" value="64.7A@30%"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="LR" value="0.25uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.2mm"/>
<attribute name="PART-NUMBER" value="744301025"/>
<attribute name="RDC" value="0.32mOhm"/>
<attribute name="SIZE" value="1190"/>
<attribute name="VALUE" value="0.25uH"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_744301033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744301033?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="44.9A@10%"/>
<attribute name="ISAT2" value="48.9A@30%"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="LR" value="0.325uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.2mm"/>
<attribute name="PART-NUMBER" value="744301033"/>
<attribute name="RDC" value="0.32mOhm"/>
<attribute name="SIZE" value="1190"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
<technology name="_744301047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744301047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="8.9mm"/>
<attribute name="IR" value="38A"/>
<attribute name="ISAT" value="32.1A@10%"/>
<attribute name="ISAT2" value="36.1A@30%"/>
<attribute name="LENGTH" value="11.3mm"/>
<attribute name="LR" value="0.24uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.2mm"/>
<attribute name="PART-NUMBER" value="744301047"/>
<attribute name="RDC" value="0.32mOhm"/>
<attribute name="SIZE" value="1190"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="11mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1088" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1088">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443082010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082010?ae"/>
<attribute name="FRES" value="94MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="107.3A@10%"/>
<attribute name="ISAT2" value="114.1A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.099uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082010"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="SIZE" value="1088"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
<technology name="_7443082012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082012?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="93.1A@10%"/>
<attribute name="ISAT2" value="100A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.118uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082012"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="SIZE" value="1088"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
<technology name="_7443082015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082015?ae"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="80.5A@10%"/>
<attribute name="ISAT2" value="87.1A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.147uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082015"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="SIZE" value="1088"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
<technology name="_7443082017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082017?ae"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="62.9A@10%"/>
<attribute name="ISAT2" value="69.3A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082017"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="SIZE" value="1088"/>
<attribute name="VALUE" value="0.17uH"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
<technology name="_7443082018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082018?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="59.3A@10%"/>
<attribute name="ISAT2" value="66.4A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.165uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082018"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="SIZE" value="1088"/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
<technology name="_7443082022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443082022?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="8.1mm"/>
<attribute name="IR" value="60A"/>
<attribute name="ISAT" value="52.7A@10%"/>
<attribute name="ISAT2" value="59.3A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.154uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="7443082022"/>
<attribute name="RDC" value="0.18mOhm"/>
<attribute name="SIZE" value="1088"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1050" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744303012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744303012?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="51.2A@10%"/>
<attribute name="ISAT2" value="59.8A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.118uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="744303012"/>
<attribute name="RDC" value="0.325mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744303015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744303015?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="44.5A@10%"/>
<attribute name="ISAT2" value="51.5A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.15uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="744303015"/>
<attribute name="RDC" value="0.325mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.155uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744303022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744303022?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="31A"/>
<attribute name="ISAT" value="27A@10%"/>
<attribute name="ISAT2" value="34.5A@30%"/>
<attribute name="LENGTH" value="10.2mm"/>
<attribute name="LR" value="0.18uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="744303022"/>
<attribute name="RDC" value="0.325mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_9065" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_9065">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744300006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744300006?ae"/>
<attribute name="FRES" value="124MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="60.9A@10%"/>
<attribute name="ISAT2" value="65.6A@30%"/>
<attribute name="LENGTH" value="8.64mm"/>
<attribute name="LR" value="0.059uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="744300006"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="SIZE" value="9065"/>
<attribute name="VALUE" value="0.06uH"/>
<attribute name="WIDTH" value="6.35mm"/>
</technology>
<technology name="_744300008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744300008?ae"/>
<attribute name="FRES" value="94MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="48.7A@10%"/>
<attribute name="ISAT2" value="53.1A@30%"/>
<attribute name="LENGTH" value="8.64mm"/>
<attribute name="LR" value="0.078uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="744300008"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="SIZE" value="9065"/>
<attribute name="VALUE" value="0.08uH"/>
<attribute name="WIDTH" value="6.35mm"/>
</technology>
<technology name="_744300010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744300010?ae"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="39.5A@10%"/>
<attribute name="ISAT2" value="43.1A@30%"/>
<attribute name="LENGTH" value="8.64mm"/>
<attribute name="LR" value="0.093uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="744300010"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="SIZE" value="9065"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="6.35mm"/>
</technology>
<technology name="_744300015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744300015?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="28.3A@10%"/>
<attribute name="ISAT2" value="32.3A@30%"/>
<attribute name="LENGTH" value="8.64mm"/>
<attribute name="LR" value="0.034uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="744300015"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="SIZE" value="9065"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="6.35mm"/>
</technology>
<technology name="_744300022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744300022?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="4.5mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="18.8A@10%"/>
<attribute name="ISAT2" value="21.6A@30%"/>
<attribute name="LENGTH" value="8.64mm"/>
<attribute name="LR" value="0.024uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.7mm"/>
<attribute name="PART-NUMBER" value="744300022"/>
<attribute name="RDC" value="0.22mOhm"/>
<attribute name="SIZE" value="9065"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="6.35mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1820_THREE-TURNS" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCM_1820_THREE-TURNS"/>
</gates>
<devices>
<device name="" package="WE-HCM_1820_THREE-TURNS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_74431821100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431821100?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="23A"/>
<attribute name="ISAT" value="6.6A@10%"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="LENGTH" value="16.4mm"/>
<attribute name="LR" value="0.1uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="3mm"/>
<attribute name="PART-NUMBER" value="74431821100"/>
<attribute name="RDC" value="0.33mOhm"/>
<attribute name="SIZE" value="1820"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="13.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1012" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74431012007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431012007?ae"/>
<attribute name="FRES" value="149MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="125A@10%"/>
<attribute name="ISAT2" value="125A@30%"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LR" value="0.069uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.4mm"/>
<attribute name="PART-NUMBER" value="74431012007"/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="SIZE" value="1012"/>
<attribute name="VALUE" value="0.07uH"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_74431012010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431012010?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="125A@10%"/>
<attribute name="ISAT2" value="125A@30%"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LR" value="0.099uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.4mm"/>
<attribute name="PART-NUMBER" value="74431012010"/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="SIZE" value="1012"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_74431012012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431012012?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="121.1A@10%"/>
<attribute name="ISAT2" value="125A@30%"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LR" value="0.119uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.4mm"/>
<attribute name="PART-NUMBER" value="74431012012"/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="SIZE" value="1012"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_74431012015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74431012015?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IR" value="37A"/>
<attribute name="ISAT" value="99.4A@10%"/>
<attribute name="ISAT2" value="108.4A@30%"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LR" value="0.144uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.4mm"/>
<attribute name="PART-NUMBER" value="74431012015"/>
<attribute name="RDC" value="0.125mOhm"/>
<attribute name="SIZE" value="1012"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_5030" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435030010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74435030010?ae"/>
<attribute name="FRES" value="83MHz"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="18A@10%"/>
<attribute name="ISAT2" value="19.1A@30%"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="LR" value="0.01uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="5.6mm"/>
<attribute name="PART-NUMBER" value="74435030010"/>
<attribute name="RDC" value="0.31mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="3.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1052" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744306020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744306020?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="34A@10%"/>
<attribute name="ISAT2" value="36.1A@30%"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="LR" value="0.195uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744306020"/>
<attribute name="RDC" value="0.26mOhm"/>
<attribute name="SIZE" value="1052"/>
<attribute name="VALUE" value="0.2uH"/>
<attribute name="WIDTH" value="10.3mm"/>
</technology>
<technology name="_744306025">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744306025?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="30.3A@10%"/>
<attribute name="ISAT2" value="32.3A@30%"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="LR" value="0.24uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744306025"/>
<attribute name="RDC" value="0.26mOhm"/>
<attribute name="SIZE" value="1052"/>
<attribute name="VALUE" value="0.25uH"/>
<attribute name="WIDTH" value="10.3mm"/>
</technology>
<technology name="_744306030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744306030?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="22.2A@10%"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="LENGTH" value="10.5mm"/>
<attribute name="LR" value="0.22uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2mm"/>
<attribute name="PART-NUMBER" value="744306030"/>
<attribute name="RDC" value="0.26mOhm"/>
<attribute name="SIZE" value="1052"/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="WIDTH" value="10.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1240" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_1240">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744304010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744304010?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="57.4A@10%"/>
<attribute name="ISAT2" value="68.1A@30%"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="LR" value="0.095uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.75mm"/>
<attribute name="PART-NUMBER" value="744304010"/>
<attribute name="RDC" value="0.17mOhm"/>
<attribute name="SIZE" value="1240"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="11.8mm"/>
</technology>
<technology name="_744304016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744304016?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="34.2A@10%"/>
<attribute name="ISAT2" value="42.4A@30%"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="LR" value="0.127uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.75mm"/>
<attribute name="PART-NUMBER" value="744304016"/>
<attribute name="RDC" value="0.17mOhm"/>
<attribute name="SIZE" value="1240"/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="11.8mm"/>
</technology>
<technology name="_744304022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744304022?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="3.8mm"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="22.1A@10%"/>
<attribute name="ISAT2" value="27.7A@30%"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="LR" value="0.08uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="1.75mm"/>
<attribute name="PART-NUMBER" value="744304022"/>
<attribute name="RDC" value="0.17mOhm"/>
<attribute name="SIZE" value="1240"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="11.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_7050" prefix="L">
<description>&lt;b&gt;WE-HCM SMT High Current Flat Wire Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;High saturation current up to 125 A
&lt;br&gt;Extremly low DCR
&lt;br&gt;Magnetically shielded
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;CPU/RAM power supply
&lt;br&gt;Power PC
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14798v209%20family-WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HCM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-12-23&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-HCM_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744302007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744302007?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="62A@10%"/>
<attribute name="ISAT2" value="64A@30%"/>
<attribute name="LENGTH" value="7.15mm"/>
<attribute name="LR" value="0.071uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="744302007"/>
<attribute name="RDC" value="0.235mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.072uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744302010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744302010?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="45A@10%"/>
<attribute name="ISAT2" value="51A@30%"/>
<attribute name="LENGTH" value="7.15mm"/>
<attribute name="LR" value="0.104uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="744302010"/>
<attribute name="RDC" value="0.235mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.105uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
<technology name="_744302015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744302015?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="30A@10%"/>
<attribute name="ISAT2" value="35A@30%"/>
<attribute name="LENGTH" value="7.15mm"/>
<attribute name="LR" value="0.125uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PAD-WIDTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="744302015"/>
<attribute name="RDC" value="0.235mOhm"/>
<attribute name="SIZE" value="7050"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
