<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-PMFI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-07-01&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PMFI_353220">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;353220, SMT, 2pins
&lt;br&gt;LXWXH=3.5X3.2X2mm</description>
</package>
<package name="WE-PMFI_252012_LP2">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;252012, SMT, 2pins
&lt;br&gt;LXWXH=2.5X2X1.2mm
&lt;br&gt;This Land Pattern is compatible with the WE-PMCI series</description>
</package>
<package name="WE-PMFI_252012">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;252012, SMT, 2pins
&lt;br&gt;LXWXH=2.5X2X1.2mm</description>
</package>
<package name="WE-PMFI_201610">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;201610, SMT, 2pins
&lt;br&gt;LXWXH=2X1.6X1mm</description>
</package>
<package name="WE-PMFI_322512_LP2">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;322512, SMT, 2pins
&lt;br&gt;LXWXH=3.2X2.5X1.2mm
&lt;br&gt;This Land Pattern is compatible with the WE-PMCI series</description>
</package>
<package name="WE-PMFI_322512">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;322512, SMT, 2pins
&lt;br&gt;LXWXH=3.2X2.5X1.2mm</description>
</package>
<package name="WE-PMFI_201610_LP2">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor
&lt;/b&gt;&lt;br&gt;&lt;br&gt;201610, SMT, 2pins
&lt;br&gt;LXWXH=2X1.6X1mm
&lt;br&gt;This Land Pattern is compatible with the WE-PMCI series</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PMFI_353220" prefix="L">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very small profile molded power inductor
&lt;br&gt;High range of inductance values due to inner core construction
&lt;br&gt;Flat wire technology decreases RDC, starting at 4.8 mΩ
&lt;br&gt;High rated current values due to low RDC, up to 16 A
&lt;br&gt;Very low total losses lead to a high efficiency
&lt;br&gt;Hohe Betriebstemperatur von -55°C bis +150°C
&lt;br&gt;AEC-Q 200 qualified

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC-converters for high current power supplies
&lt;br&gt;Wearables like smartphones, tablets and cameras
&lt;br&gt;CPU power supllies (IMX95)
&lt;br&gt;RAM power supplies (DDR5)
&lt;br&gt;Devices with low profiles and case sizes (Sensors)
&lt;br&gt;Battery powered devices
&lt;br&gt;High frequency devices (GaN and SiC)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMFI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-07-01
&lt;br&gt;&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_353220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479335329110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479335329110?ae"/>
<attribute name="FRES" value="310MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479335329110"/>
<attribute name="RDC-TYP" value="4.8mOhm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74479335329147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479335329147?ae"/>
<attribute name="FRES" value="92MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="9.9A"/>
<attribute name="ISAT" value="13.2A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479335329147"/>
<attribute name="RDC-TYP" value="12.7mOhm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74479335329210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479335329210?ae"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="7.3A"/>
<attribute name="ISAT" value="10.8A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479335329210"/>
<attribute name="RDC-TYP" value="18.4mOhm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74479335329222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479335329222?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="7.8A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479335329222"/>
<attribute name="RDC-TYP" value="31.6mOhm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74479335329247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479335329247?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="3.85A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479335329247"/>
<attribute name="RDC-TYP" value="63.2mOhm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMFI_252012" prefix="L">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very small profile molded power inductor
&lt;br&gt;High range of inductance values due to inner core construction
&lt;br&gt;Flat wire technology decreases RDC, starting at 4.8 mΩ
&lt;br&gt;High rated current values due to low RDC, up to 16 A
&lt;br&gt;Very low total losses lead to a high efficiency
&lt;br&gt;Hohe Betriebstemperatur von -55°C bis +150°C
&lt;br&gt;AEC-Q 200 qualified

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC-converters for high current power supplies
&lt;br&gt;Wearables like smartphones, tablets and cameras
&lt;br&gt;CPU power supllies (IMX95)
&lt;br&gt;RAM power supplies (DDR5)
&lt;br&gt;Devices with low profiles and case sizes (Sensors)
&lt;br&gt;Battery powered devices
&lt;br&gt;High frequency devices (GaN and SiC)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMFI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-07-01
&lt;br&gt;&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_252012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479325207110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207110?ae"/>
<attribute name="FRES" value="438MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="18.7A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207110"/>
<attribute name="RDC-TYP" value="5.6mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207147?ae"/>
<attribute name="FRES" value="97MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="9.3A"/>
<attribute name="ISAT" value="7.9A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207147"/>
<attribute name="RDC-TYP" value="11.3mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207210?ae"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="6.1A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207210"/>
<attribute name="RDC-TYP" value="23.8mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207222?ae"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207222"/>
<attribute name="RDC-TYP" value="50.1mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207247?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.75A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207247"/>
<attribute name="RDC-TYP" value="114mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_LP2" package="WE-PMFI_252012_LP2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479325207110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207110?ae"/>
<attribute name="FRES" value="438MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="18.7A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207110"/>
<attribute name="RDC-TYP" value="5.6mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207147?ae"/>
<attribute name="FRES" value="97MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="9.3A"/>
<attribute name="ISAT" value="7.9A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207147"/>
<attribute name="RDC-TYP" value="11.3mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207210?ae"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="6.1A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207210"/>
<attribute name="RDC-TYP" value="23.8mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207222?ae"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207222"/>
<attribute name="RDC-TYP" value="50.1mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479325207247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479325207247?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.75A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207247"/>
<attribute name="RDC-TYP" value="114mOhm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMFI_322512" prefix="L">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very small profile molded power inductor
&lt;br&gt;High range of inductance values due to inner core construction
&lt;br&gt;Flat wire technology decreases RDC, starting at 4.8 mΩ
&lt;br&gt;High rated current values due to low RDC, up to 16 A
&lt;br&gt;Very low total losses lead to a high efficiency
&lt;br&gt;Hohe Betriebstemperatur von -55°C bis +150°C
&lt;br&gt;AEC-Q 200 qualified

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC-converters for high current power supplies
&lt;br&gt;Wearables like smartphones, tablets and cameras
&lt;br&gt;CPU power supllies (IMX95)
&lt;br&gt;RAM power supplies (DDR5)
&lt;br&gt;Devices with low profiles and case sizes (Sensors)
&lt;br&gt;Battery powered devices
&lt;br&gt;High frequency devices (GaN and SiC)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMFI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-07-01
&lt;br&gt;&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_322512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479332257110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257110?ae"/>
<attribute name="FRES" value="405MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT" value="21.5A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257110"/>
<attribute name="RDC-TYP" value="7.4mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257147?ae"/>
<attribute name="FRES" value="126MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="10.6A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257147"/>
<attribute name="RDC-TYP" value="14.2mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257210?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="9.15A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257210"/>
<attribute name="RDC-TYP" value="23.3mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257222?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257222"/>
<attribute name="RDC-TYP" value="49.6mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257247?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257247"/>
<attribute name="RDC-TYP" value="107mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
<device name="_LP2" package="WE-PMFI_322512_LP2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479332257110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257110?ae"/>
<attribute name="FRES" value="405MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT" value="21.5A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257110"/>
<attribute name="RDC-TYP" value="7.4mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257147?ae"/>
<attribute name="FRES" value="126MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="10.6A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257147"/>
<attribute name="RDC-TYP" value="14.2mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257210?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="9.15A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257210"/>
<attribute name="RDC-TYP" value="23.3mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257222?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257222"/>
<attribute name="RDC-TYP" value="49.6mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_74479332257247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479332257247?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479332257247"/>
<attribute name="RDC-TYP" value="107mOhm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMFI_201610" prefix="L">
<description>&lt;b&gt;WE-PMFI Power Molded Flatwire Inductor&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Very small profile molded power inductor
&lt;br&gt;High range of inductance values due to inner core construction
&lt;br&gt;Flat wire technology decreases RDC, starting at 4.8 mΩ
&lt;br&gt;High rated current values due to low RDC, up to 16 A
&lt;br&gt;Very low total losses lead to a high efficiency
&lt;br&gt;Hohe Betriebstemperatur von -55°C bis +150°C
&lt;br&gt;AEC-Q 200 qualified

&lt;P&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;BR&gt;
&lt;br&gt;DC/DC-converters for high current power supplies
&lt;br&gt;Wearables like smartphones, tablets and cameras
&lt;br&gt;CPU power supllies (IMX95)
&lt;br&gt;RAM power supplies (DDR5)
&lt;br&gt;Devices with low profiles and case sizes (Sensors)
&lt;br&gt;Battery powered devices
&lt;br&gt;High frequency devices (GaN and SiC)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o843010v209%20Model-WE-PMFI-744793xxxxxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMFI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-07-01
&lt;br&gt;&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_201610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479320165110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165110?ae"/>
<attribute name="FRES" value="325MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="10.2A"/>
<attribute name="ISAT" value="13.7A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165110"/>
<attribute name="RDC-TYP" value="7.2mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165147?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165147"/>
<attribute name="RDC-TYP" value="18.4mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165210?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT" value="5.25A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165210"/>
<attribute name="RDC-TYP" value="31.7mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165222?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.75A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165222"/>
<attribute name="RDC-TYP" value="81.9mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165233?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2.25A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165233"/>
<attribute name="RDC-TYP" value="146mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165247?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165247"/>
<attribute name="RDC-TYP" value="195mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_LP2" package="WE-PMFI_201610_LP2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479320165110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165110?ae"/>
<attribute name="FRES" value="325MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="10.2A"/>
<attribute name="ISAT" value="13.7A"/>
<attribute name="L" value="0.1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165110"/>
<attribute name="RDC-TYP" value="7.2mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165147?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165147"/>
<attribute name="RDC-TYP" value="18.4mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165210?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT" value="5.25A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165210"/>
<attribute name="RDC-TYP" value="31.7mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165222?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.75A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165222"/>
<attribute name="RDC-TYP" value="81.9mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165233?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2.25A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165233"/>
<attribute name="RDC-TYP" value="146mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479320165247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479320165247?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479320165247"/>
<attribute name="RDC-TYP" value="195mOhm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
