<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-XHMI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-01-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-XHMI_7030">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 7070, SMT, 2pins
&lt;br&gt;LXWXH=7.9X7.6X3.0mm</description>
</package>
<package name="WE-XHMI_6030">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6030, SMT, 2pins
&lt;br&gt;L X W X H = 6.65mm X 6.45mm X 2.75mm</description>
</package>
<package name="WE-XHMI_5050">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 5050, SMT, 2pins
&lt;br&gt;LXWXH=5.55X5.35X5.1mm</description>
</package>
<package name="WE-XHMI_6060">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;6060, SMT, 2pins
&lt;br&gt;L X W X H = 6.65mm X 6.45mm X 5.8mm</description>
</package>
<package name="WE-XHMI_1510">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1510, SMT, 2pins
&lt;br&gt;L X W X H = 16.4mm X 15.4mm X 10mm</description>
</package>
<package name="WE-XHMI_5020">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 5020, SMT, 2pins
&lt;br&gt;LXWXH=5.55X5.35X2mm</description>
</package>
<package name="WE-XHMI_8080">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;8080, SMT, 2pins
&lt;br&gt;L X W X H = 8.8mm X 8.3mm X 7.8mm</description>
</package>
<package name="WE-XHMI_5030">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 5030, SMT, 2pins
&lt;br&gt;LXWXH=5.55X5.35X3mm</description>
</package>
<package name="WE-XHMI_1090">
<description>&lt;b&gt;WE-XHMI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: &lt;/b&gt;1090, SMT, 2pins
&lt;br&gt;L X W X H = 11.6mm X 10.5mm X 8.8mm</description>
</package>
<package name="WE-XHMI_7070">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 7070, SMT, 2pins
&lt;br&gt;LXWXH=7.9X7.6X7.1mm</description>
</package>
<package name="WE-XHMI_4030">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 4030, SMT, 2pins
&lt;br&gt;LXWXH=4.3X4.3X3mm</description>
</package>
<package name="WE-XHMI_4020">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 4020, SMT, 2pins
&lt;br&gt;LXWXH=4.3X4.3X2mm</description>
</package>
<package name="WE-XHMI_4040">
<description>&lt;b&gt;WE-XHMI SMD Power Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size: 4040, SMT, 2pins
&lt;br&gt;LXWXH=4.3X4.3X4.1mm</description>
</package>
</packages>
<symbols>
<symbol name="L_POINT_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-XHMI_7030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_7030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439384010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384010?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IRP" value="23.7A"/>
<attribute name="ISAT1" value="10.7A"/>
<attribute name="ISAT2" value="25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439384010 "/>
<attribute name="RDC" value="3.9mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439384012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384012?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IRP" value="23.6A"/>
<attribute name="ISAT1" value="10.2A"/>
<attribute name="ISAT2" value="21.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439384012 "/>
<attribute name="RDC" value="4.2mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74439384015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384015?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IRP" value="20.1A"/>
<attribute name="ISAT1" value="8.7A"/>
<attribute name="ISAT2" value="18.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439384015 "/>
<attribute name="RDC" value="5.1mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439384022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384022?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IRP" value="16.7A"/>
<attribute name="ISAT1" value="6.5A"/>
<attribute name="ISAT2" value="13.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439384022 "/>
<attribute name="RDC" value="7.9mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439384033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IRP" value="11.4A"/>
<attribute name="ISAT1" value="6.4A"/>
<attribute name="ISAT2" value="13.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439384033 "/>
<attribute name="RDC" value="14.4mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439384047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439384047?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IRP" value="9.5A"/>
<attribute name="ISAT1" value="4.9A"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439384047 "/>
<attribute name="RDC" value="19.8mOhm"/>
<attribute name="SIZE" value=" 7030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-12&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393440015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440015?ae"/>
<attribute name="FRES" value="191MHz"/>
<attribute name="IRP" value="37A"/>
<attribute name="ISAT1" value="26A"/>
<attribute name="ISAT2" value="56A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393440015 "/>
<attribute name="RDC" value="1.24mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_744393440018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440018?ae"/>
<attribute name="FRES" value="169MHz"/>
<attribute name="IRP" value="35.65A"/>
<attribute name="ISAT1" value="24.9A"/>
<attribute name="ISAT2" value="50.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393440018 "/>
<attribute name="RDC" value="1.32mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
<technology name="_744393440033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440033?ae"/>
<attribute name="FRES" value="113MHz"/>
<attribute name="IRP" value="27.35A"/>
<attribute name="ISAT1" value="20A"/>
<attribute name="ISAT2" value="42.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393440033 "/>
<attribute name="RDC" value="2.1mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744393440056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393440056?ae"/>
<attribute name="FRES" value="77MHz"/>
<attribute name="IRP" value="22.75A"/>
<attribute name="ISAT1" value="14.5A"/>
<attribute name="ISAT2" value="30.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393440056 "/>
<attribute name="RDC" value="2.9mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_74439344010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IRP" value="15.75A"/>
<attribute name="ISAT1" value="11A"/>
<attribute name="ISAT2" value="24.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439344010 "/>
<attribute name="RDC" value="5.5mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439344012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IRP" value="14.45A"/>
<attribute name="ISAT1" value="7.7A"/>
<attribute name="ISAT2" value="21.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439344012 "/>
<attribute name="RDC" value="6.4mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74439344022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IRP" value="10.85A"/>
<attribute name="ISAT1" value="7.5A"/>
<attribute name="ISAT2" value="16.25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439344022 "/>
<attribute name="RDC" value="10.5mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439344033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344033?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IRP" value="7.65A"/>
<attribute name="ISAT1" value="6.7A"/>
<attribute name="ISAT2" value="14.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439344033 "/>
<attribute name="RDC" value="19.2mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439344047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439344047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IRP" value="5.8A"/>
<attribute name="ISAT1" value="3.7A"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439344047 "/>
<attribute name="RDC" value="31mOhm"/>
<attribute name="SIZE" value=" 6030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_5050" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_5050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393305056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305056?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IRP" value="6.7A"/>
<attribute name="ISAT1" value="4.8A"/>
<attribute name="ISAT2" value="9.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393305056 "/>
<attribute name="RDC" value="21.8mOhm"/>
<attribute name="SIZE" value=" 5050 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744393305068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305068?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IRP" value="6.6A"/>
<attribute name="ISAT1" value="3.4A"/>
<attribute name="ISAT2" value="6.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393305068 "/>
<attribute name="RDC" value="23.7mOhm"/>
<attribute name="SIZE" value=" 5050 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744393305082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305082?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IRP" value="5.9A"/>
<attribute name="ISAT1" value="3.1A"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393305082 "/>
<attribute name="RDC" value="29.3mOhm"/>
<attribute name="SIZE" value=" 5050 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744393305100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IRP" value="5.0A"/>
<attribute name="ISAT1" value="3.6A"/>
<attribute name="ISAT2" value="6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393305100 "/>
<attribute name="RDC" value="35.4mOhm"/>
<attribute name="SIZE" value=" 5050 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744393305150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305150?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IRP" value="4.0A"/>
<attribute name="ISAT1" value="2.3A"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393305150 "/>
<attribute name="RDC" value="56.8mOhm"/>
<attribute name="SIZE" value=" 5050 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744393305220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393305220?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IRP" value="3.5A"/>
<attribute name="ISAT1" value="2A"/>
<attribute name="ISAT2" value="4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393305220 "/>
<attribute name="RDC" value="75.0mOhm"/>
<attribute name="SIZE" value=" 5050 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6060" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-12&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_6060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439346010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346010?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IRP" value="20.95A"/>
<attribute name="ISAT1" value="11A"/>
<attribute name="ISAT2" value="24A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346010 "/>
<attribute name="RDC" value="3.39mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439346012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346012?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IRP" value="20.5A"/>
<attribute name="ISAT1" value="12A"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346012 "/>
<attribute name="RDC" value="3.65mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74439346015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346015?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IRP" value="19.35A"/>
<attribute name="ISAT1" value="10A"/>
<attribute name="ISAT2" value="20.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346015 "/>
<attribute name="RDC" value="3.9mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439346018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IRP" value="17.35A"/>
<attribute name="ISAT1" value="9A"/>
<attribute name="ISAT2" value="18.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346018 "/>
<attribute name="RDC" value="4.7mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_74439346022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IRP" value="15.75A"/>
<attribute name="ISAT1" value="8.5A"/>
<attribute name="ISAT2" value="19.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346022 "/>
<attribute name="RDC" value="5.58mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439346033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346033?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IRP" value="10.7A"/>
<attribute name="ISAT1" value="7.5A"/>
<attribute name="ISAT2" value="15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346033 "/>
<attribute name="RDC" value="10.83mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439346047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IRP" value="9.6A"/>
<attribute name="ISAT1" value="6.5A"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346047 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74439346056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346056?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IRP" value="8.9A"/>
<attribute name="ISAT1" value="5.8A"/>
<attribute name="ISAT2" value="12.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346056 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74439346068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IRP" value="8.1A"/>
<attribute name="ISAT1" value="5.65A"/>
<attribute name="ISAT2" value="11.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346068 "/>
<attribute name="RDC" value="17.6mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74439346082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346082?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IRP" value="6.95A"/>
<attribute name="ISAT1" value="4.6A"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346082 "/>
<attribute name="RDC" value="23mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74439346100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346100?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IRP" value="6.4A"/>
<attribute name="ISAT1" value="5.05A"/>
<attribute name="ISAT2" value="9.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346100 "/>
<attribute name="RDC" value="26.5mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74439346150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439346150?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IRP" value="4.9A"/>
<attribute name="ISAT1" value="3.65A"/>
<attribute name="ISAT2" value="7.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439346150 "/>
<attribute name="RDC" value="42mOhm"/>
<attribute name="SIZE" value=" 6060 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_5020" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393330016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330016?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="IRP" value="24.7A"/>
<attribute name="ISAT1" value="17.5A"/>
<attribute name="ISAT2" value="41.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393330016 "/>
<attribute name="RDC" value="2.2mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.16uH"/>
</technology>
<technology name="_744393330033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330033?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IRP" value="20.8A"/>
<attribute name="ISAT1" value="12.2A"/>
<attribute name="ISAT2" value="27A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393330033 "/>
<attribute name="RDC" value="3.0mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744393330056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330056?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IRP" value="15.4A"/>
<attribute name="ISAT1" value="9.8A"/>
<attribute name="ISAT2" value="21.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393330056 "/>
<attribute name="RDC" value="5.2mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744393330068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393330068?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IRP" value="13.3A"/>
<attribute name="ISAT1" value="8.1A"/>
<attribute name="ISAT2" value="17.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393330068 "/>
<attribute name="RDC" value="6.7mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74439333010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439333010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IRP" value="11.4A"/>
<attribute name="ISAT1" value="6.3A"/>
<attribute name="ISAT2" value="14.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439333010 "/>
<attribute name="RDC" value="9.5mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439333012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439333012?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IRP" value="10.7A"/>
<attribute name="ISAT1" value="5.2A"/>
<attribute name="ISAT2" value="11.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439333012 "/>
<attribute name="RDC" value="10.8mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_5030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340033?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IRP" value="21.2A"/>
<attribute name="ISAT1" value="15.4A"/>
<attribute name="ISAT2" value="33.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393340033 "/>
<attribute name="RDC" value="3.01mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744393340056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340056?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IRP" value="18.3A"/>
<attribute name="ISAT1" value="11.6A"/>
<attribute name="ISAT2" value="24.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393340056 "/>
<attribute name="RDC" value="3.99mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744393340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393340068?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IRP" value="15.7A"/>
<attribute name="ISAT1" value="7.9A"/>
<attribute name="ISAT2" value="17.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393340068 "/>
<attribute name="RDC" value="4.09mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74439334010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334010?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IRP" value="14.7A"/>
<attribute name="ISAT1" value="5.8A"/>
<attribute name="ISAT2" value="13.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439334010 "/>
<attribute name="RDC" value="6.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439334012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334012?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IRP" value="13.6A"/>
<attribute name="ISAT1" value="7A"/>
<attribute name="ISAT2" value="13.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439334012 "/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74439334015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334015?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IRP" value="12.0A"/>
<attribute name="ISAT1" value="6A"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439334015 "/>
<attribute name="RDC" value="8.0mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439334022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334022?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IRP" value="10.3A"/>
<attribute name="ISAT1" value="5.8A"/>
<attribute name="ISAT2" value="12.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439334022 "/>
<attribute name="RDC" value="11.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439334033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IRP" value="8.2A"/>
<attribute name="ISAT1" value="3.6A"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439334033 "/>
<attribute name="RDC" value="16.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439334047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439334047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IRP" value="6.8A"/>
<attribute name="ISAT1" value="3.3A"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439334047 "/>
<attribute name="RDC" value="22.9mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1510" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-12&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_1510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439370047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370047?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IRP" value="29.7A"/>
<attribute name="ISAT1" value="20.9A"/>
<attribute name="ISAT2" value="47.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370047 "/>
<attribute name="RDC" value="3.1mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74439370068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370068?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IRP" value="25.3A"/>
<attribute name="ISAT1" value="17.8A"/>
<attribute name="ISAT2" value="40.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370068 "/>
<attribute name="RDC" value="4.1mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74439370082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370082?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IRP" value="21.35A"/>
<attribute name="ISAT1" value="15A"/>
<attribute name="ISAT2" value="36.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370082 "/>
<attribute name="RDC" value="5.5mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74439370100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370100?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IRP" value="19.6A"/>
<attribute name="ISAT1" value="12.9A"/>
<attribute name="ISAT2" value="31.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370100 "/>
<attribute name="RDC" value="6.4mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74439370150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IRP" value="14.7A"/>
<attribute name="ISAT1" value="10.25A"/>
<attribute name="ISAT2" value="26.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370150 "/>
<attribute name="RDC" value="10.5mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74439370220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370220?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IRP" value="13.35A"/>
<attribute name="ISAT1" value="9.1A"/>
<attribute name="ISAT2" value="22.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370220 "/>
<attribute name="RDC" value="12.5mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74439370330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439370330?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IRP" value="10.8A"/>
<attribute name="ISAT1" value="6.8A"/>
<attribute name="ISAT2" value="18.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439370330 "/>
<attribute name="RDC" value="18mOhm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_8080" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-12&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_8080">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393580068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393580068?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IRP" value="38A"/>
<attribute name="ISAT1" value="26A"/>
<attribute name="ISAT2" value="52.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393580068 "/>
<attribute name="RDC" value="1.41mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74439358010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358010?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IRP" value="30.25A"/>
<attribute name="ISAT1" value="18.15A"/>
<attribute name="ISAT2" value="38.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358010 "/>
<attribute name="RDC" value="2.1mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439358015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358015?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IRP" value="25.1A"/>
<attribute name="ISAT1" value="15A"/>
<attribute name="ISAT2" value="32A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358015 "/>
<attribute name="RDC" value="2.91mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439358022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358022?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IRP" value="21.85A"/>
<attribute name="ISAT1" value="12.55A"/>
<attribute name="ISAT2" value="26.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358022 "/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439358047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IRP" value="13.35A"/>
<attribute name="ISAT1" value="7.5A"/>
<attribute name="ISAT2" value="16.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358047 "/>
<attribute name="RDC" value="8.65mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74439358068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IRP" value="10.55A"/>
<attribute name="ISAT1" value="8.5A"/>
<attribute name="ISAT2" value="17.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358068 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74439358100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358100?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IRP" value="8.5A"/>
<attribute name="ISAT1" value="6.3A"/>
<attribute name="ISAT2" value="13.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358100 "/>
<attribute name="RDC" value="19mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74439358150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439358150?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IRP" value="7.25A"/>
<attribute name="ISAT1" value="5.6A"/>
<attribute name="ISAT2" value="10.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439358150 "/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="SIZE" value=" 8080 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1090" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-12&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_1090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439369015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369015?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IRP" value="40.6A"/>
<attribute name="ISAT1" value="19A"/>
<attribute name="ISAT2" value="38.55A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369015 "/>
<attribute name="RDC" value="1.46mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439369022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369022?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IRP" value="32.05A"/>
<attribute name="ISAT1" value="15.65A"/>
<attribute name="ISAT2" value="32.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369022 "/>
<attribute name="RDC" value="2.2mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439369033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IRP" value="24.95A"/>
<attribute name="ISAT1" value="15.6A"/>
<attribute name="ISAT2" value="34A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369033 "/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439369047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369047?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IRP" value="20A"/>
<attribute name="ISAT1" value="13.6A"/>
<attribute name="ISAT2" value="28.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369047 "/>
<attribute name="RDC" value="5mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74439369056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369056?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IRP" value="18.15A"/>
<attribute name="ISAT1" value="11.1A"/>
<attribute name="ISAT2" value="24.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369056 "/>
<attribute name="RDC" value="5.9mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74439369068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369068?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IRP" value="16.3A"/>
<attribute name="ISAT1" value="10.7A"/>
<attribute name="ISAT2" value="23.25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369068 "/>
<attribute name="RDC" value="7.16mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74439369082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369082?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IRP" value="13.4A"/>
<attribute name="ISAT1" value="9.4A"/>
<attribute name="ISAT2" value="20.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369082 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74439369100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369100?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IRP" value="12.7A"/>
<attribute name="ISAT1" value="9.2A"/>
<attribute name="ISAT2" value="20.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369100 "/>
<attribute name="RDC" value="11mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74439369150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439369150?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IRP" value="10.75A"/>
<attribute name="ISAT1" value="7.2A"/>
<attribute name="ISAT2" value="16.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439369150 "/>
<attribute name="RDC" value="14.8mOhm"/>
<attribute name="SIZE" value=" 1090 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_7070" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_7070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439387033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IRP" value="18.2A"/>
<attribute name="ISAT1" value="8.8A"/>
<attribute name="ISAT2" value="18.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439387033 "/>
<attribute name="RDC" value="6.4mOhm"/>
<attribute name="SIZE" value=" 7070 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439387047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IRP" value="15.0A"/>
<attribute name="ISAT1" value="8A"/>
<attribute name="ISAT2" value="16A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439387047 "/>
<attribute name="RDC" value="9.2mOhm"/>
<attribute name="SIZE" value=" 7070 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74439387056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387056?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IRP" value="14.8A"/>
<attribute name="ISAT1" value="6.9A"/>
<attribute name="ISAT2" value="13.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439387056 "/>
<attribute name="RDC" value="12.4mOhm"/>
<attribute name="SIZE" value=" 7070 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74439387068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387068?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IRP" value="12.5A"/>
<attribute name="ISAT1" value="6.8A"/>
<attribute name="ISAT2" value="13.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439387068 "/>
<attribute name="RDC" value="12.4mOhm"/>
<attribute name="SIZE" value=" 7070 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74439387082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387082?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IRP" value="11.2A"/>
<attribute name="ISAT1" value="6A"/>
<attribute name="ISAT2" value="12.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439387082 "/>
<attribute name="RDC" value="14.5mOhm"/>
<attribute name="SIZE" value=" 7070 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74439387100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439387100?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IRP" value="9.6A"/>
<attribute name="ISAT1" value="5.7A"/>
<attribute name="ISAT2" value="12.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439387100 "/>
<attribute name="RDC" value="19mOhm"/>
<attribute name="SIZE" value=" 7070 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_4030" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393240047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240047?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IRP" value="17.10A"/>
<attribute name="ISAT1" value="9A"/>
<attribute name="ISAT2" value="19.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393240047 "/>
<attribute name="RDC" value="3.9mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744393240064">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240064?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IRP" value="15.20A"/>
<attribute name="ISAT1" value="8.4A"/>
<attribute name="ISAT2" value="17A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393240064 "/>
<attribute name="RDC" value="4.8mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="0.64uH"/>
</technology>
<technology name="_744393240090">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393240090?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IRP" value="14.00A"/>
<attribute name="ISAT1" value="7.3A"/>
<attribute name="ISAT2" value="15.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393240090 "/>
<attribute name="RDC" value="6.1mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="0.9uH"/>
</technology>
<technology name="_74439324010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IRP" value="11.10A"/>
<attribute name="ISAT1" value="5.8A"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439324010 "/>
<attribute name="RDC" value="8.7mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439324012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324012?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IRP" value="10.90A"/>
<attribute name="ISAT1" value="5.6A"/>
<attribute name="ISAT2" value="11.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439324012 "/>
<attribute name="RDC" value="8.9mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74439324015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324015?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IRP" value="10.60A"/>
<attribute name="ISAT1" value="5.4A"/>
<attribute name="ISAT2" value="11.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439324015 "/>
<attribute name="RDC" value="10.1mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439324022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324022?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IRP" value="7.80A"/>
<attribute name="ISAT1" value="4.8A"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439324022 "/>
<attribute name="RDC" value="16.6mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74439324033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324033?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IRP" value="7.10A"/>
<attribute name="ISAT1" value="3.9A"/>
<attribute name="ISAT2" value="8.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439324033 "/>
<attribute name="RDC" value="20.2mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439324047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439324047?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IRP" value="5.30A"/>
<attribute name="ISAT1" value="2.8A"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439324047 "/>
<attribute name="RDC" value="31.3mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_4020" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393230022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230022?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IRP" value="20.00A"/>
<attribute name="ISAT1" value="11A"/>
<attribute name="ISAT2" value="24.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393230022 "/>
<attribute name="RDC" value="3.05mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744393230047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230047?ae"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="IRP" value="14.50A"/>
<attribute name="ISAT1" value="5.6A"/>
<attribute name="ISAT2" value="12.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393230047 "/>
<attribute name="RDC" value="5.25mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744393230056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230056?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IRP" value="12.70A"/>
<attribute name="ISAT1" value="5.5A"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393230056 "/>
<attribute name="RDC" value="6.3mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744393230068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230068?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IRP" value="12.60A"/>
<attribute name="ISAT1" value="5.3A"/>
<attribute name="ISAT2" value="11.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393230068 "/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744393230082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744393230082?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IRP" value="10.80A"/>
<attribute name="ISAT1" value="5.2A"/>
<attribute name="ISAT2" value="11.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744393230082 "/>
<attribute name="RDC" value="9.3mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74439323010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323010?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IRP" value="10.00A"/>
<attribute name="ISAT1" value="4.6A"/>
<attribute name="ISAT2" value="10.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439323010 "/>
<attribute name="RDC" value="10.7mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74439323012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323012?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IRP" value="8.90A"/>
<attribute name="ISAT1" value="3.8A"/>
<attribute name="ISAT2" value="8.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439323012 "/>
<attribute name="RDC" value="12.5mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74439323015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323015?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IRP" value="7.80A"/>
<attribute name="ISAT1" value="3.6A"/>
<attribute name="ISAT2" value="8.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439323015 "/>
<attribute name="RDC" value="16.3mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74439323022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439323022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IRP" value="7.20A"/>
<attribute name="ISAT1" value="3.1A"/>
<attribute name="ISAT2" value="6.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439323022 "/>
<attribute name="RDC" value="20.2mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_4040" prefix="L">
<description>&lt;B&gt;WE-XHMI SMT Power Inductor&lt;br&gt;
&lt;/b&gt;Shielded&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Flat wire coil for low copper losses
&lt;br&gt; Composite core material allows high saturation currents
&lt;br&gt; Compact design
&lt;br&gt; Magnetically shielded
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt; Low leakage flux noise
&lt;br&gt; Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; DC/DC-converter for high current power supplies
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt; Power supplies for mobile devices
&lt;br&gt; POL-converters
&lt;br&gt; Mainboards/ graphic cards
&lt;br&gt; Battery powered devices
&lt;br&gt; Wireless communication devices
&lt;br&gt; Filter

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14900v209%20Family_WE-XHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-XHMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-XHMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-11&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-XHMI_4040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439325033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325033?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IRP" value="7.2A"/>
<attribute name="ISAT1" value="3.7A"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439325033 "/>
<attribute name="RDC" value="20.4mOhm"/>
<attribute name="SIZE" value=" 4040 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74439325047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IRP" value="5.7A"/>
<attribute name="ISAT1" value="2.7A"/>
<attribute name="ISAT2" value="5.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439325047 "/>
<attribute name="RDC" value="26.5mOhm"/>
<attribute name="SIZE" value=" 4040 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74439325056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325056?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IRP" value="5.1A"/>
<attribute name="ISAT1" value="2.4A"/>
<attribute name="ISAT2" value="5.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439325056 "/>
<attribute name="RDC" value="34.2mOhm"/>
<attribute name="SIZE" value=" 4040 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74439325068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74439325068?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IRP" value="4.1A"/>
<attribute name="ISAT1" value="2.2A"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74439325068 "/>
<attribute name="RDC" value="42.3mOhm"/>
<attribute name="SIZE" value=" 4040 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
