<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Input/Output connectors - WR-CRD &lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-11-14&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="693021020811">
<description>&lt;b&gt;WR-CRD Micro SIM Card Connector Push &amp; Push with Card Detection</description>
</package>
<package name="693023010811">
<description>&lt;B&gt;WR-CRD Micro SIM Card Connector Push &amp; Pull with Card Detection</description>
</package>
<package name="693072010801">
<description>&lt;B&gt;WR-CRD Micro SD Card Connector Hinge 8 pins</description>
</package>
<package name="693120025011">
<description>&lt;B&gt;WR-CRD Compact Flash Card Connector Header Reverse type 50 pins</description>
</package>
<package name="693043020611">
<description>&lt;B&gt;WR-CRD Nano SIM Card Connector</description>
</package>
<package name="693010010601">
<description>&lt;B&gt;WR-CRD SIM Card Connector (Mini SIM) Header - 6 pins</description>
</package>
<package name="693120035011">
<description>&lt;B&gt;WR-CRD Compact Flash Card Connector Header Shrouded type 50 pins</description>
</package>
<package name="693061010911">
<description>&lt;B&gt;WR-CRD SD Card Connector Push &amp; Push with Card Detection 9 pins</description>
</package>
<package name="693010020611">
<description>&lt;B&gt;WR-CRD&lt;/B&gt;&lt;BR&gt;SIM Card Connector (Mini SIM) Header Shielded ,6Pins</description>
</package>
<package name="693071010811">
<description>&lt;B&gt;WR-CRD Micro SD Card Connector Push &amp; Push 8 pins</description>
</package>
<package name="693161011911">
<description>&lt;B&gt;WR-CRD SD Card Connector 4.0 Push &amp; Push with Card Detection 19 pins</description>
</package>
<package name="693022010811">
<description>&lt;B&gt;WR-CRD Micro SIM Card Connector Hinge Type</description>
</package>
<package name="693071020811">
<description>&lt;B&gt;WR-CRD Micro SD Card Connector Push &amp; Push 8 pins</description>
</package>
<package name="693063010911">
<description>&lt;B&gt;WR-CRD SD Card Connector Push &amp; Pull with Card Detection 9 pins</description>
</package>
<package name="693071030811">
<description>&lt;B&gt;WR-CRD Micro SD Card Connector Push &amp; Push 8 pins</description>
</package>
<package name="693120015011">
<description>&lt;B&gt;WR-CRD Compact Flash Card Connector Header 50 pins</description>
</package>
<package name="693063020911">
<description>&lt;B&gt;WR-CRD SD Card Connector Push &amp; Pull Short Type with Card Detection 9 pins</description>
</package>
</packages>
<symbols>
<symbol name="693023010811">
<description>Micro SIM Card Connector,9Pins</description>
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="RFU1"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="RFU2"/>
<pin name="DETECT"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="MINI_SIM_CARD_6PINS">
<description>SIM Card Connector (Mini SIM) Header,6Pins</description>
<pin name="VCC"/>
<pin name="RET"/>
<pin name="CLK"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="693021020811">
<description>Micro SD Card,8Pins</description>
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="SHIELD"/>
<pin name="CD"/>
</symbol>
<symbol name="693043020611">
<description>Nano SIM Card,6Pins</description>
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="COMPACT_FLASH_CARD">
<description>Compact Flash Card,50Pins</description>
<pin name="1" direction="pwr"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13" direction="pwr"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38" direction="pwr"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50" direction="pwr"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="693072010801">
<description>Micro SD,8Pins</description>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="VSS"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="693161011911">
<description>SD Card,19Pins</description>
<pin name="VSS3"/>
<pin name="DAT2"/>
<pin name="D0+"/>
<pin name="CD/DAT3"/>
<pin name="D0-"/>
<pin name="CMD"/>
<pin name="CD"/>
<pin name="VSS1"/>
<pin name="VSS4"/>
<pin name="VDD2"/>
<pin name="VDD1"/>
<pin name="D1-"/>
<pin name="CLK"/>
<pin name="D1+"/>
<pin name="VSS2"/>
<pin name="VSS5"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="WP"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="SD_CARD_9PINS">
<description>SD Card ,9Pins</description>
<pin name="DAT3"/>
<pin name="CMD"/>
<pin name="VSS1"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="VSS2"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="CD"/>
<pin name="WP"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="693022010811">
<description>Micro SIM Card ,8Pins</description>
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="RFU1"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="RFU2"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="693071010811">
<description>Micro SD Card,8Pins</description>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="VSS"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="CDSW1"/>
<pin name="CDSW2"/>
</symbol>
<symbol name="693071030811">
<description>Micro SD Card,8Pins</description>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="VSS"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="CDSW1"/>
<pin name="GND"/>
</symbol>
<symbol name="693071020811">
<description>Micro SD Card,8Pins</description>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="VSS"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="CDSW1"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="693023010811" prefix="J">
<description>&lt;b&gt;WR-CRD Micro SIM Card Connector Push &amp; Pull with Card Detection &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:5000 Mating cycles
&lt;br&gt;Gender:Socket
&lt;br&gt;Type:Push &amp; Pull
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1:1 A
&lt;br&gt;Working Voltage:30V (AC)
&lt;/b&gt;Withstanding Voltage:500V (AC)
&lt;br&gt;Contact Resistance:100mΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Stainless Steel
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33065v209%20Family_WR-CRD_Micro_SIM_PushPull_8Pins_693023010811.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33065v209%20Family_WR-CRD_Micro_SIM_PushPull_8Pins_693023010811.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_MICRO_SIM_PUSH_AND_PULL_CRD_DETECTION_8_PINS"&gt;www.we-online.com/en/components/products/CRD_MICRO_SIM_PUSH_AND_PULL_CRD_DETECTION_8_PINS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-27&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="693023010811"/>
</gates>
<devices>
<device name="" package="693023010811">
<connects>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="DETECT" pad="SW"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RFU1" pad="C4"/>
<connect gate="G$1" pin="RFU2" pad="C8"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693023010811?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693023010811"/>
<attribute name="PINS" value="8"/>
<attribute name="TYPE" value="Push &amp; Pull"/>
<attribute name="VALUE" value="693023010811"/>
<attribute name="WORKING-VOLTAGE" value="15V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693072010801" prefix="J">
<description>&lt;b&gt;WR-CRD Micro SD Card Connector Hinge 8 pins
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Gender Socket 
&lt;br&gt;Type Hinge 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Stainless Steel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Working Voltage 100 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 100 mΩ 

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33063v209%20Family_05_SMT_ZIF_Horizontal_p294_WR-FPC_6871xx182122_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33063v209%20Family_05_SMT_ZIF_Horizontal_p294_WR-FPC_6871xx182122_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_SD_MICRO_HINGEL_8_PINS"&gt;www.we-online.com/en/components/products/CRD_SD_MICRO_HINGEL_8_PINS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-04-15&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="693072010801"/>
</gates>
<devices>
<device name="" package="693072010801">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="2"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="3"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4" route="any"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693072010801?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693072010801"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="TYPE" value="Hinge"/>
<attribute name="VALUE" value="693072010801"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693021020811">
<description>&lt;b&gt;WR-CRD Micro SIM Card Connector Push &amp; Push with Card Detection&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Gender Receptacle 
&lt;br&gt;Type Push &amp; Push 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -20 up to +70 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 50 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 100 mΩ 
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Brass 
&lt;br&gt;Contact Plating Gold over Nickel 
&lt;br&gt;Shielding Material Steel 
&lt;br&gt;Shielding Plating Tin 


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o732987v209%20693021020811_Multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o732987v209%20693021020811_Multi-parts.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/MICRO_SIM_CARD_CONNECTOR_PUSH_PUSH_WIH_CARD_DETECTION"&gt;www.we-online.com/en/components/products/MICRO_SIM_CARD_CONNECTOR_PUSH_PUSH_WIH_CARD_DETECTION&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-03-28&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="693021020811"/>
</gates>
<devices>
<device name="" package="693021020811">
<connects>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693120035011?ae"/>
<attribute name="GERDER" value="Receptacle"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693120035011"/>
<attribute name="PINS" value="7"/>
<attribute name="TYPE" value="Push &amp; Push"/>
<attribute name="VALUE" value=" 693021020811 "/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693120025011" prefix="J">
<description>&lt;b&gt;WR-CRD Compact Flash Card Connector Header Reverse type 50 pins
&lt;br&gt;
&lt;br&gt;
Kind Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 10000 Mating cycles
&lt;br&gt;Gender Socket 
&lt;br&gt;Type Header
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C;​ 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color White
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material：Copper Alloy
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties 
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;IR 1：0.5A
&lt;br&gt;Working Voltage 100V (AC)
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 40 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33061v209%20Family_WR-CRD_Compact%20Flash%20Card%20Kartensockel_invertiert_693120025011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33061v209%20Family_WR-CRD_Compact%20Flash%20Card%20Kartensockel_invertiert_693120025011.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_REVERSE_TYPE_50_PINS"&gt;www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_REVERSE_TYPE_50_PINS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMPACT_FLASH_CARD"/>
</gates>
<devices>
<device name="" package="693120025011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693120025011?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693120025011"/>
<attribute name="PINS" value="50"/>
<attribute name="TYPE" value="Header"/>
<attribute name="VALUE" value="693120025011"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693043020611" prefix="J">
<description>&lt;b&gt;WR-CRD Nano SIM Card Connector&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Gender:Socket
&lt;br&gt;Type:Push &amp; Push
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage:15 V (AC)
&lt;br&gt;Withstanding Voltage:500 V (AC)
&lt;br&gt;Contact Resistance:100 mΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type{Stamped
&lt;br&gt;Shielding Material:Stainless Steel
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33068v209%20Family_WR-CRD_Nano_SIM_PushPull_6Pins_693043020611.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33068v209%20Family_WR-CRD_Nano_SIM_PushPull_6Pins_693043020611.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_NANO_SIM_PUSH_AND_PULL"&gt;www.we-online.com/en/components/products/CRD_NANO_SIM_PUSH_AND_PULL&lt;/a&gt;&lt;p&gt;

Created by Yingchun,Shan  2019-11-21&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="693043020611"/>
</gates>
<devices>
<device name="" package="693043020611">
<connects>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4 S5 S6" route="any"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693043020611?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693043020611"/>
<attribute name="PINS" value="6"/>
<attribute name="TYPE" value="Push &amp; Push "/>
<attribute name="VALUE" value="693043020611"/>
<attribute name="WORKING-VOLTAGE" value="15V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693010010601" prefix="J">
<description>&lt;b&gt;WR-CRD SIM Card Connector (Mini SIM) Header - 6 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:5000 Mating cycles
&lt;br&gt;Gender:Socket
&lt;br&gt;Type:Header
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1:0.5A
&lt;br&gt;Working Voltage:50V (AC)
&lt;br&gt;Withstanding Voltage:500V (AC)
&lt;br&gt;Contact Resistance:50mΩ
&lt;br&gt;&lt;b&gt;
&lt;br&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o32835v209%20Family_Speicherkarten%20Sockel_WR-CRD_693010010601.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32835v209%20Family_Speicherkarten%20Sockel_WR-CRD_693010010601.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_MINI_SIM_HEADER_6_PINS"&gt;www.we-online.com/en/components/products/CRD_MINI_SIM_HEADER_6_PINS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-27&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MINI_SIM_CARD_6PINS"/>
</gates>
<devices>
<device name="" package="693010010601">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="I/O" pad="6"/>
<connect gate="G$1" pin="RET" pad="2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693010010601?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693010010601"/>
<attribute name="PINS" value="6"/>
<attribute name="TYPE" value="Header"/>
<attribute name="VALUE" value="693010010601"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693061010911" prefix="J">
<description>&lt;b&gt;WR-CRD SD Card Connector Push &amp; Push with Card Detection&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Gender:Socket
&lt;br&gt;Type:Push &amp; Push
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage:100 V (AC)
&lt;br&gt;Withstanding Voltage:500 V (AC)
&lt;br&gt;Contact Resistance:100 mΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33071v209%20Family_WR-CRD_SD%20Kartensockel_Push%20u.%20Push_693061010911.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33071v209%20Family_WR-CRD_SD%20Kartensockel_Push%20u.%20Push_693061010911.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_SD_PUSH_AND_PUSH_CRD_DETETCION_9_PINS"&gt;www.we-online.com/en/components/products/CRD_SD_PUSH_AND_PUSH_CRD_DETETCION_9_PINS&lt;/a&gt;&lt;p&gt;

Created by Yingchun,Shan  2019-11-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="SD_CARD_9PINS"/>
</gates>
<devices>
<device name="" package="693061010911">
<connects>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="DAT3" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WP" pad="WP"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693061010911?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693061010911"/>
<attribute name="PINS" value="9"/>
<attribute name="TYPE" value="Push &amp; Push"/>
<attribute name="VALUE" value="693061010911"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693010020611" prefix="J">
<description>&lt;b&gt;WR-CRD SIM Card Connector (Mini SIM) Header Shielded - 6 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Gender:Socket
&lt;br&gt;Type:Header
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1:0.5A
&lt;br&gt;Working Voltage:50V (AC)
&lt;br&gt;Withstanding Voltage:500V (AC)
&lt;br&gt;Contact Resistance:50mΩ
&lt;br&gt;
&lt;b&gt;&lt;br&gt;Material Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:elective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Stainless Steel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33072v209%20Family_WR-CRD_SIM%20Kartensockel_geschirmt_693010020611.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33072v209%20Family_WR-CRD_SIM%20Kartensockel_geschirmt_693010020611.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_MINI_SIM_HEADER_SHIELDED_6_PINS"&gt;www.we-online.com/en/components/products/CRD_MINI_SIM_HEADER_SHIELDED_6_PINS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-27&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="MINI_SIM_CARD_6PINS"/>
</gates>
<devices>
<device name="" package="693010020611">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="I/O" pad="7"/>
<connect gate="G$1" pin="RET" pad="2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693010020611?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693010020611"/>
<attribute name="PINS" value="6"/>
<attribute name="TYPE" value="Header"/>
<attribute name="VALUE" value="693010020611"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693071010811" prefix="J">
<description>&lt;b&gt;WR-CRD Micro SD Card Connector Push &amp; Push 8 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Quality Class 10 000 Mating cycles 
&lt;br&gt;Gender Socket 
&lt;br&gt;Type Push &amp; Push 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C; -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Working Voltage 30 V (AC); 100 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 100 mΩ 
&lt;br&gt;Contact Resistance 500 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Color Black 
&lt;br&gt;Cover Material Stainless Steel 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 1 u' on contact area; Selective Gold 
&lt;br&gt;Contact Type Stamped 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttps://www.we-online.com/components/media/o32845v209%20Family_ConCRD_693071010811.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32845v209%20Family_ConCRD_693071010811.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_SD_MICRO_PUSH_AND_PULL_8_PINS"&gt;www.we-online.com/en/components/products/CRD_SD_MICRO_PUSH_AND_PULL_8_PINS&lt;/a&gt;&lt;p&gt;

Created by Yingchun,Shan  2019-11-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="693071010811"/>
</gates>
<devices>
<device name="" package="693071010811">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="2"/>
<connect gate="G$1" pin="CDSW1" pad="9 9-1"/>
<connect gate="G$1" pin="CDSW2" pad="10 10-1"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="3"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693071010811?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693071010811"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="TYPE" value="Push &amp; Push"/>
<attribute name="VALUE" value="693071010811"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693161011911" prefix="J">
<description>&lt;b&gt;WR-CRD SD Card Connector 4.0 Push &amp; Push with Card Detection &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;Kind Properties &lt;/b&gt;
&lt;br&gt;&lt;br&gt;
&lt;br&gt;Gender:Socket
&lt;br&gt;Type:Push &amp; Pull
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-20up to +60 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
&lt;br&gt;Working Voltage:10V (AC)
&lt;br&gt;Withstanding Voltage:500 V (AC)
&lt;br&gt;Contact Resistance:100 mΩ
&lt;br&gt;&lt;b&gt;
&lt;br&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Stainless Steel
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o72612v209%20Family_WR-CRD_693161011911.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o72612v209%20Family_WR-CRD_693161011911.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_SMT_SD_PUSH_AND_PUSH_CARD_DETECTION_19_PINS"&gt;www.we-online.com/en/components/products/CRD_SMT_SD_PUSH_AND_PUSH_CARD_DETECTION_19_PINS&lt;/a&gt;&lt;p&gt;

Created by Yingchun,Shan  2019-11-22&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="693161011911"/>
</gates>
<devices>
<device name="" package="693161011911">
<connects>
<connect gate="G$1" pin="CD" pad="7"/>
<connect gate="G$1" pin="CD/DAT3" pad="4"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="CMD" pad="6"/>
<connect gate="G$1" pin="D0+" pad="3"/>
<connect gate="G$1" pin="D0-" pad="5"/>
<connect gate="G$1" pin="D1+" pad="14"/>
<connect gate="G$1" pin="D1-" pad="12"/>
<connect gate="G$1" pin="DAT0" pad="17"/>
<connect gate="G$1" pin="DAT1" pad="18"/>
<connect gate="G$1" pin="DAT2" pad="2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VDD1" pad="11"/>
<connect gate="G$1" pin="VDD2" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="15"/>
<connect gate="G$1" pin="VSS3" pad="1"/>
<connect gate="G$1" pin="VSS4" pad="9"/>
<connect gate="G$1" pin="VSS5" pad="16"/>
<connect gate="G$1" pin="WP" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693161011911?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693161011911"/>
<attribute name="PINS" value=" 19 "/>
<attribute name="TYPE" value="Push &amp; Push"/>
<attribute name="VALUE" value="693161011911"/>
<attribute name="WORKING-VOLTAGE" value="10V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693120035011" prefix="J">
<description>&lt;b&gt;https://www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_SHROUDED_TYPE_50_PINS
&lt;br&gt;
&lt;br&gt;
Kind Properties 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 10000 Mating cycles
&lt;br&gt;Gender Socket 
&lt;br&gt;Type Shrouded
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C;​ 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color White
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;IR 1：0.5A
&lt;br&gt;Working Voltage 100V (AC)
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 40 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33062v214%20Family_I-O_COM_CRD_Compact-Flash_693120035011_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33062v214%20Family_I-O_COM_CRD_Compact-Flash_693120035011_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_SHROUDED_TYPE_50_PINS"&gt;www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_SHROUDED_TYPE_50_PINS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMPACT_FLASH_CARD"/>
</gates>
<devices>
<device name="" package="693120035011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693120035011?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693120035011"/>
<attribute name="PINS" value="50"/>
<attribute name="TYPE" value="Shrouded "/>
<attribute name="VALUE" value="693120035011"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693022010811" prefix="J">
<description>&lt;b&gt;WR-CRD Micro SIM Card Connector Hinge Type &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:2 500 Mating cycles
&lt;br&gt;Gender:Socket
&lt;br&gt;Type:Hinge
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR 1:1 A
&lt;br&gt;Working Voltage:15 V (AC)
&lt;br&gt;Withstanding Voltage:500 V (AC)
&lt;br&gt;Contact Resistance:30mΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Stainless Steel
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33064v209%20Family_WR-CRD_Micro_SIM_Hinge_8Pins_693022010811.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33064v209%20Family_WR-CRD_Micro_SIM_Hinge_8Pins_693022010811.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_MICRO_SIM"&gt;www.we-online.com/en/components/products/CRD_MICRO_SIM&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-05-27&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="693022010811"/>
</gates>
<devices>
<device name="" package="693022010811">
<connects>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RFU1" pad="C4"/>
<connect gate="G$1" pin="RFU2" pad="C8"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693022010811?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693022010811"/>
<attribute name="PINS" value="8"/>
<attribute name="TYPE" value="Hinge"/>
<attribute name="VALUE" value="693022010811"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693063010911" prefix="J">
<description>&lt;b&gt;WR-CRD SD Card Connector Push &amp; Pull with Card Detection 9 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;

&lt;b&gt;General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature	-25 °C up to +85 °C
&lt;br&gt;Gender	Socket
&lt;br&gt;Type	Push &amp; Pull
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-25 up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Working Voltage	100 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	100 mΩ
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Material Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Insulator Material	LCP
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;Shielding Material	Copper Alloy
&lt;br&gt;Shielding Plating	Nickel (Ni)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o70346v209%20Family_WR-CRD_SD_Normal_693063010911_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o70346v209%20Family_WR-CRD_SD_Normal_693063010911_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/CRD_SD_PUSH_AND_PULL_CRD_DETETCION_9_PINS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/CRD_SD_PUSH_AND_PULL_CRD_DETETCION_9_PINS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="SD_CARD_9PINS"/>
</gates>
<devices>
<device name="" package="693063010911">
<connects>
<connect gate="G$1" pin="CD" pad="10"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="DAT3" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WP" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693063010911?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693063010911"/>
<attribute name="PINS" value="9"/>
<attribute name="TYPE" value="Push &amp; Pull"/>
<attribute name="VALUE" value="693063010911"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693071020811" prefix="J">
<description>&lt;b&gt;WR-CRD Micro SD Card Connector Push &amp; Push 8 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Quality Class 10 000 Mating cycles 
&lt;br&gt;Gender Socket 
&lt;br&gt;Type Push &amp; Push 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C; -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Working Voltage 30 V (AC); 100 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 100 mΩ 
&lt;br&gt;Contact Resistance 500 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Color Black 
&lt;br&gt;Cover Material Stainless Steel 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 1 u' on contact area; Selective Gold 
&lt;br&gt;Contact Type Stamped 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttps://www.we-online.com/components/media/o32845v209%20Family_ConCRD_693071010811.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32845v209%20Family_ConCRD_693071010811.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_SD_MICRO_PUSH_AND_PULL_8_PINS"&gt;www.we-online.com/en/components/products/CRD_SD_MICRO_PUSH_AND_PULL_8_PINS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-04-15&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="693071020811"/>
</gates>
<devices>
<device name="" package="693071020811">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="2"/>
<connect gate="G$1" pin="CDSW1" pad="9"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="3"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="GND" pad="10 11 12 13"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693071020811?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693071020811"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="TYPE" value="Push &amp; Push"/>
<attribute name="VALUE" value="693071020811"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693071030811" prefix="J">
<description>&lt;b&gt;WR-CRD Micro SD Card Connector Push &amp; Push 8 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Quality Class 10 000 Mating cycles 
&lt;br&gt;Gender Socket 
&lt;br&gt;Type Push &amp; Push 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C; -40 up to +85 °C 
&lt;br&gt;Compliance RoHS 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Working Voltage 30 V (AC); 100 V (AC) 
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 100 mΩ 
&lt;br&gt;Contact Resistance 500 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Color Black 
&lt;br&gt;Cover Material Stainless Steel 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 1 u' on contact area; Selective Gold 
&lt;br&gt;Contact Type Stamped 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttps://www.we-online.com/components/media/o32845v209%20Family_ConCRD_693071010811.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o32845v209%20Family_ConCRD_693071010811.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_SD_MICRO_PUSH_AND_PULL_8_PINS"&gt;www.we-online.com/en/components/products/CRD_SD_MICRO_PUSH_AND_PULL_8_PINS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2020-04-15&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="693071030811"/>
</gates>
<devices>
<device name="" package="693071030811">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="2"/>
<connect gate="G$1" pin="CDSW1" pad="9"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="3"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="GND" pad="10 11-1 11-3 11-4 11-5 11-6 11-7 11-8 11-9 11-10"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693071030811?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693071030811"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="TYPE" value="Push &amp; Push"/>
<attribute name="VALUE" value="693071030811"/>
<attribute name="WORKING-VOLTAGE" value="30V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693120015011" prefix="J">
<description>&lt;b&gt;WR-CRD Compact Flash Card Connector Header 50 pins
&lt;br&gt;
&lt;br&gt;
Kind Properties 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class 5 000 Mating cycles
&lt;br&gt;Gender Socket 
&lt;br&gt;Type Header
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -25 up to +85 °C;​ 
&lt;br&gt;Compliance RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Color White
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold;​ 
&lt;br&gt;Contact Type Stamped  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;IR 1：0.5A
&lt;br&gt;Working Voltage 50V (AC)
&lt;br&gt;Withstanding Voltage 500 V (AC) 
&lt;br&gt;Contact Resistance 50 mΩ 
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33060v209%20Family_WR-CRD_Compact%20Flash%20Card%20Kartensockel_693120015011.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33060v209%20Family_WR-CRD_Compact%20Flash%20Card%20Kartensockel_693120015011.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Details see: &lt;a href="https://www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_50_PINS"&gt;https://www.we-online.com/en/components/products/CRD_COMPACT_FLASH_HEADER_50_PINS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-11-25&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="COMPACT_FLASH_CARD"/>
</gates>
<devices>
<device name="" package="693120015011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693120015011?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693120015011"/>
<attribute name="PINS" value="50"/>
<attribute name="TYPE" value="Header"/>
<attribute name="VALUE" value="693120015011"/>
<attribute name="WORKING-VOLTAGE" value="50V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="693063020911" prefix="J">
<description>&lt;b&gt;WR-CRD SD Card Connector Push &amp; Pull Short Type with Card Detection 9 pins&lt;br&gt; &lt;/b&gt;
&lt;br&gt;

&lt;b&gt;General Information&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature	-25 °C up to +85 °C
&lt;br&gt;Gender	Socket
&lt;br&gt;Type	Push &amp; Pull
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage	100 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	100 mΩ
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;b&gt;Material Properties&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Insulator Material	PA9T
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;Shielding Material	Copper Alloy
&lt;br&gt;Shielding Plating	Nickel (Ni)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33070v209%20Family_WR-CRD_SD%20Kartensockel_Push%20u.%20Pull_kurz_693063020911.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33070v209%20Family_WR-CRD_SD%20Kartensockel_Push%20u.%20Pull_kurz_693063020911.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/CRD_SD_PUSH_AND_PULL_CRD_DETETCION_SHORT_TYPE_9_PINS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/CRD_SD_PUSH_AND_PULL_CRD_DETETCION_SHORT_TYPE_9_PINS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="SD_CARD_9PINS"/>
</gates>
<devices>
<device name="" package="693063020911">
<connects>
<connect gate="G$1" pin="CD" pad="10"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="DAT3" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WP" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/693063020911?ae"/>
<attribute name="GERDER" value="Socket"/>
<attribute name="IR" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="693063020911"/>
<attribute name="PINS" value="9"/>
<attribute name="TYPE" value="Push &amp; Pull"/>
<attribute name="VALUE" value="693063020911"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
