<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Input/Output connectors - WR-MJ &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023b, 2023-11-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="615006144121">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Vertical Plastic 6PxC Modular Jack With Ear,6 pins</description>
</package>
<package name="615002138421">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 6PxC Tab Up,2 Pins</description>
</package>
<package name="634008137221">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Modular Jack SMT Horizontal Plastic 8P8C Tab Down,8 Pins</description>
</package>
<package name="615024143921">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Horizontal Plastic 4 Port 6P6C Modular Jack Tab Up, 24 pins</description>
</package>
<package name="615008185221">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Horizontal Shielded w. LED and EMI Panel Finger 8P8C Tab Down ,8Pins</description>
</package>
<package name="615008142521">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack 45° Plastic 8P8C</description>
</package>
<package name="615008138321">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Vertical Shielded 8P8C w. LED, 8 pins</description>
</package>
<package name="615008149521M">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Assembly Tab Up</description>
</package>
<package name="615006141121">
<description>&lt;b&gt;WR-MJ&lt;/b&gt; &lt;br&gt;Horizontal Plastic 6P6C Modular Jack Tab Down, 6 Pins</description>
</package>
<package name="615008160121">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack THT Horizontal Shielded 8P8C Tab Up</description>
</package>
<package name="615008137121">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Horizontal Plastic 8P8C Modular Jack Tab Down, 8 Pins</description>
</package>
<package name="615008145121">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Modular Jack 45° Entry Shielded 8P8C Standard &amp; Reverse Metal Post Trail, 8 pins</description>
</package>
<package name="615006143421">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Horizontal 6P6C Half Shielded Modular Jack Tab Down, 6 Pins</description>
</package>
<package name="615016245421">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Shielded Dual Stacked w. LED and EMI Panel Finger 8P8C Tab Up&amp;Down,16 Pins</description>
</package>
<package name="615008149521R">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Assembly Tab Up</description>
</package>
<package name="615008143721">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Horizontal Plastic 8P8C Tab Down, 8 Pins</description>
</package>
<package name="615006138521">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Vertical Plastic 6P6C w. Ears, 8 pins</description>
</package>
<package name="634008138121">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack SMT Vertical Plastic 8P8C ,8 pins</description>
</package>
<package name="615008143521">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Half Shielded 8P8C Tab Down , 8 Pins</description>
</package>
<package name="615008144221">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Vertical Plastic 8P8C w. Ears, 8 pins</description>
</package>
<package name="615032149521">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Assembly Tab Up</description>
</package>
<package name="615004144121">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Vertical Plastic 6PxC w. Ears , 4 pins</description>
</package>
<package name="615024149521">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Assembly Tab Up</description>
</package>
<package name="615006138421">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Horizontal Plastic 6P6C Modular Jack Tab Up, 6 Pins</description>
</package>
<package name="634108185321">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack Vertical Shielded SMT w. Solder Tab 8P8C Top Entry</description>
</package>
<package name="615016149521">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Assembly Tab Up</description>
</package>
<package name="615024149421">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 6P6C Assembly Tab Up</description>
</package>
<package name="634008149721">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded SMT with EMI Panel Finger 8P8C</description>
</package>
<package name="634108185421">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded SMT 8P8C Tab Down</description>
</package>
<package name="615008160221">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Modular Jack THT Horizontal Shielded EMI 8P8C</description>
</package>
<package name="615008140421">
<description>&lt;b&gt;WR-MJ&lt;/b&gt; &lt;br&gt;Vertical Shielded 8P8C Rear Post Modular Jack, 8 pins</description>
</package>
<package name="615008160521">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack THT Vertical Shielded EMI 8P8C</description>
</package>
<package name="615008160321">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Modular Jack THT Vertical Plastic 8P8C</description>
</package>
<package name="615016137621">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Horizontal Shielded Dual Port 8P8C Modular Jack Tab Down, 16 Pins</description>
</package>
<package name="615032137821">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Horizontal Shielded Ganged 4 Ports 8P8C Modular Jack Tab Down, 32 Pins</description>
</package>
<package name="615008140621">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack Horizontal Shielded w. EMI Panel Finger 8P8C Tab Up</description>
</package>
<package name="615004143821">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack Horizontal Plastic 4P4C Tab Up, 4 Pins</description>
</package>
<package name="615008160421">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack THT Vertical Shielded 8P8C,8Pins</description>
</package>
<package name="615016240521">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Horizontal Shielded Dual Stacked Port with EMI Panel Finger 8P8C Modular Jack Tab Up &amp; Down, 16 Pins</description>
</package>
<package name="615012143921">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack THT Horizontal Plastic Dual Port 6P6C Tab Up,12Pins</description>
</package>
<package name="615008140121">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Front Grounding Post 8P8C Tab Down
&lt;/b&gt;&lt;br&gt;&lt;br&gt;THT, 8 pins</description>
</package>
<package name="615008160721">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack THT 47,5° Shielded 8P8C</description>
</package>
<package name="615004141121">
<description>&lt;b&gt;WR-MJ&lt;/b&gt; &lt;br&gt;Horizontal Plastic 6P4C Modular Jack Tab Down, 4 Pins</description>
</package>
<package name="61500814221">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded 8P8C Tab Down, 8 Pins</description>
</package>
<package name="634108185521">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack SMT Horizontal Plastic 8P8C Tab Down</description>
</package>
<package name="615004144021">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Vertical Plastic 4P4C w. Ears,4Pins</description>
</package>
<package name="615096243321">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Horizontal Shielded 2 x 6 Stacked Port with EMI Panel Finger 8P8C Modular Jack Tab Up &amp; Down, 96 Pins</description>
</package>
<package name="615032137921">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Horizontal Shielded Ganged 4 Ports w. LED and EMI Panel Finger 8P8C Tab Up, 32 Pins</description>
</package>
<package name="615016137721">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Horizontal Shielded Dual Port w. EMI Panel Finger 8P8C Tab Up,16 Pins</description>
</package>
<package name="615008142121">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Tab Up, 8 Pins</description>
</package>
<package name="615018149421">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 6P6C Assembly Tab Up</description>
</package>
<package name="615006149421L">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 6P6C Assembly Tab Up</description>
</package>
<package name="615006143221">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded 6P6C Tab Up</description>
</package>
<package name="615008150121">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack THT Horizontal Mid-Mount Plastic Tab Up with LED Y/G</description>
</package>
<package name="615008160621">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack THT 47,5° 8P8C</description>
</package>
<package name="615008185121">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Horizontal Shielded Low Profile w. LED 8P8C Tab Up</description>
</package>
<package name="634008149821">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded SMT 8P8C Tab Up</description>
</package>
<package name="615008141321">
<description>&lt;b&gt;WR-MJ &lt;/b&gt;&lt;br&gt;Modular Jack Tab Up ,8 pins</description>
</package>
<package name="615108150221R">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack THR Horizontal Mid-Mount Shielded Tab Down</description>
</package>
<package name="615008137421">
<description>&lt;B&gt;WR-MJ Modular Jack Tab Up
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;THT,8Pins</description>
</package>
<package name="634008137521">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded SMT w. LED and EMI Panel Finger 8P8C Tab Up</description>
</package>
<package name="634108149621">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack SMT Vertical Plastic 8P8C Top Entry</description>
</package>
<package name="615008145221">
<description>&lt;B&gt;WR-MJ&lt;/B&gt; &lt;BR&gt;Modular Jack 45° Entry Shielded 8P8C Standard &amp; Reverse Metal Post Trail, 8 pins</description>
</package>
<package name="615006149421R">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack Horizontal Plastic 6P6C Assembly Tab Up &lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="615008160021">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack THT Horizontal Plastic 8P8C Tab Up</description>
</package>
<package name="615012149421">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 6P6C Assembly Tab Up</description>
</package>
<package name="615008142621">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Rear Grounding Post 8P8C Tab Down
&lt;/b&gt;&lt;br&gt; &lt;br&gt; THT, 8 Pins</description>
</package>
<package name="634104149621">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack SMT Vertical Plastic 4P4C Top Entry</description>
</package>
<package name="615004138421">
<description>WR-MJ Horizontal Plastic 6P4C Modular Jack Tab Up, 4 Pins</description>
</package>
<package name="615008149521L">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Assembly Tab Up</description>
</package>
<package name="615064243321">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Modular Jack Horizontal Shielded 2x 4 Stacked w. EMI Panel Finger 8P8C Tab Up&amp;Down, 64 Pins</description>
</package>
<package name="634106149621">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack SMT Vertical Plastic 6P6C Top Entry</description>
</package>
<package name="634108150321">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack SMT Horizontal Mid-Mount Shielded Tab Up</description>
</package>
<package name="615008145521">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt; Modular Jack Horizontal Shielded w. EMI Panel Finger 8P8C CAT 5e Tab Down ,8 Pins</description>
</package>
<package name="615006143621">
<description>&lt;b&gt;WR-MJ&lt;/b&gt;&lt;br&gt;Horizontal Plastic 6P6C Modular Jack Tab Down, 6 Pins</description>
</package>
<package name="615006149421M">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 6P6C Assembly Tab Up</description>
</package>
<package name="615032243321">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Horizontal Shielded 2 x Dual Stacked Port with EMI Panel Finger 8P8C M. Jack Tab Up &amp; Down, 32 Pins</description>
</package>
<package name="615008138221">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Shielded 8P8C Front Post
&lt;/b&gt;&lt;br&gt; &lt;br&gt;THT, 8 pins</description>
</package>
<package name="615008148521">
<description>&lt;b&gt;WR-MJ&lt;/B&gt;&lt;BR&gt;Modular Jack Horizontal Plastic 8P8C Tab Up</description>
</package>
<package name="615108137421R">
<description>&lt;B&gt;WR-MJ &lt;/B&gt;&lt;BR&gt;Modular Jack THR Horizontal Shielded w. LED and EMI Finger 8P8C Tab Up</description>
</package>
<package name="615008150021">
<description>&lt;B&gt;WR-MJ&lt;/B&gt;&lt;BR&gt; Modular Jack THT Horizontal Mid-Mount Plastic Tab Up</description>
</package>
<package name="615008138021">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 8P8C
&lt;/b&gt;&lt;br&gt;&lt;br&gt; THT, 8 pins</description>
</package>
</packages>
<symbols>
<symbol name="6P2C">
<description>6P2C</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="8P8C_2">
<description>8P8C</description>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="6P6C">
<description>6P6C</description>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="8P8C_S_LEDYG">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_S">
<description>8P8C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="6P6C_S">
<description>6P6C</description>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="6P4C">
<description>6P4C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="8P8C_S1">
<description>8p8c</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="8P8C_S_2LEDYG">
<description>8P8C with LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="G+Y-_1" direction="pas"/>
<pin name="G-Y+_1" direction="pas"/>
<pin name="G+Y-_2" direction="pas"/>
<pin name="G-Y+_2" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="8P8C_LEDYG">
<description>8P8C With LED</description>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="6P4C_S">
<description>4P4C</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="SHILED" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="615002138421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6PxC Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33138v209%20Family_WR-MJ_61500x138421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33138v209%20Family_WR-MJ_61500x138421.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P2C"/>
</gates>
<devices>
<device name="" package="615002138421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615002138421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615002138421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615002138421"/>
<attribute name="XPXC" value="6P2C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008137221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack SMT Horizontal Plastic 8P8C Tab Down&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;&lt;/b&gt;Quality Class:500 Mating cycles
&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;Withstanding Voltage:1000 V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Cover Material:Bronze
&lt;br&gt;Cover Plating:Nickel
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating: Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60735v209%20Family_I-O_MJ-H_Plastic_Down_634008137221_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60735v209%20Family_I-O_MJ-H_Plastic_Down_634008137221_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_PLASTIC_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_PLASTIC_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-03&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="634008137221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634008137221?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634008137221"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="634008137221"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008185221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded w. LED and EMI Panel Finger 8P8C Tab Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:750 Mating cycles
&lt;br&gt;LED:yellow-green
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:Lead free / RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 125 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:30mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;Qty. 70
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106787v209%20Family_WR-MJ_615008185221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106787v209%20Family_WR-MJ_615008185221.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2020-01-02&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008185221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008185221?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008185221"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008185221"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615024143921" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Plastic 4Port 6P6C Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33144v209%20Family_WR-MJ_615024143921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33144v209%20Family_WR-MJ_615024143921.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_PLASTIC_4_PORT_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_PLASTIC_4_PORT_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C"/>
<gate name="B" symbol="6P6C"/>
<gate name="C" symbol="6P6C"/>
<gate name="D" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615024143921">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615024143921?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615024143921"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615024143921"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008138321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded SMT w. LED and EMI Panel Finger 8P8C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;LED yellow-green 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 120 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 500 MΩ 

&lt;br&gt;&lt;b&gt;
&lt;br&gt;Material Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Bronze 
&lt;br&gt;Shielding Plating Nickel (Ni) 
&lt;br&gt;

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Packaging Tray 
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33126v209%20Family_WR-MJ_615008138321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33126v209%20Family_WR-MJ_615008138321.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_VERTICAL_SHIELDED_8P8C_W_LED/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MJ_VERTICAL_SHIELDED_8P8C_W_LED&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-06-27&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008138321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008138321?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008138321"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008138321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006144121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 6PxC w. Ears &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
Kind Properties
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60666v209%20WR-MJ_61500x144121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60666v209%20WR-MJ_61500x144121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_6PXC_W_EARS/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_6PXC_W_EARS/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006144121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006144121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006144121"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615006144121"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008142521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack 45° Plastic 8P8C  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:White
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33130v209%20Family_WR-MJ_615008142521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33130v209%20Family_WR-MJ_615008142521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_45-DEGREE_PLASTIC_8P8C/"&gt;https://www.we-online.com/catalog/en/MJ_45-DEGREE_PLASTIC_8P8C/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008142521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008142521?ae"/>
<attribute name="LED" value="/"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008142521"/>
<attribute name="TYPE" value="45° "/>
<attribute name="VALUE" value="615008142521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008149521M" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008149521M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008149521M?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008149521M"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008149521M"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Shielded 8P8C Tab Up
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact plating 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 125 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161615v209%20Family_WR-MJTH_615008160121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161615v209%20Family_WR-MJTH_615008160121.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_HORIZONTAL_SHIELDED_8P8C_TAB_UP"&gt;https://katalog.we-online.com/en/em/MJ_THT_HORIZONTAL_SHIELDED_8P8C_TAB_UP&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Yingchun,Shan 2020-01-03&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008160121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006141121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6PxC Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33139v209%20Family_WR-MJ_61500x141121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33139v209%20Family_WR-MJ_61500x141121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006141121">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006141121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006141121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006141121"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008137121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Plastic 8P8C Tab Down   &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60728v209%20Family_I_O_MJ-H_Plastic_Down_615008137121_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60728v209%20Family_I_O_MJ-H_Plastic_Down_615008137121_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_PLASTIC_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_PLASTIC_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008137121">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008137121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008137121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008137121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008145121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack 45° Entry Shielded 8P8C Standard &amp; Reverse Metal Post Trail&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator Material PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Bronze 
&lt;br&gt;Shielding Plating Nickel (Ni) 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 120 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 500 MΩ 
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Packaging Tray 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33136v209%20Family_WR-MJ_615008145x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33136v209%20Family_WR-MJ_615008145x21.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_45-DEGREE_ENTRY_SHIELDED_8P8C_STANDARD_REVERSE_METAL_POST_TAIL_615008145X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/MJ_45-DEGREE_ENTRY_SHIELDED_8P8C_STANDARD_REVERSE_METAL_POST_TAIL_615008145X21&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-06-27&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008145121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008145121?ae"/>
<attribute name="LED" value="/"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008145121"/>
<attribute name="TYPE" value="45° "/>
<attribute name="VALUE" value="615008145121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006143421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Half Shielded 6P6C Tab Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33120v209%20Family_WR-MJ_615006143421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33120v209%20Family_WR-MJ_615006143421.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_HALF_SHIELDED_6P6C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_HALF_SHIELDED_6P6C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-03&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006143421">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006143421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006143421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006143421"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016245421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Dual Stacked w. LED and EMI Panel Finger 8P8C Tab Up&amp;Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;LED:yellow-green
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120 V (AC)
&lt;br&gt;Withstanding Voltage:1000 V (AC)
&lt;br&gt;Contact Resistance:20 mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33143v209%20Family_WR-MJ_615016245421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33143v209%20Family_WR-MJ_615016245421.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_STACKED_PORT_W_LED_AND_EMI_FINGER_8P8C_TAB_UP_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_STACKED_PORT_W_LED_AND_EMI_FINGER_8P8C_TAB_UP_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-12-08&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_LEDYG"/>
<gate name="B" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615016245421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+" pad="A11"/>
<connect gate="A" pin="G-" pad="A12"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="A" pin="Y+" pad="A9"/>
<connect gate="A" pin="Y-" pad="A10"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+" pad="B11"/>
<connect gate="B" pin="G-" pad="B12"/>
<connect gate="B" pin="SHIELD" pad="S3 S4"/>
<connect gate="B" pin="Y+" pad="B9"/>
<connect gate="B" pin="Y-" pad="B10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615016245421?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615016245421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615016245421"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008149521R" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008149521R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008149521R?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008149521R"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008149521R"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008143721" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Tab Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33133v209%20Family_WR-MJ_615008143721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33133v209%20Family_WR-MJ_615008143721.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008143721">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008143721?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008143721"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008143721"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008138121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack SMT Vertical Plastic 8P8C &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
Kind Properties
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60707v209%20Family_WR-MJ_634008138121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60707v209%20Family_WR-MJ_634008138121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_8P8C/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_8P8C_W_EARS/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="634008138121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634008138121?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634008138121"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="634008138121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008144221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 8P8C w. Ears  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
Kind Properties
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33134v209%20Family_WR-MJ_615008144221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33134v209%20Family_WR-MJ_615008144221.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_8P8C_W_EARS/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_8P8C_W_EARS/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2020-06-30&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008144221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008144221?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008144221"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008144221"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006138521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 6P6C w. Ears &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
Kind Properties
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33118v209%20Family_WR-MJ_615006138521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33118v209%20Family_WR-MJ_615006138521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_6P6C_W_EARS/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_6P6C_W_EARS/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006138521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006138521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006138521"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615006138521"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008143521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Half Shielded 8P8C Tab Down&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33132v209%20Family_WR-MJ_615008143521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33132v209%20Family_WR-MJ_615008143521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_HALF_SHIELDED_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_HALF_SHIELDED_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2020-01-03&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008143521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008143521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008143521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008143521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004144121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 6PxC w. Ears &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
Kind Properties
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60666v209%20WR-MJ_61500x144121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60666v209%20WR-MJ_61500x144121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_6PXC_W_EARS/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_6PXC_W_EARS/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004144121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615004144121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615004144121"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615004144121"/>
<attribute name="XPXC" value="6P4C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032149521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_2"/>
<gate name="C" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615032149521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615032149521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615032149521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615032149521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108185321" prefix="J">
<description>&lt;b&gt;Modular Jack Vertical Shielded SMT with Solder Tab 8P8C Top Entry WR-MJ&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Quality Class 750 Mating cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Brass 
&lt;br&gt;Shielding Plating Nickel 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;GENERAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;Operating Temperature -40 °C up to +85 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES:&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Working Voltage:125 V (AC)
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 30 mΩ 
&lt;br&gt;Insulation Resistance 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES:&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Packaging Tape and Reel &amp; Mylar 
&lt;br&gt;Packaging Unit (Qty.) 150 mm 
&lt;br&gt;
&lt;br&gt;
&lt;a href="https://www.we-online.com/catalog/media/o106788v209%20Family_WR-MJ_634108185321.jpg" title="Enlarge picture"&gt;

&lt;img src="https://www.we-online.com/catalog/media/o106788v209%20Family_WR-MJ_634108185321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt; Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_SHIELDED_SMT_W_SOLDER_TAB_8P8C_TOP_ENTRY/"&gt; https://www.we-online.com/catalog/en/MJ_VERTICAL_SHIELDED_SMT_W_SOLDER_TAB_8P8C_TOP_ENTRY/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Yingchun Shan,2020-01-07&lt;br&gt;
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108185321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634108185321?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634108185321"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="634108185321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006138421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6PxC Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33138v209%20Family_WR-MJ_61500x138421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33138v209%20Family_WR-MJ_61500x138421.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006138421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006138421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006138421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006138421"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016149521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615016149521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615016149521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615016149521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615016149521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615024149521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615024149521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615024149521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615024149521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615024149521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615024149421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C_S"/>
<gate name="D" symbol="6P6C_S"/>
<gate name="B" symbol="6P6C"/>
<gate name="C" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615024149421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615024149421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615024149421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615024149421"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008149721" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded SMT with EMI Panel Finger 8P8C&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PA9T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Cover Material Bronze
&lt;br&gt;Cover Plating Nickel
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60684v209%20Family_WR-MJ_Horizontal_Shielded_634008149721_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60684v209%20Family_WR-MJ_Horizontal_Shielded_634008149721_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_SHIELDED_W_EMI_PANEL_FINGER_8P8C/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_SHIELDED_W_EMI_PANEL_FINGER_8P8C/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634008149721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634008149721?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634008149721"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="634008149721"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108185421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded SMT 8P8C Tab Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:750 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:Lead free / RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;br&gt;Working Voltage:125 V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:35 mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PA9T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tape and Reel
&lt;br&gt;Qty.:150

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106789v209%20Family_WR-MJ_634108185421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106789v209%20Family_WR-MJ_634108185421.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_SMT_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_SMT_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108185421">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634108185421?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634108185421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="634108185421"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008140421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Shielded 8P8C Rear Post &lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;&lt;br&gt;

&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MATERIAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material :PBT
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating: Nickel 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;GENERAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;Operating Temperature -40 °C up to +85 °C 
&lt;br&gt;Compliance : RoHS 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;ELECTRICAL PROPERTIES:&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Rated Current :1.5 A 
&lt;br&gt;Working Voltage:120 V (AC)
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;Insulation Resistance 500 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES:&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;
&lt;a href="https://www.we-online.com/catalog/media/o33128v209%20Family_WR-MJ_615008140421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33128v209%20Family_WR-MJ_615008140421.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt; Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_SHIELDED_8P8C_REAR_POST/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_SHIELDED_8P8C_REAR_POST/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by Yingchun Shan,2020-01-07&lt;br&gt;
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008140421">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008140421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008140421"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008140421"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Shielded EMI 8P8C
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact plating 
&lt;br&gt;Contact Type Wired 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161617v209%20Family_WR-MJTH_615008160221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161617v209%20Family_WR-MJTH_615008160221.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_HORIZONTAL_SHIELDED_8P8C_EMI"&gt;https://katalog.we-online.com/en/em/MJ_THT_HORIZONTAL_SHIELDED_8P8C_EMI&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Yingchun Shan 2020-01-03&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160221?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160221"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008160221"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Vertical Plastic 8P8C
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact area 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 125 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161619v209%20Family_WR-MJTH_615008160321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161619v209%20Family_WR-MJTH_615008160321.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_VERTICAL_PLASTIC_8P8C"&gt;https://katalog.we-online.com/en/em/MJ_THT_VERTICAL_PLASTIC_8P8C&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-11-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008160321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160321?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160321"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008160321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016137621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Dual Port 8P8C Tab Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 120V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33140v209%20Family_WR-MJ_615016137621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33140v209%20Family_WR-MJ_615016137621.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_PORT_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_PORT_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;
Updated by Yingchun,Shan  2020-01-02&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615016137621">
<connects>
<connect gate="A" pin="1" pad="A8"/>
<connect gate="A" pin="2" pad="A7"/>
<connect gate="A" pin="3" pad="A6"/>
<connect gate="A" pin="4" pad="A5"/>
<connect gate="A" pin="5" pad="A4"/>
<connect gate="A" pin="6" pad="A3"/>
<connect gate="A" pin="7" pad="A2"/>
<connect gate="A" pin="8" pad="A1"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="B" pin="1" pad="B8"/>
<connect gate="B" pin="2" pad="B7"/>
<connect gate="B" pin="3" pad="B6"/>
<connect gate="B" pin="4" pad="B5"/>
<connect gate="B" pin="5" pad="B4"/>
<connect gate="B" pin="6" pad="B3"/>
<connect gate="B" pin="7" pad="B2"/>
<connect gate="B" pin="8" pad="B1"/>
<connect gate="B" pin="SHIELD" pad="S3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615016137621?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615016137621"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615016137621"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032137821" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Ganged 4 Ports 8P8C Tab Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 120V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33145v209%20Family_WR-MJ_615032137821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33145v209%20Family_WR-MJ_615032137821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_GANGED_4_PORTS_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_GANGED_4_PORTS_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2020-01-02&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S1"/>
</gates>
<devices>
<device name="" package="615032137821">
<connects>
<connect gate="A" pin="1" pad="A8"/>
<connect gate="A" pin="2" pad="A7"/>
<connect gate="A" pin="3" pad="A6"/>
<connect gate="A" pin="4" pad="A5"/>
<connect gate="A" pin="5" pad="A4"/>
<connect gate="A" pin="6" pad="A3"/>
<connect gate="A" pin="7" pad="A2"/>
<connect gate="A" pin="8" pad="A1"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B8"/>
<connect gate="B" pin="2" pad="B7"/>
<connect gate="B" pin="3" pad="B6"/>
<connect gate="B" pin="4" pad="B5"/>
<connect gate="B" pin="5" pad="B4"/>
<connect gate="B" pin="6" pad="B3"/>
<connect gate="B" pin="7" pad="B2"/>
<connect gate="B" pin="8" pad="B1"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
<connect gate="C" pin="1" pad="C8"/>
<connect gate="C" pin="2" pad="C7"/>
<connect gate="C" pin="3" pad="C6"/>
<connect gate="C" pin="4" pad="C5"/>
<connect gate="C" pin="5" pad="C4"/>
<connect gate="C" pin="6" pad="C3"/>
<connect gate="C" pin="7" pad="C2"/>
<connect gate="C" pin="8" pad="C1"/>
<connect gate="D" pin="1" pad="D8"/>
<connect gate="D" pin="2" pad="D7"/>
<connect gate="D" pin="3" pad="D6"/>
<connect gate="D" pin="4" pad="D5"/>
<connect gate="D" pin="5" pad="D4"/>
<connect gate="D" pin="6" pad="D3"/>
<connect gate="D" pin="7" pad="D2"/>
<connect gate="D" pin="8" pad="D1"/>
<connect gate="D" pin="SHIELD" pad="S3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615032137821?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615032137821"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615032137821"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008140621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded w. EMI Panel Finger 8P8C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60639v209%20Family_WR-MJ_Modular_Jack_Tab_Up_615008140621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60639v209%20Family_WR-MJ_Modular_Jack_Tab_Up_615008140621.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_EMI_PANEL_FINGER_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_EMI_PANEL_FINGER_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008140621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008140621?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008140621"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008140621"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Vertical Shielded EMI 8P8C
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact area 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 125 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161623v209%20Family_WR-MJTH_615008160521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161623v209%20Family_WR-MJTH_615008160521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_VERTICAL_SHIELDED_8P8C_EMI"&gt;https://katalog.we-online.com/en/em/MJ_THT_VERTICAL_SHIELDED_8P8C_EMI&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Yingchun Shan  2020-01-03&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160521"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008160521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004143821" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 4P4C Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33116v209%20Family_WR-MJ_615004143821.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33116v209%20Family_WR-MJ_615004143821.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_4P4C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_4P4C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004143821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615004143821?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615004143821"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615004143821"/>
<attribute name="XPXC" value="4P4C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Vertical Shielded 8P8C
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact plating 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 125 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161621v209%20Family_WR-MJTH_615008160421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161621v209%20Family_WR-MJTH_615008160421.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_VERTICAL_SHIELDED_8P8C"&gt;https://katalog.we-online.com/en/em/MJ_THT_VERTICAL_SHIELDED_8P8C&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-11-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160421">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160421"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008160421"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016240521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Dual Stacked w. EMI Panel Finger 8P8C Tab Up&amp;Down   &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120 V (AC)
&lt;br&gt;Withstanding Voltage:1000 V (AC)
&lt;br&gt;Contact Resistance:20 mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;br&gt;Insulator Material:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33142v209%20Family_WR-MJ_615016240521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33142v209%20Family_WR-MJ_615016240521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2020-01-02&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615016240521">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S1 S2"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S3 S4 S5 S6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615016240521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615016240521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615016240521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008140121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Front Grounding Post 8P8C Tab Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature	-40 up to +85 °C
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage	120 V (AC)
&lt;br&gt;Withstanding Voltage	1000 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;RISO	500 MΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	PBT
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;Shielding Material	Bronze
&lt;br&gt;Shielding Plating	Nickel (Ni)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o127572v209%20Family_MJ_Horizontal_Shielded_Front_Grounding_Post_8P8C_Tab_Down.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o127572v209%20Family_MJ_Horizontal_Shielded_Front_Grounding_Post_8P8C_Tab_Down.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_HORIZONTAL_SHIELDED_FRONT_GROUNDING_POST_8P8C_TAB_DOWN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MJ_HORIZONTAL_SHIELDED_FRONT_GROUNDING_POST_8P8C_TAB_DOWN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-13&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008140121">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008140121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008140121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008140121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615012143921" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Plastic Dual Port 6P6C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33115v209%20Family_WR-MC_615012143921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33115v209%20Family_WR-MC_615012143921.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_PLASTIC_DUAL_PORT_6P6C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_PLASTIC_DUAL_PORT_6P6C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C"/>
<gate name="B" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615012143921">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615012143921?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615012143921"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615012143921"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61500814221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded 8P8C Tab Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33129v209%20Family_WR-MJ_61500814221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33129v209%20Family_WR-MJ_61500814221.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_8P8C_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_8P8C_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-02&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="61500814221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/61500814221?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 61500814221 "/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value=" 61500814221 "/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160721" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT 47,5° Shielded 8P8C
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact area 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 125 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161627v209%20Family_WR-MJTH_615008160721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161627v209%20Family_WR-MJTH_615008160721.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_47_5-DEGREE_8P8C_SHIELDED"&gt;https://katalog.we-online.com/en/em/MJ_THT_47_5-DEGREE_8P8C_SHIELDED&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008160721">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160721?ae"/>
<attribute name="LED" value="/"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160721"/>
<attribute name="TYPE" value="47.5° "/>
<attribute name="VALUE" value="615008160721"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004141121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6PxC Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33139v209%20Family_WR-MJ_61500x141121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33139v209%20Family_WR-MJ_61500x141121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004141121">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615004141121?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615004141121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615004141121"/>
<attribute name="XPXC" value="6P4C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004144021" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 4P4C w. Ears &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;
Kind Properties
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33117v209%20Family_WR-MJ_615004144021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33117v209%20Family_WR-MJ_615004144021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_4P4C_W_EARS/"&gt;https://www.we-online.com/catalog/en/MJ_VERTICAL_PLASTIC_4P4C_W_EARS/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004144021">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615004144021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615004144021"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615004144021"/>
<attribute name="XPXC" value="4P4C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615096243321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded 2x 6 Stacked w. EMI Panel Finger 8P8C Tab Up&amp;Down   &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties

&lt;br&gt;&lt;/b&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:PA9T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating: Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material  Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33150v209%20Family_WR-MJ_615096243321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33150v209%20Family_WR-MJ_615096243321.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_2X_6_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_2X_6_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-03&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S"/>
<gate name="E" symbol="8P8C_S"/>
<gate name="F" symbol="8P8C_S"/>
<gate name="G" symbol="8P8C_S"/>
<gate name="L" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S1"/>
<gate name="H" symbol="8P8C_S1"/>
<gate name="I" symbol="8P8C_S1"/>
<gate name="J" symbol="8P8C_S1"/>
<gate name="K" symbol="8P8C_S1"/>
</gates>
<devices>
<device name="" package="615096243321">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S3"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S4"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="SHIELD" pad="S5"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="E" pin="1" pad="E1"/>
<connect gate="E" pin="2" pad="E2"/>
<connect gate="E" pin="3" pad="E3"/>
<connect gate="E" pin="4" pad="E4"/>
<connect gate="E" pin="5" pad="E5"/>
<connect gate="E" pin="6" pad="E6"/>
<connect gate="E" pin="7" pad="E7"/>
<connect gate="E" pin="8" pad="E8"/>
<connect gate="E" pin="SHIELD" pad="S6"/>
<connect gate="F" pin="1" pad="F1"/>
<connect gate="F" pin="2" pad="F2"/>
<connect gate="F" pin="3" pad="F3"/>
<connect gate="F" pin="4" pad="F4"/>
<connect gate="F" pin="5" pad="F5"/>
<connect gate="F" pin="6" pad="F6"/>
<connect gate="F" pin="7" pad="F7"/>
<connect gate="F" pin="8" pad="F8"/>
<connect gate="F" pin="SHIELD" pad="S7"/>
<connect gate="G" pin="1" pad="G1"/>
<connect gate="G" pin="2" pad="G2"/>
<connect gate="G" pin="3" pad="G3"/>
<connect gate="G" pin="4" pad="G4"/>
<connect gate="G" pin="5" pad="G5"/>
<connect gate="G" pin="6" pad="G6"/>
<connect gate="G" pin="7" pad="G7"/>
<connect gate="G" pin="8" pad="G8"/>
<connect gate="G" pin="SHIELD" pad="S8 S9"/>
<connect gate="H" pin="1" pad="H1"/>
<connect gate="H" pin="2" pad="H2"/>
<connect gate="H" pin="3" pad="H3"/>
<connect gate="H" pin="4" pad="H4"/>
<connect gate="H" pin="5" pad="H5"/>
<connect gate="H" pin="6" pad="H6"/>
<connect gate="H" pin="7" pad="H7"/>
<connect gate="H" pin="8" pad="H8"/>
<connect gate="I" pin="1" pad="I1"/>
<connect gate="I" pin="2" pad="I2"/>
<connect gate="I" pin="3" pad="I3"/>
<connect gate="I" pin="4" pad="I4"/>
<connect gate="I" pin="5" pad="I5"/>
<connect gate="I" pin="6" pad="I6"/>
<connect gate="I" pin="7" pad="I7"/>
<connect gate="I" pin="8" pad="I8"/>
<connect gate="J" pin="1" pad="J1"/>
<connect gate="J" pin="2" pad="J2"/>
<connect gate="J" pin="3" pad="J3"/>
<connect gate="J" pin="4" pad="J4"/>
<connect gate="J" pin="5" pad="J5"/>
<connect gate="J" pin="6" pad="J6"/>
<connect gate="J" pin="7" pad="J7"/>
<connect gate="J" pin="8" pad="J8"/>
<connect gate="K" pin="1" pad="K1"/>
<connect gate="K" pin="2" pad="K2"/>
<connect gate="K" pin="3" pad="K3"/>
<connect gate="K" pin="4" pad="K4"/>
<connect gate="K" pin="5" pad="K5"/>
<connect gate="K" pin="6" pad="K6"/>
<connect gate="K" pin="7" pad="K7"/>
<connect gate="K" pin="8" pad="K8"/>
<connect gate="L" pin="1" pad="L1"/>
<connect gate="L" pin="2" pad="L2"/>
<connect gate="L" pin="3" pad="L3"/>
<connect gate="L" pin="4" pad="L4"/>
<connect gate="L" pin="5" pad="L5"/>
<connect gate="L" pin="6" pad="L6"/>
<connect gate="L" pin="7" pad="L7"/>
<connect gate="L" pin="8" pad="L8"/>
<connect gate="L" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615096243321?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615096243321"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615096243321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032137921" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Ganged 4 Ports w. LED and EMI Panel Finger 8P8C Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;LED:yellow-green
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material  Bronze
&lt;br&gt;Shielding Plating:Nickel


&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33146v209%20Family_WR-MJ_615032137921.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33146v209%20Family_WR-MJ_615032137921.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_GANGED_4_PORTS_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_GANGED_4_PORTS_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;
Updated by Yingchun,Shan  2020-01-02&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_LEDYG"/>
<gate name="B" symbol="8P8C_S_LEDYG"/>
<gate name="C" symbol="8P8C_S_LEDYG"/>
<gate name="D" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615032137921">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+" pad="A10"/>
<connect gate="A" pin="G-" pad="A9"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="A" pin="Y+" pad="A12"/>
<connect gate="A" pin="Y-" pad="A11"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+" pad="B10"/>
<connect gate="B" pin="G-" pad="B9"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
<connect gate="B" pin="Y+" pad="B12"/>
<connect gate="B" pin="Y-" pad="B11"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="G+" pad="C10"/>
<connect gate="C" pin="G-" pad="C9"/>
<connect gate="C" pin="SHIELD" pad="S3"/>
<connect gate="C" pin="Y+" pad="C12"/>
<connect gate="C" pin="Y-" pad="C11"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="G+" pad="D10"/>
<connect gate="D" pin="G-" pad="D9"/>
<connect gate="D" pin="SHIELD" pad="S4"/>
<connect gate="D" pin="Y+" pad="D12"/>
<connect gate="D" pin="Y-" pad="D11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615032137921?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615032137921"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615032137921"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615016137721" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Dual Port w. EMI Panel Finger 8P8C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;LED:yellow-green
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;br&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material  Bronze
&lt;br&gt;Shielding Plating:Nickel


&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33141v209%20Family_WR-MJ_615016137721.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33141v209%20Family_WR-MJ_615016137721.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_PORT_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_DUAL_PORT_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;
Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S_LEDYG"/>
<gate name="B" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615016137721">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="G+" pad="A10"/>
<connect gate="A" pin="G-" pad="A9"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="A" pin="Y+" pad="A12"/>
<connect gate="A" pin="Y-" pad="A11"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="G+" pad="B10"/>
<connect gate="B" pin="G-" pad="B9"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
<connect gate="B" pin="Y+" pad="B12"/>
<connect gate="B" pin="Y-" pad="B11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615016137721?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615016137721"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615016137721"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006149421L" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006149421L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006149421L?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006149421L"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006149421L"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615018149421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C_S"/>
<gate name="C" symbol="6P6C_S"/>
<gate name="B" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615018149421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615018149421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615018149421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615018149421"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006143221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded 6P6C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33119v209%20Family_WR-MJ_615006143221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33119v209%20Family_WR-MJ_615006143221.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006143221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006143221?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006143221"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006143221"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008142121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:750 Mating cycles
&lt;br&gt;LED:2xBipolar Y/G; yellow-green
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:-40 V (AC); 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33152v209%20Family_WR-MJ_6150081xxx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33152v209%20Family_WR-MJ_6150081xxx21.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_2LEDYG"/>
</gates>
<devices>
<device name="" package="615008142121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+Y-_1" pad="11"/>
<connect gate="G$1" pin="G+Y-_2" pad="9"/>
<connect gate="G$1" pin="G-Y+_1" pad="12"/>
<connect gate="G$1" pin="G-Y+_2" pad="10"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008142121?ae"/>
<attribute name="LED" value="2xBipolar Y/G"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008142121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008142121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108185521" prefix="J">
<description>&lt;b&gt;Modular Jack SMT Horizontal Plastic 8P8C Tab Down WR-MJ&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;KIND PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Quality Class 750 Mating cycles 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;MATERIAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;GENERAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Operating Temperature -40 °C up to +85 °C 
&lt;br&gt;Compliance Lead free / RoHS 
&lt;/b&gt;
&lt;br&gt;&lt;br&gt;ELECTRICAL PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Rated Current [1] 1.5 A 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;Insulation Resistance 1000 MΩ 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;STANDARD:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;UL Approval E324776 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;PACKAGING PROPERTIES:&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel &amp; Mylar 
&lt;br&gt;Packaging Unit (Qty.) 120 mm 
&lt;br&gt;
&lt;br&gt;
&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WR-MJ_634108185521.jpg" title="Enlarge picture"&gt;

&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WR-MJ_634108185521.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt; Details see: &lt;a href="http://katalog.we-online.de/em/datasheet/634108185521.pdf"&gt; http://katalog.we-online.de/em/datasheet/634108185521.pdf&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated byYingchun,Shan ,2020-01-03&lt;br&gt;
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108185521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634108185521?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634108185521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="634108185521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT 47,5° 8P8C
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact area 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 125 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 35 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161625v209%20Family_WR-MJTH_615008160621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161625v209%20Family_WR-MJTH_615008160621.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_47_5-DEGREE_8P8C"&gt;https://katalog.we-online.com/en/em/MJ_THT_47_5-DEGREE_8P8C&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2019-11-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008160621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160621?ae"/>
<attribute name="LED" value="/"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160621"/>
<attribute name="TYPE" value="47.5° "/>
<attribute name="VALUE" value="615008160621"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008150121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Mid-Mount Plastic Tab Up with LED Y/G  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;B&gt;Kind Properties&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt; yellow-green
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: Lead free / RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Working Voltage:125V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135224v209%20Family_WR-MJ-615008150121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135224v209%20Family_WR-MJ-615008150121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_MID_MOUNT_PLASTIC_TAB_UP_W_LED/"&gt;https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_MID_MOUNT_PLASTIC_TAB_UP_W_LED/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-12-08&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_LEDYG"/>
</gates>
<devices>
<device name="" package="615008150121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008150121?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008150121"/>
<attribute name="TYPE" value="Right Angle"/>
<attribute name="VALUE" value="615008150121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008141321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:750 Mating cycles
&lt;br&gt;LED:2xBipolar Y/G; yellow-green
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:-40 V (AC); 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33152v209%20Family_WR-MJ_6150081xxx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33152v209%20Family_WR-MJ_6150081xxx21.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_2LEDYG"/>
</gates>
<devices>
<device name="" package="615008141321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+Y-_1" pad="12"/>
<connect gate="G$1" pin="G+Y-_2" pad="10"/>
<connect gate="G$1" pin="G-Y+_1" pad="11"/>
<connect gate="G$1" pin="G-Y+_2" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008141321?ae"/>
<attribute name="LED" value="2xBipolar Y/G"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008141321"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008141321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008149821" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded SMT 8P8C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PA9T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Cover Material Brass
&lt;br&gt;Cover Plating Nickel
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60696v209%20Family_WR-MJ_Horizontal_Shielded_634008149821_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60696v209%20Family_WR-MJ_Horizontal_Shielded_634008149821_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_SHIELDED_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_SHIELDED_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634008149821">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634008149821?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634008149821"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="634008149821"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008185121" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Low Profile w. LED 8P8C Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;LED:yellow-green
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C

&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;br&gt;Working Voltage:-40 V (AC); 120 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:30mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PA10T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Stainless Steel


&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tape and Reel
&lt;br&gt;Qty.160

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106786v209%20Family_WR-MJ_615008185121.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106786v209%20Family_WR-MJ_615008185121.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_LOW_PROFILE_W_LED_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_LOW_PROFILE_W_LED_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2019-11-26&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008185121">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008185121?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008185121"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008185121"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008137421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C
&lt;br&gt;LED 2xBipolar Y/G; yellow-green
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage	120 V (AC)
&lt;br&gt;Withstanding Voltage	1000 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;RISO	500 MΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	PBT
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;&lt;br&gt;Contact Type	Stamped
&lt;br&gt;Shielding Material	Bronze
&lt;br&gt;Shielding Plating	Nickel (Ni)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33152v209%20Family_WR-MJ_6150081xxx21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33152v209%20Family_WR-MJ_6150081xxx21.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-13&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615008137421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008137421?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008137421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008137421"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108150221R" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THR Horizontal Mid-Mount Shielded Tab Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;/b&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:Lead free / RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Working Voltage: 125 V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Materia:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;
&lt;br&gt;Packaging:Tape and Reel
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135233v209%20Family_WR-MJ_615108150221R.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135233v209%20Family_WR-MJ_615108150221R.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_THR_HORIZONTAL_MID_MOUNT_SHIELDED_TAB_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_THR_HORIZONTAL_MID_MOUNT_SHIELDED_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2021-12-08&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615108150221R">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615108150221R?ae"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="615108150221R"/>
<attribute name="TYPE" value="Right Angle"/>
<attribute name="VALUE" value="615108150221R"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108149621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack SMT Vertical Plastic 8P8C Top Entry&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tape and Reel &amp; Mylar
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60722v209%20Family_WR-MJ_634108149621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60722v209%20Family_WR-MJ_634108149621.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_8P8C_TOP_ENTRY/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_8P8C_TOP_ENTRY/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108149621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634108149621?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634108149621"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="634108149621"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634008137521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded SMT w. LED and EMI Panel Finger 8P8C Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;LED yellow-green 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 120 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 500 MΩ 

&lt;br&gt;&lt;b&gt;
&lt;br&gt;Material Properties&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Brass 
&lt;br&gt;Shielding Plating Nickel (Ni) 
&lt;br&gt;

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Packaging Tape and Reel 
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o60691v209%20Family_WR-MJ_634008137521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o60691v209%20Family_WR-MJ_634008137521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_SMT_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/MJ_SMT_HORIZONTAL_SHIELDED_W_LED_AND_EMI_PANEL_FINGER_8P8C_TAB_UP&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-06-27&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="634008137521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="11"/>
<connect gate="G$1" pin="G-" pad="12"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="9"/>
<connect gate="G$1" pin="Y-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634008137521?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634008137521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="634008137521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008145221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack 45° Entry Shielded 8P8C Standard &amp; Reverse Metal Post Trail&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;&lt;br&gt;
Material Properties&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Insulator Material PBT 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating Selective Gold 
&lt;br&gt;Contact Type Stamped 
&lt;br&gt;Shielding Material Bronze 
&lt;br&gt;Shielding Plating Nickel (Ni) 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 120 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 500 MΩ 
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;&lt;br&gt;
&lt;br&gt;Packaging Tray 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33136v209%20Family_WR-MJ_615008145x21.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33136v209%20Family_WR-MJ_615008145x21.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_45-DEGREE_ENTRY_SHIELDED_8P8C_STANDARD_REVERSE_METAL_POST_TAIL_615008145X21/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/MJ_45-DEGREE_ENTRY_SHIELDED_8P8C_STANDARD_REVERSE_METAL_POST_TAIL_615008145X21&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-06-27&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008145221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008145221?ae"/>
<attribute name="LED" value="/"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008145221"/>
<attribute name="TYPE" value="45° "/>
<attribute name="VALUE" value="615008145221"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006149421R" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615006149421R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006149421R?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006149421R"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006149421R"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008142621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded Front Grounding Post 8P8C Tab Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature	-40 up to +85 °C
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage	120 V (AC)
&lt;br&gt;Withstanding Voltage	1000 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;RISO	500 MΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	PBT
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;Shielding Material	Bronze
&lt;br&gt;Shielding Plating	Nickel (Ni)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33131v209%20Family_WR-MJ_615008142621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33131v209%20Family_WR-MJ_615008142621.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_HORIZONTAL_SHIELDED_REAR_GROUNDING_POST_8P8C_TAB_DOWN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MJ_HORIZONTAL_SHIELDED_REAR_GROUNDING_POST_8P8C_TAB_DOWN&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-13&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008142621">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008142621?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008142621"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008142621"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008160021" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Plastic 8P8C Tab Up
&lt;br&gt;
&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PA9T 
&lt;br&gt;Insulator Flammability Rating UL94 V-0 
&lt;br&gt;Insulator Color Black 
&lt;br&gt;Contact Material Copper Alloy 
&lt;br&gt;Contact Plating 6u' on contact plating 
&lt;br&gt;Contact Type Wired 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -40 up to +85 °C 
&lt;br&gt;&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage 150 V (AC) 
&lt;br&gt;Withstanding Voltage 1000 V (AC) 
&lt;br&gt;Contact Resistance 20 mΩ 
&lt;br&gt;RISO 1000 MΩ 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o161613v209%20Family_WR-MJTH_615008160021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o161613v209%20Family_WR-MJTH_615008160021.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/em/MJ_THT_HORIZONTAL_PLASTIC_8P8C_TAB_UP"&gt;https://katalog.we-online.com/en/em/MJ_THT_HORIZONTAL_PLASTIC_8P8C_TAB_UP&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-11-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008160021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008160021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008160021"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008160021"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615004138421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6PxC Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33138v209%20Family_WR-MJ_61500x138421.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33138v209%20Family_WR-MJ_61500x138421.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6PXC_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C"/>
</gates>
<devices>
<device name="" package="615004138421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615004138421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615004138421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615004138421"/>
<attribute name="XPXC" value="6P4C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615012149421" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="6P6C_S"/>
<gate name="B" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="615012149421">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="SHIELD" pad="S1"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="SHIELD" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615012149421?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615012149421"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615012149421"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634104149621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack SMT Vertical Plastic 4P4C Top Entry  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60710v209%20Family_I-O_MJ_Vertical_Plastic_Top%20Entry%20_4P4C_634104149621_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60710v209%20Family_I-O_MJ_Vertical_Plastic_Top%20Entry%20_4P4C_634104149621_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_4P4C_TOP_ENTRY/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_4P4C_TOP_ENTRY/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P4C_S"/>
</gates>
<devices>
<device name="" package="634104149621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="SHILED" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634104149621?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634104149621"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="634104149621"/>
<attribute name="XPXC" value="4P4C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008149521L" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64597v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149521_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_8P8C_TAB_UP/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008149521L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008149521L?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008149521L"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008149521L"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634108150321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack SMT Horizontal Mid-Mount Shielded Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:Lead free / RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;br&gt;Working Voltage:125V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating: Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tape and Reel

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135236v209%20Family_WR-MJ_634108150321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135236v209%20Family_WR-MJ_634108150321.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_MID_MOUNT_SHIELDED_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_HORIZONTAL_MID_MOUNT_SHIELDED_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-1-3&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="634108150321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634108150321?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634108150321"/>
<attribute name="TYPE" value="Right Angle"/>
<attribute name="VALUE" value="634108150321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008145521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded w. EMI Panel Finger 8P8C CAT 5e Tab Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 125 V (AC)
&lt;br&gt;&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PA66
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33135v209%20Family_WR-MJ_615008145521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33135v209%20Family_WR-MJ_615008145521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_HORIZONTAL_SHIELDED_W_EMI_PANEL_FINGER_8P8C_CAT_5E_TAB_DOWN/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/MJ_HORIZONTAL_SHIELDED_W_EMI_PANEL_FINGER_8P8C_CAT_5E_TAB_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-07-19&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008145521">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008145521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008145521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008145521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006149421M" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Assembly Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33122v209%20Family_Con_WR-MJ_Horizontal_Plastic_6150xx149421_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_ASSEMBLY_6P6C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006149421M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006149421M?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006149421M"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006149421M"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615064243321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded 2x 4 Stacked w. EMI Panel Finger 8P8C Tab Up&amp;Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties

&lt;br&gt;&lt;/b&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage: 120 V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:PA9T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating: Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material  Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33148v209%20Family_WR-MJ_615064243321.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33148v209%20Family_WR-MJ_615064243321.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_2X_4_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_2X_4_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-03&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S1"/>
<gate name="C" symbol="8P8C_S1"/>
<gate name="F" symbol="8P8C_S1"/>
<gate name="G" symbol="8P8C_S1"/>
<gate name="H" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
<gate name="E" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615064243321">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S3"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="SHIELD" pad="S4"/>
<connect gate="E" pin="1" pad="E1"/>
<connect gate="E" pin="2" pad="E2"/>
<connect gate="E" pin="3" pad="E3"/>
<connect gate="E" pin="4" pad="E4"/>
<connect gate="E" pin="5" pad="E5"/>
<connect gate="E" pin="6" pad="E6"/>
<connect gate="E" pin="7" pad="E7"/>
<connect gate="E" pin="8" pad="E8"/>
<connect gate="E" pin="SHIELD" pad="S5 S6"/>
<connect gate="F" pin="1" pad="F1"/>
<connect gate="F" pin="2" pad="F2"/>
<connect gate="F" pin="3" pad="F3"/>
<connect gate="F" pin="4" pad="F4"/>
<connect gate="F" pin="5" pad="F5"/>
<connect gate="F" pin="6" pad="F6"/>
<connect gate="F" pin="7" pad="F7"/>
<connect gate="F" pin="8" pad="F8"/>
<connect gate="G" pin="1" pad="G1"/>
<connect gate="G" pin="2" pad="G2"/>
<connect gate="G" pin="3" pad="G3"/>
<connect gate="G" pin="4" pad="G4"/>
<connect gate="G" pin="5" pad="G5"/>
<connect gate="G" pin="6" pad="G6"/>
<connect gate="G" pin="7" pad="G7"/>
<connect gate="G" pin="8" pad="G8"/>
<connect gate="H" pin="1" pad="H1"/>
<connect gate="H" pin="2" pad="H2"/>
<connect gate="H" pin="3" pad="H3"/>
<connect gate="H" pin="4" pad="H4"/>
<connect gate="H" pin="5" pad="H5"/>
<connect gate="H" pin="6" pad="H6"/>
<connect gate="H" pin="7" pad="H7"/>
<connect gate="H" pin="8" pad="H8"/>
<connect gate="H" pin="SHIELD" pad="S1 S2" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615064243321?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615064243321"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615064243321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615032243321" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Shielded 2x Dual Stacked w. EMI Panel Finger 8P8C Tab Up&amp;Down  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Quality Class:500 Mating cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;IR 1:1.5 A
&lt;br&gt;Working Voltage:120 V (AC)
&lt;br&gt;Withstanding Voltage:1000 V (AC)
&lt;br&gt;Contact Resistance:20 mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties&lt;/b&gt;
&lt;br&gt;Insulator Material:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Material:Bronze
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_2X_DUAL_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_2X_DUAL_STACKED_PORT_EMI_FINGER_8P8C_TAB_UP_DOWN/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan 2020-1-2&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="A" symbol="8P8C_S"/>
<gate name="B" symbol="8P8C_S"/>
<gate name="C" symbol="8P8C_S"/>
<gate name="D" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615032243321">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="A" pin="3" pad="A3"/>
<connect gate="A" pin="4" pad="A4"/>
<connect gate="A" pin="5" pad="A5"/>
<connect gate="A" pin="6" pad="A6"/>
<connect gate="A" pin="7" pad="A7"/>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="SHIELD" pad="S3 S4"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="B" pin="3" pad="B3"/>
<connect gate="B" pin="4" pad="B4"/>
<connect gate="B" pin="5" pad="B5"/>
<connect gate="B" pin="6" pad="B6"/>
<connect gate="B" pin="7" pad="B7"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="SHIELD" pad="S5"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="C" pin="3" pad="C3"/>
<connect gate="C" pin="4" pad="C4"/>
<connect gate="C" pin="5" pad="C5"/>
<connect gate="C" pin="6" pad="C6"/>
<connect gate="C" pin="7" pad="C7"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="SHIELD" pad="S6 S7"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
<connect gate="D" pin="3" pad="D3"/>
<connect gate="D" pin="4" pad="D4"/>
<connect gate="D" pin="5" pad="D5"/>
<connect gate="D" pin="6" pad="D6"/>
<connect gate="D" pin="7" pad="D7"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615032243321?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615032243321"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615032243321"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="634106149621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack SMT Vertical Plastic 6P6C Top Entry &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;Working Voltage:120V (AC)
&lt;/b&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;/B&gt;&lt;br&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tape and Reel &amp; Mylar
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o60720v209%20Family_WR-MJ_Vertical_Plastic_634106149621_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o60720v209%20Family_WR-MJ_Vertical_Plastic_634106149621_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_6P6C_TOP_ENTRY/"&gt;https://www.we-online.com/catalog/en/MJ_SMT_VERTICAL_PLASTIC_6P6C_TOP_ENTRY/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C_S"/>
</gates>
<devices>
<device name="" package="634106149621">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/634106149621?ae"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="634106149621"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="634106149621"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008138221" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Shielded 8P8C Front Post &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature	-40 up to +85 °C
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage	120 V (AC)
&lt;br&gt;Withstanding Voltage	1000 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;RISO	500 MΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	PBT
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;Shielding Material	Bronze
&lt;br&gt;Shielding Plating	Nickel (Ni)
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33125v209%20Family_WR-MJ_615008138221.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33125v209%20Family_WR-MJ_615008138221.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_VERTICAL_SHIELDED_8P8C_FRONT_POST/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MJ_VERTICAL_SHIELDED_8P8C_FRONT_POST&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-13&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S"/>
</gates>
<devices>
<device name="" package="615008138221">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008138221?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008138221"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008138221"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615006143621" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 6P6C Tab Down &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o33121v209%20Family_WR-MJ_THT_6P6C_61500X143621.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o33121v209%20Family_WR-MJ_THT_6P6C_61500X143621.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6P6C_TAB_DOWN/?"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_6P6C_TAB_DOWN/?&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6P6C"/>
</gates>
<devices>
<device name="" package="615006143621">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615006143621?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615006143621"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615006143621"/>
<attribute name="XPXC" value="6P6C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615108137421R" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THR Horizontal Shielded w. LED and EMI Finger 8P8C Tab Up&lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Kind Properties
&lt;br&gt;&lt;/b&gt;Quality Class:750 Mating cycles
&lt;br&gt;LED:yellow-green
&lt;/b&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance:Lead free / RoHS
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR1:1.5A
&lt;br&gt;Working Voltage: 125 V (AC)
&lt;br&gt;Withstanding Voltage:1000 V (AC)
&lt;br&gt;Contact Resistance:30mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;br&gt;&lt;/b&gt;Insulator MateriaL:PA9T
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material:Copper Alloy
&lt;br&gt;Contact Plating: Selective Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;Shielding Materia:Brass
&lt;br&gt;Shielding Plating:Nickel
&lt;br&gt;

&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tape and Reel
&lt;br&gt;Qty. 100
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o107344v209%20Family_WR-MJ_615108137421R.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o107344v209%20Family_WR-MJ_615108137421R.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_FINGER_THR_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_SHIELDED_W_LED_AND_EMI_FINGER_THR_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-03&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_S_LEDYG"/>
</gates>
<devices>
<device name="" package="615108137421R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="G+" pad="10"/>
<connect gate="G$1" pin="G-" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2"/>
<connect gate="G$1" pin="Y+" pad="12"/>
<connect gate="G$1" pin="Y-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615108137421R?ae"/>
<attribute name="LED" value="yellow-green"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="PART-NUMBER" value="615108137421R"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615108137421R"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008138021" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Vertical Plastic 8P8C &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature	-40 up to +85 °C
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Working Voltage	120 V (AC)
&lt;br&gt;Withstanding Voltage	1000 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;RISO	500 MΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material	PBT
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Black
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Selective Gold
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Packaging Properties
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o33124v209%20Family_WR-MJ_615008138021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o33124v209%20Family_WR-MJ_615008138021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MJ_VERTICAL_PLASTIC_8P8C/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MJ_VERTICAL_PLASTIC_8P8C&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-13&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008138021">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008138021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008138021"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="VALUE" value="615008138021"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008148521" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack Horizontal Plastic 8P8C Tab Up  &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Quality Class:500 Mating cycles

&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: RoHS
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
&lt;br&gt;IR 1:1.5A
&lt;br&gt;Working Voltage:120V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:500 MΩ
&lt;br&gt;
&lt;br&gt;Material Properties
&lt;br&gt;Insulator MateriaL:PBT
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o76656v209%20Family_WR-MJ_Plastic_Horizontal_Tab-UP_615008148521.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o76656v209%20Family_WR-MJ_Plastic_Horizontal_Tab-UP_615008148521.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_8P8C_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_HORIZONTAL_PLASTIC_8P8C_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-06&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008148521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008148521?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008148521"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE" value="615008148521"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="615008150021" prefix="J">
<description>&lt;b&gt;WR-MJ Modular Jack THT Horizontal Mid-Mount Plastic Tab Up &lt;br&gt; &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;br&gt;
&lt;b&gt;General Information
&lt;br&gt;
&lt;/b&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;Compliance: Lead free / RoHS
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Electrical Properties
&lt;/b&gt;
&lt;br&gt;Working Voltage:125V (AC)
&lt;br&gt;Withstanding Voltage:1000V (AC)
&lt;br&gt;Contact Resistance:20mΩ
&lt;br&gt;RISO:1000 MΩ
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Material Properties
&lt;br&gt;
&lt;br&gt;&lt;/B&gt;Insulator MateriaL:LCP
&lt;br&gt;Insulator Flammability Rating:UL94 V-0
&lt;br&gt;Color:Black
&lt;br&gt;Contact Material Copper Alloy
&lt;br&gt;Contact Plating:Gold
&lt;br&gt;Contact Type:Stamped
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Packaging Properties&lt;/B&gt;
&lt;br&gt;Packaging:Tray
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135222v209%20Family_WR-MJ_615008150021.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135222v209%20Family_WR-MJ_615008150021.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_MID_MOUNT_PLASTIC_TAB_UP/"&gt;https://www.we-online.com/catalog/en/MJ_THT_HORIZONTAL_MID_MOUNT_PLASTIC_TAB_UP/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun,Shan  2020-01-07&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8P8C_2"/>
</gates>
<devices>
<device name="" package="615008150021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/615008150021?ae"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="615008150021"/>
<attribute name="TYPE" value="Right Angle"/>
<attribute name="VALUE" value="615008150021"/>
<attribute name="XPXC" value="8P8C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
