<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Coaxial Connectors - N-Type Connectors - WR-NTYPE &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-11-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="60411052241502">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Right Angle Jack, THT, 5pins</description>
</package>
<package name="60412042241503">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Jack, THT, 5pins</description>
</package>
<package name="60412052241504">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Straight Jack, THT, 5pins</description>
</package>
<package name="60411042241501">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Right Angle Jack, THT, 5pins</description>
</package>
</packages>
<symbols>
<symbol name="JACK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="60411052241502" prefix="J">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50 Ohm
&lt;br&gt;Plating: Nickel and Gold
&lt;br&gt;Mating: Screw (Recommended: Torque wrench tool)
&lt;br&gt;Ingress Protection: IP67
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and Measurement Equipment
&lt;br&gt;Industrial application
&lt;br&gt;High power machinery
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2022-11-23&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60411052241502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø1.6"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60411052241502?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~4 GHz"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 up to +165 °C"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PANEL-THICKNESS" value="6.5mm"/>
<attribute name="PART-NUMBER" value="60411052241502"/>
<attribute name="VALUE" value="60411052241502"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60412042241503" prefix="J">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50 Ohm
&lt;br&gt;Plating: Nickel and Gold
&lt;br&gt;Mating: Screw (Recommended: Torque wrench tool)
&lt;br&gt;Ingress Protection: IP67
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and Measurement Equipment
&lt;br&gt;Industrial application
&lt;br&gt;High power machinery
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2022-11-23&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60412042241503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø1.14"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60412042241503?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 up to +165 °C"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PANEL-THICKNESS" value="6.5mm"/>
<attribute name="PART-NUMBER" value="60412042241503"/>
<attribute name="VALUE" value="60412042241503"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60412052241504" prefix="J">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50 Ohm
&lt;br&gt;Plating: Nickel and Gold
&lt;br&gt;Mating: Screw (Recommended: Torque wrench tool)
&lt;br&gt;Ingress Protection: IP67
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and Measurement Equipment
&lt;br&gt;Industrial application
&lt;br&gt;High power machinery
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2022-11-23&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60412052241504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø1.14"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60412052241504?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~6 GHz"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 up to +165 °C"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PANEL-THICKNESS" value="6.5mm"/>
<attribute name="PART-NUMBER" value="60412052241504"/>
<attribute name="VALUE" value="60412052241504"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60411042241501" prefix="J">
<description>&lt;b&gt;WR-NTYPE N Type PCB Connectors&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
Characteristics 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface: MIL-STD-348
&lt;br&gt;Mating Cycle: 500 Cycles
&lt;br&gt;Impedance: 50 Ohm
&lt;br&gt;Plating: Nickel and Gold
&lt;br&gt;Mating: Screw (Recommended: Torque wrench tool)
&lt;br&gt;Ingress Protection: IP67
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Network and communications
&lt;br&gt;RF Test and Measurement Equipment
&lt;br&gt;Industrial application
&lt;br&gt;High power machinery
&lt;br&gt;Outdoor or humid environment
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o698256v209%20family-wr-ntype-60411042241501.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/catalog/WR-NTYPE_PCB_CONNECTORS&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2022-11-23&lt;br&gt;
2022(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="" package="60411042241501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CENTER-CONTACT" value="Ø1.6"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/60411042241501?ae"/>
<attribute name="FREQUENCY-RANGE" value="DC~4 GHz"/>
<attribute name="GENDER" value="Jack"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="OPERATING-TEMPERATURE" value="-65 up to +165 °C"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PANEL-THICKNESS" value="6.5mm"/>
<attribute name="PART-NUMBER" value="60411042241501"/>
<attribute name="VALUE" value="60411042241501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
