<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Wire-to-Board Connectors - WR-RAST &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-10-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="637101110102">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110207">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110503">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110202">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110104">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120307">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110103">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110205">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110703">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110109">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110108">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110107">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110105">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110204">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120107">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120205">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120108">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120102">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120202">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120203">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120207">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120703">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110110">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120106">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110106">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101120110">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120105">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120109">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120103">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120204">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120104">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101120503">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header</description>
</package>
<package name="637101110203">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
<package name="637101110307">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header</description>
</package>
</packages>
<symbols>
<symbol name="12PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="3PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="4PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="11PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="2PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="9PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="7PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="8PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="6PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="10PT">
<description>Pin Header THT</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="637101110102" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101110102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110102?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110102 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 2 "/>
<attribute name="VALUE" value=" 637101110102 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110207" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101110207">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110207?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110207 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="VALUE" value=" 637101110207 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110503" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110503">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110503?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110503 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101110503 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110202" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101110202">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110202?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110202 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 2 "/>
<attribute name="VALUE" value=" 637101110202 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110104" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101110104">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110104?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110104 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="VALUE" value=" 637101110104 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120307" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101120307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120307?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120307 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="VALUE" value=" 637101120307 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110103" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110103">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110103?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110103 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101110103 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110205" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101110205">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110205?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110205 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="VALUE" value=" 637101110205 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110703" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110703">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110703?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110703 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101110703 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110109" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="637101110109">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110109?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110109 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 9 "/>
<attribute name="VALUE" value=" 637101110109 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110108" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="637101110108">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110108?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110108 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="VALUE" value=" 637101110108 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110107" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101110107">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110107?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110107 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="VALUE" value=" 637101110107 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110105" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101110105">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110105?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110105 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="VALUE" value=" 637101110105 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110204" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101110204">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110204?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110204 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="VALUE" value=" 637101110204 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120107" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101120107">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120107?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120107 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="VALUE" value=" 637101120107 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120205" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101120205">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120205?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120205 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="VALUE" value=" 637101120205 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120108" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8PT"/>
</gates>
<devices>
<device name="" package="637101120108">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120108?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120108 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 8 "/>
<attribute name="VALUE" value=" 637101120108 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120102" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101120102">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120102?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120102 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 2 "/>
<attribute name="VALUE" value=" 637101120102 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120202" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="2PT"/>
</gates>
<devices>
<device name="" package="637101120202">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120202?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120202 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 2 "/>
<attribute name="VALUE" value=" 637101120202 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120203" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120203">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120203?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120203 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101120203 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120703" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120703">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120703?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120703 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101120703 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120207" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101120207">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120207?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120207 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="VALUE" value=" 637101120207 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110110" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="637101110110">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110110?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110110 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 10 "/>
<attribute name="VALUE" value=" 637101110110 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120106" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="637101120106">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120106?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120106 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 6 "/>
<attribute name="VALUE" value=" 637101120106 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110106" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="6PT"/>
</gates>
<devices>
<device name="" package="637101110106">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110106?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110106 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 6 "/>
<attribute name="VALUE" value=" 637101110106 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120110" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="10PT"/>
</gates>
<devices>
<device name="" package="637101120110">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="10" pad="10 A10"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120110?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120110 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 10 "/>
<attribute name="VALUE" value=" 637101120110 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120105" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="5PT"/>
</gates>
<devices>
<device name="" package="637101120105">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120105?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120105 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 5 "/>
<attribute name="VALUE" value=" 637101120105 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120109" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="9PT"/>
</gates>
<devices>
<device name="" package="637101120109">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
<connect gate="G$1" pin="8" pad="8 A8"/>
<connect gate="G$1" pin="9" pad="9 A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120109?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120109 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 9 "/>
<attribute name="VALUE" value=" 637101120109 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120103" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120103">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120103?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120103 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101120103 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120204" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101120204">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120204?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120204 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="VALUE" value=" 637101120204 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120104" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="4PT"/>
</gates>
<devices>
<device name="" package="637101120104">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120104?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120104 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 4 "/>
<attribute name="VALUE" value=" 637101120104 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101120503" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Horizontal Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798408v209%20Multi-WR-RAST5-637101120102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_HORIZONTAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_HORIZONTAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101120503">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101120503?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101120503 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101120503 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110203" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="3PT"/>
</gates>
<devices>
<device name="" package="637101110203">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110203?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110203 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 3 "/>
<attribute name="VALUE" value=" 637101110203 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="637101110307" prefix="J">
<description>&lt;b&gt;WR-RAST 5mm Male Vertical Header&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Pitch: 5mm
&lt;br&gt;Operating Temperature: -40 °C up to +110 °C
&lt;br&gt;Contact Type: Stamped
&lt;br&gt;Insulator Material: PA66
&lt;br&gt;Insulator Flammability Rating: UL94 V-0
&lt;br&gt;Insulator Color: Natural
&lt;br&gt;Contact Material: Copper Alloy
&lt;br&gt;Contact Plating: Tin
&lt;br&gt;Withstanding Voltage: 500 V (AC)
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Glow-Wire Compliancy
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Conform to IEC 60335-1
&lt;br&gt;Tested at 750 °C and 850 °C
&lt;br&gt;Perform by third party laboratory
&lt;br&gt;Suitable for non-attended appliances and many other applications
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;White goods
&lt;br&gt;Unattended appliance
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Electrical Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;IR	16 A
&lt;br&gt;Working Voltage	380 V (AC)
&lt;br&gt;Withstanding Voltage	500 V (AC)
&lt;br&gt;Contact Resistance	20 mΩ
&lt;br&gt;&lt;br&gt;

&lt;b&gt;General Information
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Pitch	5 mm
&lt;br&gt;Operating Temperature	-40 °C up to +110 °C
&lt;br&gt;Contact Type	Stamped
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Packaging Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Packaging	Tray
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Material Properties
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Insulator Material	PA66
&lt;br&gt;Insulator Flammability Rating	UL94 V-0
&lt;br&gt;Insulator Color	Natural
&lt;br&gt;Contact Material	Copper Alloy
&lt;br&gt;Contact Plating	Tin
&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798300v209%20Multi-WR-RAST5-637101110102.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WR_RAST_5MM_MALE_VERTICAL_HEADER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WR_RAST_5MM_MALE_VERTICAL_HEADER&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-10-10 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7PT"/>
</gates>
<devices>
<device name="" package="637101110307">
<connects>
<connect gate="G$1" pin="1" pad="1 A1"/>
<connect gate="G$1" pin="2" pad="2 A2"/>
<connect gate="G$1" pin="3" pad="3 A3"/>
<connect gate="G$1" pin="4" pad="4 A4"/>
<connect gate="G$1" pin="5" pad="5 A5"/>
<connect gate="G$1" pin="6" pad="6 A6"/>
<connect gate="G$1" pin="7" pad="7 A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="CONTACT-RESISTANCE" value="20mOhm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/637101110307?ae"/>
<attribute name="INSULATOR-COLOR" value="Natural"/>
<attribute name="INSULATOR-MATERIAL" value="PA66"/>
<attribute name="IR" value="16A"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 637101110307 "/>
<attribute name="PITCH" value="5mm"/>
<attribute name="POLARITY" value=" 7 "/>
<attribute name="VALUE" value=" 637101110307 "/>
<attribute name="WORKING-VOLTAGE" value="380V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
