<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Dip Switches - SMT Dip Switch - WS-DISV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-01-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="418121160810">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,10 poles</description>
</package>
<package name="418121160807">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,7 poles</description>
</package>
<package name="418121160806">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,6 poles</description>
</package>
<package name="418121160809">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,9 poles</description>
</package>
<package name="418121160801">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,1 poles</description>
</package>
<package name="416131160806">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,6Pole</description>
</package>
<package name="416131160805">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,5Pole</description>
</package>
<package name="416131160808">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,8Pole</description>
</package>
<package name="416131160804">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,4Pole</description>
</package>
<package name="416131160812">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,12Pole</description>
</package>
<package name="416131160803">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,3Pole</description>
</package>
<package name="418121160802">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,2 poles</description>
</package>
<package name="416131160801">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,1Pole</description>
</package>
<package name="418121160803">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,3 poles</description>
</package>
<package name="418121270812">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,12poles</description>
</package>
<package name="418121270809">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,9poles</description>
</package>
<package name="418121160808">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,8 poles</description>
</package>
<package name="418121160805">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,5 poles</description>
</package>
<package name="416131160810">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,10Pole</description>
</package>
<package name="418121270805">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,5poles</description>
</package>
<package name="418121270810">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,10poles</description>
</package>
<package name="418121270807">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,7poles</description>
</package>
<package name="418121270804">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,4poles</description>
</package>
<package name="416131160802">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 1.27 mm,2Pole</description>
</package>
<package name="418121270806">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,6poles</description>
</package>
<package name="418121270802">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,2poles</description>
</package>
<package name="418121270808">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,8poles</description>
</package>
<package name="418121160804">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,4 poles</description>
</package>
<package name="418121270803">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,3poles</description>
</package>
<package name="418121270801">
<description>&lt;B&gt;WS-DISV&lt;/B&gt;&lt;BR&gt; Small Compact SMT with Raised Actuator 2.54 mm,1pole</description>
</package>
<package name="418121160812">
<description>&lt;b&gt;WS-DISV&lt;/b&gt;&lt;br&gt; Small Compact SMT Flat Actuator with Top Tape 2.54 mm ,12 poles</description>
</package>
</packages>
<symbols>
<symbol name="10POLES">
<description>This symbol is 10 pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="A10" direction="pas"/>
</symbol>
<symbol name="7POLES">
<description>This symbol is 7pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
</symbol>
<symbol name="9POLES">
<description>This symbol is 9pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
</symbol>
<symbol name="6POLES">
<description>This symbol is 6pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
</symbol>
<symbol name="4POLES">
<description>This symbol is 4pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
</symbol>
<symbol name="2POLES">
<description>This symbol is 2pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="5POLES">
<description>This symbol is 5pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
</symbol>
<symbol name="3POLES">
<description>This symbol is 3pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
</symbol>
<symbol name="1POLE">
<description>This symbol is 1pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
<symbol name="12POLES">
<description>This symbol is 12pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
</symbol>
<symbol name="8POLES">
<description>This symbol is 8pole</description>
<pin name="1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="A8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="418121160810" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418121160810">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160810.pdf"/>
<attribute name="PART-NUMBER" value="418121160810"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160809" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9POLES"/>
</gates>
<devices>
<device name="" package="418121160809">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160809.pdf"/>
<attribute name="PART-NUMBER" value="418121160809"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160801" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="418121160801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160801.pdf"/>
<attribute name="PART-NUMBER" value="418121160801"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160808" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="416131160808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160808.pdf"/>
<attribute name="PART-NUMBER" value="416131160808"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160804" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="416131160804">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160804.pdf"/>
<attribute name="PART-NUMBER" value="416131160804"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160805" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="416131160805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160805.pdf"/>
<attribute name="PART-NUMBER" value="416131160805"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160806" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="416131160806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160806.pdf"/>
<attribute name="PART-NUMBER" value="416131160806"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160812" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="416131160812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160812.pdf"/>
<attribute name="PART-NUMBER" value="416131160812"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160807" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7POLES"/>
</gates>
<devices>
<device name="" package="418121160807">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160807.pdf"/>
<attribute name="PART-NUMBER" value="418121160807"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160806" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418121160806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160806.pdf"/>
<attribute name="PART-NUMBER" value="418121160806"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160803" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="416131160803">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160803.pdf"/>
<attribute name="PART-NUMBER" value="416131160803"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160802" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418121160802">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160802.pdf"/>
<attribute name="PART-NUMBER" value="418121160802"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160801" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="416131160801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160801.pdf"/>
<attribute name="PART-NUMBER" value="416131160801"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160803" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418121160803">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160803.pdf"/>
<attribute name="PART-NUMBER" value="418121160803"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270812" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="418121270812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270812.pdf"/>
<attribute name="PART-NUMBER" value="418121270812"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160808" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418121160808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160808.pdf"/>
<attribute name="PART-NUMBER" value="418121160808"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160805" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="418121160805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160805.pdf"/>
<attribute name="PART-NUMBER" value="418121160805"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270805" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="5POLES"/>
</gates>
<devices>
<device name="" package="418121270805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270805.pdf"/>
<attribute name="PART-NUMBER" value="418121270805"/>
<attribute name="PINS" value=" 5 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160810" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="416131160810">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160810.pdf"/>
<attribute name="PART-NUMBER" value="416131160810"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270810" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="10POLES"/>
</gates>
<devices>
<device name="" package="418121270810">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270810.pdf"/>
<attribute name="PART-NUMBER" value="418121270810"/>
<attribute name="PINS" value=" 10 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270807" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7POLES"/>
</gates>
<devices>
<device name="" package="418121270807">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270807.pdf"/>
<attribute name="PART-NUMBER" value="418121270807"/>
<attribute name="PINS" value=" 7 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270804" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418121270804">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270804.pdf"/>
<attribute name="PART-NUMBER" value="418121270804"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="416131160802" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 1.27 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:500 g
&lt;BR&gt;Electrical Life:1000 Cycles
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:200 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:300 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PPA
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Brown
&lt;BR&gt;Base Material:PPA
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Brown
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78362v209%20Family_WS-DISV_SMD_FLAT_ACTUATOR_4161311608xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_1_27_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="416131160802">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/416131160802.pdf"/>
<attribute name="PART-NUMBER" value="416131160802"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 2000 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160804" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="4POLES"/>
</gates>
<devices>
<device name="" package="418121160804">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160804.pdf"/>
<attribute name="PART-NUMBER" value="418121160804"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270802" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="2POLES"/>
</gates>
<devices>
<device name="" package="418121270802">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270802.pdf"/>
<attribute name="PART-NUMBER" value="418121270802"/>
<attribute name="PINS" value=" 2 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270803" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3POLES"/>
</gates>
<devices>
<device name="" package="418121270803">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270803.pdf"/>
<attribute name="PART-NUMBER" value="418121270803"/>
<attribute name="PINS" value=" 3 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270806" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6POLES"/>
</gates>
<devices>
<device name="" package="418121270806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270806.pdf"/>
<attribute name="PART-NUMBER" value="418121270806"/>
<attribute name="PINS" value=" 6 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121160812" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT Flat Actuator with Top Tape 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Flat Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o64617v209%20Family_WS-DISV_4181211608xxA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_FLAT_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="12POLES"/>
</gates>
<devices>
<device name="" package="418121160812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121160812.pdf"/>
<attribute name="PART-NUMBER" value="418121160812"/>
<attribute name="PINS" value=" 12 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270801" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="1POLE"/>
</gates>
<devices>
<device name="" package="418121270801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270801.pdf"/>
<attribute name="PART-NUMBER" value="418121270801"/>
<attribute name="PINS" value=" 1 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270809" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="9POLES"/>
</gates>
<devices>
<device name="" package="418121270809">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270809.pdf"/>
<attribute name="PART-NUMBER" value="418121270809"/>
<attribute name="PINS" value=" 9 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="418121270808" prefix="S" uservalue="yes">
<description>&lt;B&gt;WS-DISV Small Compact SMT with Raised Actuator 2.54 mm 
&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;
&lt;BR&gt;Operation Force:600 g
&lt;BR&gt;Electrical Life:2000 Times
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Properties&lt;/b&gt;
&lt;BR&gt;IR:25 mA
&lt;BR&gt;VR:24 V (DC)
&lt;BR&gt;IR:100 mA
&lt;BR&gt;VR:50 V (DC)
&lt;BR&gt;Contact Resistance Initial:50 mΩ
&lt;BR&gt;Contact Resistance After Life Test:100 mΩ
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:500 V (AC)
&lt;BR&gt;Actuator Type:Raise Type
&lt;BR&gt;Switch Position:Off
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Material Properties
&lt;/b&gt;&lt;BR&gt;Cover Material:PA9T
&lt;BR&gt;Cover Flammability Rating:UL94 V-0
&lt;BR&gt;Cover Color:Black
&lt;BR&gt;Base Material:PA9T
&lt;BR&gt;Base Flammability Rating:UL94 V-0
&lt;BR&gt;Base Color:Black
&lt;BR&gt;Actuator Material:PA46
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:White
&lt;BR&gt;Contact Material:Copper Alloy
&lt;BR&gt;Contact Plating:Gold
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Gold
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tape and Reel&lt;BR&gt;&lt;BR&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o77515v209%20Family_WS-DISV_SMD_RAISED_ACTUATOR_4181212708xx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/"&gt;https://www.we-online.com/catalog/en/DISV_2_54_SMALL_COMPACT_SMD_WITH_RAISED_ACTUATOR/&lt;/a&gt;&lt;p&gt;

Updated by Yingchun, Shan 2020-01-23&lt;br&gt;
2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="8POLES"/>
</gates>
<devices>
<device name="" package="418121270808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/418121270808.pdf"/>
<attribute name="PART-NUMBER" value="418121270808"/>
<attribute name="PINS" value=" 8 "/>
<attribute name="QTY" value=" 800 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
