<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Tact Switches - WS-TATV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-02-21&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="4301X60507X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
<package name="4301X60437X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
<package name="4304X60737X6">
<description>&lt;b&gt;WS-TATV&lt;/b&gt;&lt;br&gt; THT Washable Tact Switch 12x12 mm</description>
</package>
<package name="4304X60437X6">
<description>&lt;b&gt;WS-TATV&lt;/b&gt;&lt;br&gt; THT Washable Tact Switch 12x12 mm</description>
</package>
<package name="4304X60857X6">
<description>&lt;b&gt;WS-TATV&lt;/b&gt;&lt;br&gt; THT Washable Tact Switch 12x12 mm</description>
</package>
<package name="4301X60707X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
<package name="4301X60957X6">
<description>&lt;B&gt;WS-TATV&lt;/B&gt; &lt;BR&gt;THT Tact Switch 6x6 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-TASX_4P1">
<description>WS-TASX_4P1</description>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="430156050726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60507X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156050726.pdf"/>
<attribute name="H" value="5.0mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156050726"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156050736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60507X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156050736.pdf"/>
<attribute name="H" value="5.0mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156050736"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186050716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60507X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430186050716.pdf"/>
<attribute name="H" value="5.0mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186050716"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156043726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430476073716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60737X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430476073716.pdf"/>
<attribute name="H" value="7.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430476073716"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156043736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156043736.pdf"/>
<attribute name="H" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156043736"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430466073726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60737X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430466073726.pdf"/>
<attribute name="H" value="7.3mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430466073726"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430456073736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60737X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430456073736.pdf"/>
<attribute name="H" value="7.3mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430456073736"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430466043726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430466043726.pdf"/>
<attribute name="H" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430466043726"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430476043716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430476043716.pdf"/>
<attribute name="H" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430476043716"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186043716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430186043716.pdf"/>
<attribute name="H" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186043716"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430456043736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60437X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430456043736.pdf"/>
<attribute name="H" value="4.3mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430456043736"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430476085716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60857X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430476085716.pdf"/>
<attribute name="H" value="8.5mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430476085716"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430466085726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60857X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430466085726.pdf"/>
<attribute name="H" value="8.5mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430466085726"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430456085736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Washable Tact Switch 12x12 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:Yes
&lt;BR&gt;Qty.:50
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Electrical Life:200000 Times; 300000 Times; 500000 Times
&lt;BR&gt;Stroke :0.3 mm
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:Yes


&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61120v209%20Family_WS_TSW_THT_4304x60xx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_12X12_THT_WASHABLE_4304x60xx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4304X60857X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430456085736.pdf"/>
<attribute name="H" value="8.5mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430456085736"/>
<attribute name="QTY" value=" 50 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186070716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60707X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430186070716.pdf"/>
<attribute name="H" value="7.0mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186070716"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156070726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60707X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156070726.pdf"/>
<attribute name="H" value="7.0mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156070726"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156070736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60707X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156070736.pdf"/>
<attribute name="H" value="7.0mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156070736"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430186095716" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60957X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430186095716.pdf"/>
<attribute name="H" value="9.5mm"/>
<attribute name="OPERATION-FORCE" value="160g"/>
<attribute name="PART-NUMBER" value="430186095716"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156095736" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60957X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156095736.pdf"/>
<attribute name="H" value="9.5mm"/>
<attribute name="OPERATION-FORCE" value="360g"/>
<attribute name="PART-NUMBER" value="430156095736"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430156095726" prefix="S" uservalue="yes">
<description>&lt;b&gt;WS-TATV THT Tact Switch 6x6 mm&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Material Properties&lt;/B&gt;
&lt;BR&gt;Cover Material : Stainless Steel
&lt;BR&gt;&lt;BR&gt;
&lt;B&gt;Properties&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Actuator Material:LCP
&lt;BR&gt;Actuator Flammability Rating:UL94 V-0
&lt;BR&gt;Actuator Color:Black; Salmon; White
&lt;BR&gt;Frame Material:PPA
&lt;BR&gt;Frame Flammability Rating:UL94 HB
&lt;BR&gt;Frame Color:Black
&lt;BR&gt;Contact Material:Stainless Steel
&lt;BR&gt;Contact Plating:Silver
&lt;BR&gt;Terminal Material:Copper Alloy
&lt;BR&gt;Terminal Plating:Silver
&lt;BR&gt;VR:12 V (DC)
&lt;BR&gt;Contact Resistance Initial:100 mΩ
&lt;BR&gt;Contact Resistance After Life Test:2 Ω
&lt;BR&gt;RISO:100 MΩ
&lt;BR&gt;Withstanding Voltage:250 V (AC)
&lt;BR&gt;Washable:No
&lt;BR&gt;Qty.:200
&lt;BR&gt;
&lt;BR&gt;
&lt;b&gt;Mechanical Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Stroke  0.25 mm 
&lt;BR&gt;
&lt;BR&gt;&lt;b&gt;General Information&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;Washable:No
&lt;BR&gt;&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Packaging:Bulk

&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o61106v209%20Family_WS_TST_THT_4301x6xxx7x6_pf2.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/"&gt;https://www.we-online.com/catalog/en/TATV_6X6_THT_4301x6xxx7x6/&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated by yingchun,Shan;2020-02-21
&lt;br&gt;2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-TASX_4P1"/>
</gates>
<devices>
<device name="" package="4301X60957X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/430156095726.pdf"/>
<attribute name="H" value="9.5mm"/>
<attribute name="OPERATION-FORCE" value="260g"/>
<attribute name="PART-NUMBER" value="430156095726"/>
<attribute name="QTY" value=" 200 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
