<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Mains Power Lines - WE-CMB HC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021b, 2021-04-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-CMB_HC_TYPE-S">
<description>&lt;b&gt;WE-CMB HC Common Mode Power Line Choke
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Size : Tyoe S, THT, 4pins
&lt;br&gt;L X W X H=18.5mm X 14.5mm X 22mm</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CMB_HC_TYPE-S" prefix="L">
<description>&lt;b&gt; WE-CMB HC Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Broadband filterring due to low capacitance winding technique
&lt;br&gt;High suppression of asymmetrical interferences also at low frequency range
&lt;br&gt;Very compact design
&lt;br&gt;Highest possible rated current by small size
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according to IEC 60938-2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt;Power line in- and output filter
&lt;br&gt;Filtering of devices without any ground connection
&lt;br&gt;Suppression of radio interferences in motors
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;


&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o58849v209%20Family_WE-CMB%20HC.jpg"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o58849v209%20Family_WE-CMB%20HC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-CMB-HC"&gt;https://www.we-online.com/katalog/en/WE-CMB-HC&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2021-04-02&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-CMB_HC_TYPE-S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7448225007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448225007.pdf"/>
<attribute name="IR" value="5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448225007 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="0.7mH"/>
<attribute name="VR" value="250 V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7448226404">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448226404.pdf"/>
<attribute name="IR" value="6.4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448226404 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="0.35mH"/>
<attribute name="VR" value="250 V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7448227005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448227005.pdf"/>
<attribute name="IR" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448227005 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="0.45mH"/>
<attribute name="VR" value="250 V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7448228002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7448228002.pdf"/>
<attribute name="IR" value="8A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7448228002 "/>
<attribute name="RDC" value="6mOhm"/>
<attribute name="VALUE" value="0.175mH"/>
<attribute name="VR" value="250 V (AC)"/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
