<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For DC/DC Converter - WE-PPTM&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-02-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PPTM_1212_L12.6W11.63H3.68">
<description>&lt;b&gt;WE-PPTM Push-Pull Tiny Multi-Output Transformers
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: 1212TB, SMT, 10pins

&lt;br&gt;LXWXH=12.6X11.63X3.68mm</description>
</package>
<package name="WE-PPTM_1212TB_L12.6W11.63H3.99">
<description>&lt;b&gt;WE-PPTM Push-Pull Tiny Multi-Output Transformers
&lt;br&gt;&lt;br&gt;&lt;/b&gt;
Size: 1212, SMT, 10pins

&lt;br&gt;LXWXH=12.6X11.63X1.98mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-PPTM_1212">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-PPTM_1212TB">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PPTM_1212" prefix="T">
<description>&lt;b&gt;WE-PPTM Push-Pull Tiny Multi-Output Transformers

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Small size
&lt;br&gt;Surface mount
&lt;br&gt;Through the board options
&lt;br&gt;Low profile
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;Multiple outputs
&lt;br&gt;Functional insulation

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Isolated interface power supply for CAN, RS-485, RS-422, RS-232, SPI, I2C, lower-power LAN
&lt;br&gt;Industrial automation
&lt;br&gt;Process control
&lt;br&gt;Medical equipment
&lt;br&gt;PLC analog and digital I/O modules
&lt;br&gt;Isolated gate driver power supplies
&lt;br&gt;AC motor drives
&lt;br&gt;Uninterruptible power supplies (UPS)
&lt;br&gt;Solar inverters
&lt;br&gt;Polyphase energy meters
&lt;br&gt;Protection relays and IEDs

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o765174v209%20Family-MID-PPTI-SN6505B-750316668.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o765174v209%20Family-MID-PPTI-SN6505B-750316668.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PPTM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PPTM&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-31&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-PPTM_1212"/>
</gates>
<devices>
<device name="_L12.6W11.63H3.68" package="WE-PPTM_1212_L12.6W11.63H3.68">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_750316016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316016?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="3.68mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="95mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.57:1.14"/>
<attribute name="PART-NUMBER" value=" 750316016 "/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316016 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="12.85V"/>
<attribute name="VOUT2" value="5.7V"/>
<attribute name="VOUT3" value="-5.7V"/>
<attribute name="VOUT4" value="-12.85V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
<technology name="_750316017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316017?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="3.68mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="95mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.17:3:1"/>
<attribute name="PART-NUMBER" value=" 750316017 "/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316017 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="12.85V"/>
<attribute name="VOUT2" value="4.27V"/>
<attribute name="VOUT3" value="-4.27V"/>
<attribute name="VOUT4" value="-12.85V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
<technology name="_750316018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316018?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="3.68mm"/>
<attribute name="IOUT1" value="85mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="85mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:3.14:1.14"/>
<attribute name="PART-NUMBER" value=" 750316018 "/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316018 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="15.7V"/>
<attribute name="VOUT2" value="5.7V"/>
<attribute name="VOUT3" value="-5.7V"/>
<attribute name="VOUT4" value="-15.7V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
<technology name="_750316019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316019?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="3.68mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="95mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.17:3.67:1"/>
<attribute name="PART-NUMBER" value=" 750316019 "/>
<attribute name="SIZE" value=" 1212 "/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316019 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="15.7V"/>
<attribute name="VOUT2" value="4.27V"/>
<attribute name="VOUT3" value="-4.27V"/>
<attribute name="VOUT4" value="-15.7V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PPTM_1212TB" prefix="T">
<description>&lt;b&gt;WE-PPTM Push-Pull Tiny Multi-Output Transformers

&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Small size
&lt;br&gt;Surface mount
&lt;br&gt;Through the board options
&lt;br&gt;Low profile
&lt;br&gt;Operating temp: -40°C to 125°C
&lt;br&gt;Multiple outputs
&lt;br&gt;Functional insulation

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Isolated interface power supply for CAN, RS-485, RS-422, RS-232, SPI, I2C, lower-power LAN
&lt;br&gt;Industrial automation
&lt;br&gt;Process control
&lt;br&gt;Medical equipment
&lt;br&gt;PLC analog and digital I/O modules
&lt;br&gt;Isolated gate driver power supplies
&lt;br&gt;AC motor drives
&lt;br&gt;Uninterruptible power supplies (UPS)
&lt;br&gt;Solar inverters
&lt;br&gt;Polyphase energy meters
&lt;br&gt;Protection relays and IEDs

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o765174v209%20Family-MID-PPTI-SN6505B-750316668.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o765174v209%20Family-MID-PPTI-SN6505B-750316668.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PPTM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PPTM&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2024-01-31&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-PPTM_1212TB"/>
</gates>
<devices>
<device name="_L12.6W11.63H3.99" package="WE-PPTM_1212TB_L12.6W11.63H3.99">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_750316668">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316668?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="1.98mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="95mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.57:1.14"/>
<attribute name="PART-NUMBER" value=" 750316668 "/>
<attribute name="SIZE" value="1212TB"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316668 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="12.85V"/>
<attribute name="VOUT2" value="5.7V"/>
<attribute name="VOUT3" value="-5.7V"/>
<attribute name="VOUT4" value="-12.85V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
<technology name="_750316669">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316669?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="1.98mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="95mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.17:3:1"/>
<attribute name="PART-NUMBER" value=" 750316669 "/>
<attribute name="SIZE" value="1212TB"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316669 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="12.85V"/>
<attribute name="VOUT2" value="4.27V"/>
<attribute name="VOUT3" value="-4.27V"/>
<attribute name="VOUT4" value="-12.85V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
<technology name="_750316670">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316670?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="1.98mm"/>
<attribute name="IOUT1" value="85mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="85mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:3.14:1.14"/>
<attribute name="PART-NUMBER" value=" 750316670 "/>
<attribute name="SIZE" value="1212TB"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316670 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="15.7V"/>
<attribute name="VOUT2" value="5.7V"/>
<attribute name="VOUT3" value="-5.7V"/>
<attribute name="VOUT4" value="-15.7V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
<technology name="_750316671">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316671?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="1.98mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="IOUT4" value="95mA"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="12.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.17:3.67:1"/>
<attribute name="PART-NUMBER" value=" 750316671 "/>
<attribute name="SIZE" value="1212TB"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value=" 750316671 "/>
<attribute name="VIN" value="5 V (DC)"/>
<attribute name="VOLTAGE-TIME" value="8.9Vus"/>
<attribute name="VOUT1" value="15.7V"/>
<attribute name="VOUT2" value="4.27V"/>
<attribute name="VOUT3" value="-4.27V"/>
<attribute name="VOUT4" value="-15.7V"/>
<attribute name="VT" value="3125 V(AC)"/>
<attribute name="WIDTH" value="11.63mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
