<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Power Magnetics - DC/DC Push Pull Transformers - WE-PSPA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-07-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PSPA_1006">
<description>&lt;b&gt;WE-PSPA Push Pull &amp; Gate Drive Transformer
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 1006, SMT, 6pins
&lt;br&gt;LxWxH=10.45x6.73x4.19mm</description>
</package>
<package name="WE-PSPA_1208">
<description>&lt;b&gt;WE-PSPA Push Pull &amp; Gate Drive Transformer
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 1208, SMT, 6pins
&lt;br&gt;LxWxH=12.6x8.3x4.1mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-PSPA_1006">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-PSPA_1208">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PSPA_1006" prefix="T">
<description>&lt;b&gt; WE-PSPA Push Pull &amp; Gate Drive Transformer
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Surface mount
&lt;br&gt;AEC-Q200
&lt;br&gt;Variety of turn ratios
&lt;br&gt;Output voltages from 5 V up to 23 V
&lt;br&gt;Operating temperature:-40 °C up to +125 ºC
&lt;br&gt;Automotive approved

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;As a Gate Drive Transformator
&lt;br&gt;Transformator for Push Pull DC/DC Converter
&lt;br&gt;For isolated interfaces RS 485, CAN
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o718702v209%20family-we-pspa-78931812xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o718702v209%20family-we-pspa-78931812xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PSPA_PUSH_PULL_TRANSFORMER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/components/products/WE-PSPA_PUSH_PULL_TRANSFORMER&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella 2022-12-05&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-PSPA_1006"/>
</gates>
<devices>
<device name="" package="WE-PSPA_1006">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_78931610505">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931610505?ae"/>
<attribute name="IOUT1" value="350mA"/>
<attribute name="L" value="475uH"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.15"/>
<attribute name="PART-NUMBER" value=" 78931610505 "/>
<attribute name="RDC1" value="140ohm"/>
<attribute name="RDC2" value="140ohm"/>
<attribute name="RDC3" value="150ohm"/>
<attribute name="RDC4" value="150ohm"/>
<attribute name="VALUE" value="1:1.15"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="11Vus"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931610512">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931610512?ae"/>
<attribute name="IOUT1" value="150mA"/>
<attribute name="L" value="475uH"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.54"/>
<attribute name="PART-NUMBER" value=" 78931610512 "/>
<attribute name="RDC1" value="165ohm"/>
<attribute name="RDC2" value="165ohm"/>
<attribute name="RDC3" value="335ohm"/>
<attribute name="RDC4" value="335ohm"/>
<attribute name="VALUE" value="1:2.54"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="11Vus"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931610515">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931610515?ae"/>
<attribute name="IOUT1" value="115mA"/>
<attribute name="L" value="475uH"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:3.15"/>
<attribute name="PART-NUMBER" value=" 78931610515 "/>
<attribute name="RDC1" value="155ohm"/>
<attribute name="RDC2" value="155ohm"/>
<attribute name="RDC3" value="635ohm"/>
<attribute name="RDC4" value="635ohm"/>
<attribute name="VALUE" value="1:3.15"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="11Vus"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931610518">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931610518?ae"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="L" value="475uH"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:3.77"/>
<attribute name="PART-NUMBER" value=" 78931610518 "/>
<attribute name="RDC1" value="160ohm"/>
<attribute name="RDC2" value="160ohm"/>
<attribute name="RDC3" value="775ohm"/>
<attribute name="RDC4" value="775ohm"/>
<attribute name="VALUE" value="1:3.77"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="11Vus"/>
<attribute name="VOUT1" value="18V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PSPA_1208" prefix="T">
<description>&lt;b&gt; WE-PSPA Push Pull &amp; Gate Drive Transformer
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Surface mount
&lt;br&gt;AEC-Q200
&lt;br&gt;Variety of turn ratios
&lt;br&gt;Output voltages from 5 V up to 23 V
&lt;br&gt;Operating temperature:-40 °C up to +125 ºC
&lt;br&gt;Automotive approved

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;/b&gt;
&lt;br&gt;As a Gate Drive Transformator
&lt;br&gt;Transformator for Push Pull DC/DC Converter
&lt;br&gt;For isolated interfaces RS 485, CAN
&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o718702v209%20family-we-pspa-78931812xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o718702v209%20family-we-pspa-78931812xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PSPA_PUSH_PULL_TRANSFORMER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle
"&gt;www.we-online.com/components/products/WE-PSPA_PUSH_PULL_TRANSFORMER&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella 2022-12-05&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-PSPA_1208"/>
</gates>
<devices>
<device name="" package="WE-PSPA_1208">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_78931812505">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931812505?ae"/>
<attribute name="IOUT1" value="750mA"/>
<attribute name="L" value="86uH"/>
<attribute name="LS" value="600nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.13"/>
<attribute name="PART-NUMBER" value=" 78931812505 "/>
<attribute name="RDC1" value="55ohm"/>
<attribute name="RDC2" value="55ohm"/>
<attribute name="RDC3" value="60ohm"/>
<attribute name="RDC4" value="60ohm"/>
<attribute name="VALUE" value="1:1.13"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="9.5Vus"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931812512">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931812512?ae"/>
<attribute name="IOUT1" value="310mA"/>
<attribute name="L" value="86uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.5"/>
<attribute name="PART-NUMBER" value=" 78931812512 "/>
<attribute name="RDC1" value="60ohm"/>
<attribute name="RDC2" value="60ohm"/>
<attribute name="RDC3" value="125ohm"/>
<attribute name="RDC4" value="125ohm"/>
<attribute name="VALUE" value="1:2.5"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="9.5Vus"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931812515">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931812515?ae"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="L" value="86uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:3.13"/>
<attribute name="PART-NUMBER" value=" 78931812515 "/>
<attribute name="RDC1" value="60ohm"/>
<attribute name="RDC2" value="60ohm"/>
<attribute name="RDC3" value="230ohm"/>
<attribute name="RDC4" value="230ohm"/>
<attribute name="VALUE" value="1:3.13"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="9.5Vus"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931812518">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931812518?ae"/>
<attribute name="IOUT1" value="210mA"/>
<attribute name="L" value="86uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:3.75"/>
<attribute name="PART-NUMBER" value=" 78931812518 "/>
<attribute name="RDC1" value="60ohm"/>
<attribute name="RDC2" value="60ohm"/>
<attribute name="RDC3" value="280ohm"/>
<attribute name="RDC4" value="280ohm"/>
<attribute name="VALUE" value="1:3.75"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="9.5Vus"/>
<attribute name="VOUT1" value="18V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
<technology name="_78931812523">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78931812523?ae"/>
<attribute name="IOUT1" value="165mA"/>
<attribute name="L" value="86uH"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:4.75"/>
<attribute name="PART-NUMBER" value=" 78931812523 "/>
<attribute name="RDC1" value="65ohm"/>
<attribute name="RDC2" value="65ohm"/>
<attribute name="RDC3" value="350ohm"/>
<attribute name="RDC4" value="350ohm"/>
<attribute name="VALUE" value="1:4.75"/>
<attribute name="VIN" value="5V"/>
<attribute name="VOLTAGE-TIME" value="9.5Vus"/>
<attribute name="VOUT1" value="23V"/>
<attribute name="VT" value="2500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
