<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - Optocoupler - WL-OCPT&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022b, 2022-11-11&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-OCPT_DIP4_S-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 4 S-Type, SMT, 4pins</description>
</package>
<package name="WL-OCPT_DIP4_STANDARD">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 4 Standard, THT, 4pins</description>
</package>
<package name="WL-OCPT_DIP4_M-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 4 M-Type, THT, 4pins</description>
</package>
<package name="WL-OCPT_DIP4_SL-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 4 SL-Type, SMT, 4pins</description>
</package>
<package name="WL-OCPT_DIP4_SLM-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor
 
&lt;/b&gt;&lt;br&gt;Size : DIP 4 SLM-Type, SMT, 4pins</description>
</package>
<package name="WL-OCPT_SOP4">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : SOP4, SMT, 4pins</description>
</package>
<package name="WL-OCPT_DIP8_M-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 8 M-Type, THT, 8pins</description>
</package>
<package name="WL-OCPT_DIP8_STANDARD">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 8 STANDARD, THT, 8pins</description>
</package>
<package name="WL-OCPT_DIP8_SL-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 8 SL-Type, SMT, 8pins</description>
</package>
<package name="WL-OCPT_DIP8_S-TYPE">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : DIP 8 S-Type, SMT, 8pins</description>
</package>
<package name="WL-OCPT_LSOP4">
<description>&lt;b&gt; WL-OCPT Optocoupler Phototransistor

&lt;/b&gt;&lt;br&gt;Size : LSOP4, SMT, 4pins</description>
</package>
</packages>
<symbols>
<symbol name="WL-OCPT_SERIES_814">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_356">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_827">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_817">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_357">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_101X">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_354">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WL-OCPT_SERIES_816">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-OCPT_SERIES_814" prefix="Q">
<description>&lt;b&gt; WL-OCPT DIP-4
&lt;br&gt;Series 814  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage 
&lt;br&gt;Good stability of inner isolation 
&lt;br&gt;Stable CTR in full operation 
&lt;br&gt;Different CTR binnings available 
&lt;br&gt;High Collector-Emitter Voltage 
&lt;br&gt;Fast switching times 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o198226v209%20WL-OCPT_DIP4_814_Standard_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o198226v209%20WL-OCPT_DIP4_814_Standard_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_DIP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_DIP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_814"/>
</gates>
<devices>
<device name="_DIP4_M-TYPE" package="WL-OCPT_DIP4_M-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140814241010">
<attribute name="CTR-MAX" value="300%"/>
<attribute name="CTR-MIN" value="20%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814241010?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140814241010"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814241010"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140814241110">
<attribute name="CTR-MAX" value="150%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814241110?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140814241110"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814241110"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SL-TYPE" package="WL-OCPT_DIP4_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140814243000">
<attribute name="CTR-MAX" value="300%"/>
<attribute name="CTR-MIN" value="20%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814243000?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140814243000"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814243000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140814243100">
<attribute name="CTR-MAX" value="150%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814243100?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140814243100"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814243100"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_S-TYPE" package="WL-OCPT_DIP4_S-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140814242000">
<attribute name="CTR-MAX" value="300%"/>
<attribute name="CTR-MIN" value="20%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814242000?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140814242000"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814242000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140814242100">
<attribute name="CTR-MAX" value="150%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814242100?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140814242100"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814242100"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_STANDARD" package="WL-OCPT_DIP4_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140814240010">
<attribute name="CTR-MAX" value="300%"/>
<attribute name="CTR-MIN" value="20%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814240010?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140814240010"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814240010"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140814240110">
<attribute name="CTR-MAX" value="150%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140814240110?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140814240110"/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value="140814240110"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_817" prefix="Q">
<description>&lt;b&gt; WL-OCPT DIP-4
&lt;br&gt;Series 817  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage 
&lt;br&gt;Good stability of inner isolation 
&lt;br&gt;Stable CTR in full operation 
&lt;br&gt;Different CTR binnings available 
&lt;br&gt;High Collector-Emitter Voltage 
&lt;br&gt;Fast switching times 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o198226v209%20WL-OCPT_DIP4_814_Standard_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o198226v209%20WL-OCPT_DIP4_814_Standard_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_DIP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_DIP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_817"/>
</gates>
<devices>
<device name="_DIP4_M-TYPE" package="WL-OCPT_DIP4_M-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140817141010">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817141010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817141010"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817141010"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817141110">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817141110?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817141110"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817141110"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817141210">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817141210?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817141210"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817141210"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817141310">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817141310?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817141310"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817141310"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817141410">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817141410?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817141410"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817141410"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SLM-TYPE" package="WL-OCPT_DIP4_SLM-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140817144000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817144000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817144000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817144000"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817144100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817144100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817144100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817144100"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817144200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817144200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817144200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817144200"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817144300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817144300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817144300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817144300"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817144400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817144400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817144400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817144400"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SL-TYPE" package="WL-OCPT_DIP4_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140817143000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817143000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817143000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817143000"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817143100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817143100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817143100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817143100"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817143200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817143200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817143200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817143200"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817143300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817143300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817143300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817143300"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817143400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817143400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817143400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817143400"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_S-TYPE" package="WL-OCPT_DIP4_S-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140817142000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817142000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817142000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817142000"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817142100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817142100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817142100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817142100"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817142200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817142200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817142200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817142200"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817142300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817142300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817142300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817142300"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817142400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817142400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140817142400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817142400"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_STANDARD" package="WL-OCPT_DIP4_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140817140010">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817140010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817140010"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817140010"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817140110">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817140110?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817140110"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817140110"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817140210">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817140210?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817140210"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817140210"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817140310">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817140310?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817140310"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817140310"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140817140410">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140817140410?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140817140410"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140817140410"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_816" prefix="Q">
<description>&lt;b&gt; WL-OCPT DIP-4
&lt;br&gt;Series 816  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage 
&lt;br&gt;Good stability of inner isolation 
&lt;br&gt;Stable CTR in full operation 
&lt;br&gt;Different CTR binnings available 
&lt;br&gt;High Collector-Emitter Voltage 
&lt;br&gt;Fast switching times 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o198226v209%20WL-OCPT_DIP4_814_Standard_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o198226v209%20WL-OCPT_DIP4_814_Standard_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_DIP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_DIP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_816"/>
</gates>
<devices>
<device name="_DIP4_M-TYPE" package="WL-OCPT_DIP4_M-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140816141010">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816141010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 140816141010 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140816141010 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816141110">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816141110?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816141110"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816141110"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816141210">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816141210?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816141210"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816141210"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816141310">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816141310?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816141310"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816141310"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816141410">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816141410?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816141410"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816141410"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SLM-TYPE" package="WL-OCPT_DIP4_SLM-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140816144000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816144000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140816144000 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140816144000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816144100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816144100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816144100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816144100"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816144200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816144200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816144200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816144200"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816144300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816144300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816144300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816144300"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816144400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816144400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816144400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816144400"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_SL-TYPE" package="WL-OCPT_DIP4_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140816143000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816143000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140816143000 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140816143000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816143100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816143100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816143100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816143100"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816143200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816143200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816143200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816143200"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816143300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816143300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816143300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816143300"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816143400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816143400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816143400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816143400"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_STANDARD" package="WL-OCPT_DIP4_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140816140010">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816140010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 140816140010 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140816140010 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816140110">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816140110?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816140110"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816140110"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816140210">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816140210?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 140816140210 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140816140210 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816140310">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816140310?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816140310"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816140310"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816140410">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816140410?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="140816140410"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816140410"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP4_S-TYPE" package="WL-OCPT_DIP4_S-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140816142000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816142000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140816142000 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140816142000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816142100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816142100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816142100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816142100"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816142200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816142200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816142200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816142200"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816142300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816142300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816142300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816142300"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140816142400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140816142400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140816142400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140816142400"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_356" prefix="Q">
<description>&lt;b&gt;WL-OCPT SOP-4 
&lt;br&gt;Series 356  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation temperature range
&lt;br&gt; Different CTR binnings available
&lt;br&gt; High Collector-Emitter voltage
&lt;br&gt; Fast switching times
 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o198228v209%20WL-OCPT_SOP_354_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o198228v209%20WL-OCPT_SOP_354_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_SOP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_SOP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_356"/>
</gates>
<devices>
<device name="" package="WL-OCPT_SOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140356145000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140356145000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140356145000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140356145000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140356145100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140356145100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140356145100"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140356145100"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140356145200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140356145200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140356145200 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140356145200 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140356145300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140356145300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140356145300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140356145300"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140356145400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140356145400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140356145400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140356145400"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_354" prefix="Q">
<description>&lt;b&gt;WL-OCPT SOP-4 
&lt;br&gt;Series 354  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation temperature range
&lt;br&gt; Different CTR binnings available
&lt;br&gt; High Collector-Emitter voltage
&lt;br&gt; Fast switching times
 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o198228v209%20WL-OCPT_SOP_354_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o198228v209%20WL-OCPT_SOP_354_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_SOP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_SOP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_354"/>
</gates>
<devices>
<device name="" package="WL-OCPT_SOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140354245000">
<attribute name="CTR-MAX" value="300%"/>
<attribute name="CTR-MIN" value="20%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140354245000?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140354245000 "/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140354245000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140354245100">
<attribute name="CTR-MAX" value="150%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140354245100?ae"/>
<attribute name="IF" value="±60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140354245100 "/>
<attribute name="TC-CTR" value="IF = +/-1 mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140354245100 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_357" prefix="Q">
<description>&lt;b&gt;WL-OCPT SOP-4 
&lt;br&gt;Series 357
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation temperature range
&lt;br&gt; Different CTR binnings available
&lt;br&gt; High Collector-Emitter voltage
&lt;br&gt; Fast switching times
 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o198228v209%20WL-OCPT_SOP_354_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o198228v209%20WL-OCPT_SOP_354_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_SOP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_SOP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_357"/>
</gates>
<devices>
<device name="" package="WL-OCPT_SOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140357145000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140357145000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140357145000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140357145000"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140357145100">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140357145100?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140357145100 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140357145100 "/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140357145200">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140357145200?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140357145200"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140357145200"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140357145300">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140357145300?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140357145300"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140357145300"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
<technology name="_140357145400">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140357145400?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140357145400"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140357145400"/>
<attribute name="VCE" value="35V"/>
<attribute name="VISO" value="3750(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_827" prefix="Q">
<description>&lt;b&gt; WL-OCPT DIP-8
&lt;br&gt;Series 827  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;DIP-8 series 827
&lt;br&gt;High isolation voltage
&lt;br&gt;Good stability of inner isolation
&lt;br&gt;Stable CTR in full operation temperature range
&lt;br&gt;Different CTR binnings available
&lt;br&gt;High Collector-Emitter voltage
&lt;br&gt;Fast switching times

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power supplies and chargers
&lt;br&gt;Computer and microprocessors
&lt;br&gt;Office equipment
&lt;br&gt;Instrumental applications and machines
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o707827v209%20WL-OCPT%20DIP8.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o707827v209%20WL-OCPT%20DIP8.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_DIP_8/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_DIP_8&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2022-11-11
&lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_827"/>
</gates>
<devices>
<device name="_DIP8_M-TYPE" package="WL-OCPT_DIP8_M-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="_140827181010">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140827181010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 140827181010 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140827181010 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP8_SL-TYPE" package="WL-OCPT_DIP8_SL-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="_140827183000">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140827183000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140827183000 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140827183000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP8_STANDARD" package="WL-OCPT_DIP8_STANDARD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="_140827180010">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140827180010?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 140827180010 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140827180010 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
<device name="_DIP8_S-TYPE" package="WL-OCPT_DIP8_S-TYPE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="_140827182000">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140827182000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140827182000 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140827182000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-OCPT_SERIES_101X" prefix="Q">
<description>&lt;b&gt;WL-OCPT LSOP-4
&lt;br&gt;Series 101x  
&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Characteristics
&lt;br&gt;&lt;/b&gt;&lt;br&gt;High isolation voltage
&lt;br&gt; Good stability of inner isolation
&lt;br&gt; Stable CTR in full operation temperature range
&lt;br&gt; Different CTR binnings available
&lt;br&gt; High Collector-Emitter voltage
&lt;br&gt; Fast switching times
 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;
 
&lt;b&gt;Applications
&lt;br&gt;&lt;/b&gt;&lt;br&gt;Power Supply, charger 
&lt;br&gt;Computers &amp; Microprocessors 
&lt;br&gt;Office equipment 
&lt;br&gt;Instrumental applications, machines 
&lt;br&gt;Ammeter, Smart Meter 

&lt;/b&gt;&lt;br&gt;
&lt;/b&gt;&lt;br&gt;            
&lt;br&gt;&lt;a href="https://www.we-online.de/katalog/media/o198230v209%20WL-OCPT_LSOP4_101x_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.de/katalog/media/o198230v209%20WL-OCPT_LSOP4_101x_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-OCPT_PACKAGE_LSOP-4/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-OCPT_PACKAGE_LSOP-4&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2022-06-21
 &lt;br&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-OCPT_SERIES_101X"/>
</gates>
<devices>
<device name="" package="WL-OCPT_LSOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_140100146000">
<attribute name="CTR-MAX" value="600%"/>
<attribute name="CTR-MIN" value="300%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140100146000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 140100146000 "/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value=" 140100146000 "/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140105146000">
<attribute name="CTR-MAX" value="150%"/>
<attribute name="CTR-MIN" value="50%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140105146000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140105146000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140105146000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140106146000">
<attribute name="CTR-MAX" value="300%"/>
<attribute name="CTR-MIN" value="100%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140106146000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140106146000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140106146000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140107146000">
<attribute name="CTR-MAX" value="160%"/>
<attribute name="CTR-MIN" value="80%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140107146000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140107146000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140107146000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140108146000">
<attribute name="CTR-MAX" value="260%"/>
<attribute name="CTR-MIN" value="130%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140108146000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140108146000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140108146000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
<technology name="_140109146000">
<attribute name="CTR-MAX" value="400%"/>
<attribute name="CTR-MIN" value="200%"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/140109146000?ae"/>
<attribute name="IF" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="140109146000"/>
<attribute name="TC-CTR" value="IF = 5mA,VCE = 5 V"/>
<attribute name="VALUE" value="140109146000"/>
<attribute name="VCE" value="80V"/>
<attribute name="VISO" value="5000(V(RMS))"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
