<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - Singnal LEDs &amp; Horticulture LEDs - TOP LED  - WL-SMTW&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022b, 2022-11-09&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SMTW_3020">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:3020, SMT, 2pins
&lt;br&gt;3x2x1.3mm(LXWXH)</description>
</package>
<package name="WL-SMTW_3528_ADV">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:3528 advance, SMT, 2pins
&lt;br&gt;3.5x2.8x1.9mm(LXWXH)</description>
</package>
<package name="WL-SMTW_3528">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:3528, SMT, 2pins
&lt;br&gt;3.5x2.8x1.9mm(LXWXH)</description>
</package>
<package name="WL-SMTW_2835">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:2835, SMT, 2pins
&lt;br&gt;3.5x2.8x0.8mm(LXWXH)</description>
</package>
<package name="WL-SMTW_2214">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:2214, SMT, 2pins
&lt;br&gt;2x1.4x1.31mm(LXWXH)</description>
</package>
<package name="WL-SMTW_5050">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:5050, SMT, 6pins
&lt;br&gt;5.4x5x1.6mm(LXWXH)</description>
</package>
<package name="WL-SMTW_3528_PLCC4">
<description>&lt;B&gt;WL-SMTW SMT Mono-color TOP LED Waterclear &lt;/B&gt;
&lt;br&gt;&lt;br&gt;Size:3528 PLCC4, SMT, 4pins
&lt;br&gt;3.5x2.8x1.9mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SMTW_1+">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="WL-SMTW_2+">
<description>LED</description>
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="WL-SMTW_150141XX73130">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WL-SMTW_150141XX73140">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WL-SMTW_2214">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="WL-SMTW_5050">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SMTW_3020" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_2+"/>
</gates>
<devices>
<device name="" package="WL-SMTW_3020">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_150302BS73100">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150302BS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="280mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150302BS73100"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150302BS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150302GS73100">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150302GS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="525nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.5V"/>
<attribute name="LUMINOUS-INTENSITY" value="1200mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150302GS73100"/>
<attribute name="PEAK-WAVELENGTH" value="515nm"/>
<attribute name="VALUE" value="150302GS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150302RS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150302RS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="180mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150302RS73100"/>
<attribute name="PEAK-WAVELENGTH" value="630nm"/>
<attribute name="VALUE" value="150302RS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150302VS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150302VS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="570nm"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="70mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150302VS73100"/>
<attribute name="PEAK-WAVELENGTH" value="572nm"/>
<attribute name="VALUE" value="150302VS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150302YS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150302YS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="250mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150302YS73100"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150302YS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_3528_ADV" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_1+"/>
</gates>
<devices>
<device name="" package="WL-SMTW_3528_ADV">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_150141AS73113">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141AS73113?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="609nm"/>
<attribute name="EMITTING-COLOR" value="Amber"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="800mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141AS73113"/>
<attribute name="PEAK-WAVELENGTH" value="615nm"/>
<attribute name="VALUE" value="150141AS73113"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141BS73113">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141BS73113?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="467nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="530mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141BS73113"/>
<attribute name="PEAK-WAVELENGTH" value="463nm"/>
<attribute name="VALUE" value="150141BS73113"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141GS73113">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141GS73113?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="522nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3V"/>
<attribute name="LUMINOUS-INTENSITY" value="2500mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141GS73113"/>
<attribute name="PEAK-WAVELENGTH" value="517nm"/>
<attribute name="VALUE" value="150141GS73113"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141RS73113">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RS73113?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="620nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="900mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141RS73113"/>
<attribute name="PEAK-WAVELENGTH" value="629nm"/>
<attribute name="VALUE" value="150141RS73113"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YS73113">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YS73113?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="1000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141YS73113"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150141YS73113"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_2835" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_1+"/>
</gates>
<devices>
<device name="" package="WL-SMTW_2835">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_150283BS73103">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283BS73103?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="467nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-FLUX" value="12lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283BS73103"/>
<attribute name="PEAK-WAVELENGTH" value="463nm"/>
<attribute name="VALUE" value="150283BS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150283GS73103">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283GS73103?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="522nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3V"/>
<attribute name="LUMINOUS-FLUX" value="40lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283GS73103"/>
<attribute name="PEAK-WAVELENGTH" value="517nm"/>
<attribute name="VALUE" value="150283GS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150283RS73103">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283RS73103?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="620nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-FLUX" value="19lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283RS73103"/>
<attribute name="PEAK-WAVELENGTH" value="629nm"/>
<attribute name="VALUE" value="150283RS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150283YS73103">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283YS73103?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="LUMINOUS-FLUX" value="18lm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283YS73103"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150283YS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_2214_A" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_2+"/>
</gates>
<devices>
<device name="" package="WL-SMTW_2214">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_150224BS73100A">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224BS73100A?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="320mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224BS73100A"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150224BS73100A"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224GS73100A">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224GS73100A?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="525nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.1V"/>
<attribute name="LUMINOUS-INTENSITY" value="1500mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224GS73100A"/>
<attribute name="PEAK-WAVELENGTH" value="515nm"/>
<attribute name="VALUE" value="150224GS73100A"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224RS73100A">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224RS73100A?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="350mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224RS73100A"/>
<attribute name="PEAK-WAVELENGTH" value="630nm"/>
<attribute name="VALUE" value="150224RS73100A"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224VS73100A">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224VS73100A?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="570nm"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="70mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224VS73100A"/>
<attribute name="PEAK-WAVELENGTH" value="572nm"/>
<attribute name="VALUE" value="150224VS73100A"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224YS73100A">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224YS73100A?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="330mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224YS73100A"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150224YS73100A"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_2835_HORTICULTURE" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL_SMTW_HORTICULTURE/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_1+"/>
</gates>
<devices>
<device name="" package="WL-SMTW_2835">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="_150283DS73103">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283DS73103?ae"/>
<attribute name="EMITTING-COLOR" value="Deep Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283DS73103"/>
<attribute name="PEAK-WAVELENGTH" value="450nm"/>
<attribute name="RADIANT-FLUX" value="250mW"/>
<attribute name="VALUE" value="150283DS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150283FS73103">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283FS73103?ae"/>
<attribute name="EMITTING-COLOR" value="Far Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283FS73103"/>
<attribute name="PEAK-WAVELENGTH" value="730nm"/>
<attribute name="RADIANT-FLUX" value="110mW"/>
<attribute name="VALUE" value="150283FS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150283HS73103">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150283HS73103?ae"/>
<attribute name="EMITTING-COLOR" value="Hyper Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.2V"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150283HS73103"/>
<attribute name="PEAK-WAVELENGTH" value="660nm"/>
<attribute name="RADIANT-FLUX" value="120mW"/>
<attribute name="VALUE" value="150283HS73103"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_3528" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_2+"/>
</gates>
<devices>
<device name="" package="WL-SMTW_3528">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_150141AS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141AS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="605nm"/>
<attribute name="EMITTING-COLOR" value="Amber"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="330mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141AS73100"/>
<attribute name="PEAK-WAVELENGTH" value="610nm"/>
<attribute name="VALUE" value="150141AS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141BS73100">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141BS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="270mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141BS73100"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150141BS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141GS73100">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141GS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="525nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.1V"/>
<attribute name="LUMINOUS-INTENSITY" value="1000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141GS73100"/>
<attribute name="PEAK-WAVELENGTH" value="515nm"/>
<attribute name="VALUE" value="150141GS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141RS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="300mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141RS73100"/>
<attribute name="PEAK-WAVELENGTH" value="630nm"/>
<attribute name="VALUE" value="150141RS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141VS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141VS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="570nm"/>
<attribute name="EMITTING-COLOR" value="Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="90mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141VS73100"/>
<attribute name="PEAK-WAVELENGTH" value="572nm"/>
<attribute name="VALUE" value="150141VS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="260mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141YS73100"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150141YS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_2214" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_2214"/>
</gates>
<devices>
<device name="" package="WL-SMTW_2214">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_150224AS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224AS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="605nm"/>
<attribute name="EMITTING-COLOR" value="Amber"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="210mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224AS73100"/>
<attribute name="PEAK-WAVELENGTH" value="609nm"/>
<attribute name="VALUE" value="150224AS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224BS73100">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224BS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="456nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3V"/>
<attribute name="LUMINOUS-INTENSITY" value="220mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224BS73100"/>
<attribute name="PEAK-WAVELENGTH" value="452nm"/>
<attribute name="VALUE" value="150224BS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224GS73100">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224GS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="528nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3V"/>
<attribute name="LUMINOUS-INTENSITY" value="1200mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224GS73100"/>
<attribute name="PEAK-WAVELENGTH" value="519nm"/>
<attribute name="VALUE" value="150224GS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224SS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224SS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="636nm"/>
<attribute name="EMITTING-COLOR" value="Super Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.1V"/>
<attribute name="LUMINOUS-INTENSITY" value="130mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224SS73100"/>
<attribute name="PEAK-WAVELENGTH" value="652nm"/>
<attribute name="VALUE" value="150224SS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150224YS73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150224YS73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="586nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2.1V"/>
<attribute name="LUMINOUS-INTENSITY" value="290mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150224YS73100"/>
<attribute name="PEAK-WAVELENGTH" value="589nm"/>
<attribute name="VALUE" value="150224YS73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_3528_150141XX73130" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_150141XX73130"/>
</gates>
<devices>
<device name="" package="WL-SMTW_3528_PLCC4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_150141BS73130">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141BS73130?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="1000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141BS73130"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150141BS73130"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141GS73130">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141GS73130?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="520nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="5000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141GS73130"/>
<attribute name="PEAK-WAVELENGTH" value="515nm"/>
<attribute name="VALUE" value="150141GS73130"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141RS73130">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RS73130?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="620nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.4V"/>
<attribute name="LUMINOUS-INTENSITY" value="3000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141RS73130"/>
<attribute name="PEAK-WAVELENGTH" value="630nm"/>
<attribute name="VALUE" value="150141RS73130"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YS73130">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YS73130?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2.4V"/>
<attribute name="LUMINOUS-INTENSITY" value="2000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141YS73130"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150141YS73130"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_3528_150141XX73140" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-06-21&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_150141XX73140"/>
</gates>
<devices>
<device name="" package="WL-SMTW_3528_PLCC4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_150141BS73140">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141BS73140?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="1000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141BS73140"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150141BS73140"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141GS73140">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141GS73140?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="520nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.2V"/>
<attribute name="LUMINOUS-INTENSITY" value="5000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141GS73140"/>
<attribute name="PEAK-WAVELENGTH" value="515nm"/>
<attribute name="VALUE" value="150141GS73140"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141RS73140">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RS73140?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="620nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2.4V"/>
<attribute name="LUMINOUS-INTENSITY" value="3000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141RS73140"/>
<attribute name="PEAK-WAVELENGTH" value="630nm"/>
<attribute name="VALUE" value="150141RS73140"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YS73140">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YS73140?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2.4V"/>
<attribute name="LUMINOUS-INTENSITY" value="2000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150141YS73140"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150141YS73140"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SMTW_5050" prefix="D">
<description>&lt;B&gt; WL-SMTW SMT Mono-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;Slim 
&lt;br&gt;Miniature size 
&lt;br&gt;Flexibility in design 
&lt;br&gt;Top view 
&lt;br&gt;LED PLCC 2 white package 
&lt;br&gt;Compact package outline, ideal for miniature applications 
&lt;br&gt;Variety of colors 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Signage and indirect illumination 
&lt;br&gt;Flat lamp 
&lt;br&gt;Indicator and backlight in telecommunication 
&lt;br&gt;Consumer application: dash-board, telephone or A/V equipments 
&lt;br&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Optical indicators 
&lt;br&gt;Indoor and outdoor displays 
&lt;br&gt;Scanner 
&lt;br&gt;Backlight in LCD, cellular phones, switches, keys, displays 
&lt;br&gt;lluminated advertising, panel 
&lt;br&gt;Lighting device: indicator, general lighting 
&lt;br&gt;Camera flash, hand carrier flash 
&lt;br&gt;Coupling into light guides 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14908v209%20WL-SMTW_150285BSxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SMTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SMTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2022-11-09&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SMTW_5050"/>
</gates>
<devices>
<device name="" package="WL-SMTW_5050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_150505BS73300">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150505BS73300?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="470nm"/>
<attribute name="EMITTING-COLOR" value="Blue"/>
<attribute name="FORWARD-VOLTAGE" value="3.3V"/>
<attribute name="LUMINOUS-INTENSITY" value="1000mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150505BS73300"/>
<attribute name="PEAK-WAVELENGTH" value="465nm"/>
<attribute name="VALUE" value="150505BS73300"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150505GS73300">
<attribute name="CHIP-TECHNOLOGY" value="InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150505GS73300?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="525nm"/>
<attribute name="EMITTING-COLOR" value="Green"/>
<attribute name="FORWARD-VOLTAGE" value="3.1V"/>
<attribute name="LUMINOUS-INTENSITY" value="4300mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150505GS73300"/>
<attribute name="PEAK-WAVELENGTH" value="515nm"/>
<attribute name="VALUE" value="150505GS73300"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150505RS73300">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150505RS73300?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm"/>
<attribute name="EMITTING-COLOR" value="Red"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="2300mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150505RS73300"/>
<attribute name="PEAK-WAVELENGTH" value="630nm"/>
<attribute name="VALUE" value="150505RS73300"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150505YS73300">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150505YS73300?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm"/>
<attribute name="EMITTING-COLOR" value="Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="LUMINOUS-INTENSITY" value="2400mcd"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150505YS73300"/>
<attribute name="PEAK-WAVELENGTH" value="592nm"/>
<attribute name="VALUE" value="150505YS73300"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
