<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Modules(MagI3C Series) - Isolated Converter - MagI³C-FISM &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-11-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WPME-FISM_SIP-7_L19.6W7.05H10.2">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-7, THT, 4pins
&lt;br&gt;LXWXH = 19.6X7.05X10.2mm</description>
</package>
<package name="WPME-FISM_SIP-7_1779205241">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-7, THT, 4pins
&lt;br&gt;LXWXH = 19.6X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-7_L19.65W6H10.16">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-7, THT, 4pins
&lt;br&gt;LXWXH = 19.65X6X10.16mm</description>
</package>
<package name="WPME-FISM_SMT-8_L13.2W11.4H7.25">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SMT-8, THT, 5pins
&lt;br&gt;LXWXH = 13.2X11.4X7.25mm</description>
</package>
<package name="WPME-FISM_SIP-7_L19.65W7.05H10.16">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-7, THT, 4pins
&lt;br&gt;LXWXH = 19.65X7.05X10.16mm</description>
</package>
<package name="WPME-FISM_SMT-8_L12.75W10.7H6.95">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SMT-8, THT, 5pins
&lt;br&gt;LXWXH = 12.75X10.7X6.95mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769205141">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SMT-8, THT, 5pins
&lt;br&gt;LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SMT-8_1769205241">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SMT-8, THT, 5pins
&lt;br&gt;LXWXH = 12.7X11.05X6.25mm</description>
</package>
<package name="WPME-FISM_SIP-4_L11.5W6H10">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-4, THT, 4pins
&lt;br&gt;LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_L11.6W6H10.16">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-4, THT, 4pins
&lt;br&gt;LXWXH = 11.6X6X10.16mm</description>
</package>
<package name="WPME-FISM_SIP-4_L11.6W7.55H10.16">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-4, THT, 4pins
&lt;br&gt;LXWXH = 11.6X7.55X10.16mm</description>
</package>
<package name="WPME-FISM_SIP-4_1779205211">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-4, THT, 4pins
&lt;br&gt;LXWXH = 11.5X6X10mm</description>
</package>
<package name="WPME-FISM_SIP-4_1779205111">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP Module
&lt;br&gt;&lt;/b&gt;Size : SIP-4, THT, 4pins
&lt;br&gt;LXWXH = 11.5X6X10mm</description>
</package>
</packages>
<symbols>
<symbol name="WPME-FISM_SIP-7">
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="-VOUT" direction="out"/>
<pin name="+VOUT" direction="out"/>
</symbol>
<symbol name="WPME-FISM_SMT-8">
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="-VOUT" direction="out"/>
<pin name="+VOUT" direction="out"/>
</symbol>
<symbol name="WPME-FISM_SIP-4">
<pin name="-VIN" direction="in"/>
<pin name="+VIN" direction="in"/>
<pin name="-VOUT" direction="out"/>
<pin name="+VOUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WPME-FISM_SIP-7" prefix="U">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP / SMT Module&lt;br&gt;
Unregulated output voltage&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt;
&lt;/B&gt;&lt;br&gt;Simple design (no transformer design know how required)
&lt;br&gt;Leaded through-hole package for easy manufacturing and prototyping
&lt;br&gt;Stand-alone solution (CIN and COUT integrated, no external components)
&lt;br&gt;Simple functional isolation for overvoltage protection, avoiding ground loops, ground shift and noise in signal path or sensor systems
&lt;br&gt;Industrial standard package and pin configuration
&lt;br&gt;Low conducted and radiated EMI (compliant to EN55022 class B)
&lt;br&gt;UL60950 certified
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;&lt;/B&gt;Data acquisition
&lt;br&gt;Test and measurement systems
&lt;br&gt;Interface and microcontroller supply
&lt;br&gt;Industrial control
&lt;br&gt;
&lt;br&gt;

&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84919v209%20Family-Magic-FISM-1779205x11-1779205x41-17694051.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84919v209%20Family-Magic-FISM-1779205x11-1779205x41-17694051.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-FISM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-FISM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-05
&lt;br&gt;&lt;/b&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-FISM_SIP-7"/>
</gates>
<devices>
<device name="_L19.65W6H10.16" package="WPME-FISM_SIP-7_L19.65W6H10.16">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="_1779205141">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779205141?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="19.65mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779205141 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_1779205341">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779205341?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="19.65mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779205341 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L19.6W7.05H10.2" package="WPME-FISM_SIP-7_L19.6W7.05H10.2">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="_177920514">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/177920514?ae"/>
<attribute name="HEIGHT" value="10.2mm"/>
<attribute name="LENGTH" value="19.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 177920514 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="4000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
<technology name="_177920524">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/177920524?ae"/>
<attribute name="HEIGHT" value="10.2mm"/>
<attribute name="LENGTH" value="19.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 177920524 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="4000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
</technologies>
</device>
<device name="_L19.65W7.05H10.16" package="WPME-FISM_SIP-7_L19.65W7.05H10.16">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="_1779405141">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779405141?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="19.65mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779405141 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
<technology name="_1779405241">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779405241?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="19.65mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779405241 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
<technology name="_1779405341">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779405341?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="19.65mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779405341 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
</technologies>
</device>
<device name="_1779205241" package="WPME-FISM_SIP-7_1779205241">
<connects>
<connect gate="G$1" pin="+VIN" pad="1"/>
<connect gate="G$1" pin="+VOUT" pad="7"/>
<connect gate="G$1" pin="-VIN" pad="2"/>
<connect gate="G$1" pin="-VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779205241?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="19.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779205241 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-7"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WPME-FISM_SMT-8" prefix="U">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP / SMT Module&lt;br&gt;
Unregulated output voltage&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt;
&lt;/B&gt;&lt;br&gt;Simple design (no transformer design know how required)
&lt;br&gt;Leaded through-hole package for easy manufacturing and prototyping
&lt;br&gt;Stand-alone solution (CIN and COUT integrated, no external components)
&lt;br&gt;Simple functional isolation for overvoltage protection, avoiding ground loops, ground shift and noise in signal path or sensor systems
&lt;br&gt;Industrial standard package and pin configuration
&lt;br&gt;Low conducted and radiated EMI (compliant to EN55022 class B)
&lt;br&gt;UL60950 certified
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;&lt;/B&gt;Data acquisition
&lt;br&gt;Test and measurement systems
&lt;br&gt;Interface and microcontroller supply
&lt;br&gt;Industrial control
&lt;br&gt;
&lt;br&gt;

&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84919v209%20Family-Magic-FISM-1779205x11-1779205x41-17694051.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84919v209%20Family-Magic-FISM-1779205x11-1779205x41-17694051.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-FISM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-FISM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-05
&lt;br&gt;&lt;/b&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-FISM_SMT-8"/>
</gates>
<devices>
<device name="_L12.75W10.7H6.95" package="WPME-FISM_SMT-8_L12.75W10.7H6.95">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="_176861512">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/176861512?ae"/>
<attribute name="HEIGHT" value="6.7mm"/>
<attribute name="LENGTH" value="12.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 176861512 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 15Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="2000V"/>
<attribute name="VOUT" value="15V"/>
<attribute name="WIDTH" value="10.7mm"/>
</technology>
<technology name="_176881212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/176881212?ae"/>
<attribute name="HEIGHT" value="6.7mm"/>
<attribute name="LENGTH" value="12.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 176881212 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 12Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="2000V"/>
<attribute name="VOUT" value="12V"/>
<attribute name="WIDTH" value="10.7mm"/>
</technology>
<technology name="_176920502">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/176920502?ae"/>
<attribute name="HEIGHT" value="6.7mm"/>
<attribute name="LENGTH" value="12.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 176920502 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.97 - 3.63Vin, 5Vout"/>
<attribute name="VIN" value="2.97 - 3.63V"/>
<attribute name="VISO" value="2000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="10.7mm"/>
</technology>
<technology name="_176920512">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/176920512?ae"/>
<attribute name="HEIGHT" value="6.7mm"/>
<attribute name="LENGTH" value="12.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 176920512 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="2000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="10.7mm"/>
</technology>
<technology name="_176920522">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/176920522?ae"/>
<attribute name="HEIGHT" value="6.7mm"/>
<attribute name="LENGTH" value="12.75mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 176920522 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="2000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="10.7mm"/>
</technology>
</technologies>
</device>
<device name="_L13.2W11.4H7.25" package="WPME-FISM_SMT-8_L13.2W11.4H7.25">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="_1769205041">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769205041?ae"/>
<attribute name="HEIGHT" value="7.25mm"/>
<attribute name="LENGTH" value="13.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769205041 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.97 - 3.63Vin, 5Vout"/>
<attribute name="VIN" value="2.97 - 3.63V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_1769205341">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769205341?ae"/>
<attribute name="HEIGHT" value="7.25mm"/>
<attribute name="LENGTH" value="13.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769205341 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_1769405141">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769405141?ae"/>
<attribute name="HEIGHT" value="7.25mm"/>
<attribute name="LENGTH" value="13.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769405141 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_1769405241">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769405241?ae"/>
<attribute name="HEIGHT" value="7.25mm"/>
<attribute name="LENGTH" value="13.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769405241 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
<technology name="_1769405341">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769405341?ae"/>
<attribute name="HEIGHT" value="7.25mm"/>
<attribute name="LENGTH" value="13.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769405341 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.4mm"/>
</technology>
</technologies>
</device>
<device name="_1769205141" package="WPME-FISM_SMT-8_1769205141">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769205141?ae"/>
<attribute name="HEIGHT" value="6.25mm"/>
<attribute name="LENGTH" value="12.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769205141 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.05mm"/>
</technology>
</technologies>
</device>
<device name="_1769205241" package="WPME-FISM_SMT-8_1769205241">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="5"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1769205241?ae"/>
<attribute name="HEIGHT" value="6.25mm"/>
<attribute name="LENGTH" value="12.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 1769205241 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SMT-8"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="3000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="11.05mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WPME-FISM_SIP-4" prefix="U">
<description>&lt;b&gt;MagI³C-FISM Fixed Isolated SIP / SMT Module&lt;br&gt;
Unregulated output voltage&lt;br&gt;

&lt;br&gt;Characteristics
&lt;br&gt;
&lt;/B&gt;&lt;br&gt;Simple design (no transformer design know how required)
&lt;br&gt;Leaded through-hole package for easy manufacturing and prototyping
&lt;br&gt;Stand-alone solution (CIN and COUT integrated, no external components)
&lt;br&gt;Simple functional isolation for overvoltage protection, avoiding ground loops, ground shift and noise in signal path or sensor systems
&lt;br&gt;Industrial standard package and pin configuration
&lt;br&gt;Low conducted and radiated EMI (compliant to EN55022 class B)
&lt;br&gt;UL60950 certified
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;&lt;br&gt;&lt;/B&gt;Data acquisition
&lt;br&gt;Test and measurement systems
&lt;br&gt;Interface and microcontroller supply
&lt;br&gt;Industrial control
&lt;br&gt;
&lt;br&gt;

&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o84919v209%20Family-Magic-FISM-1779205x11-1779205x41-17694051.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o84919v209%20Family-Magic-FISM-1779205x11-1779205x41-17694051.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/MAGIC-FISM/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/MAGIC-FISM&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-05
&lt;br&gt;&lt;/b&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WPME-FISM_SIP-4"/>
</gates>
<devices>
<device name="_L11.5W6H10" package="WPME-FISM_SIP-4_L11.5W6H10">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="_177920501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/177920501?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 177920501 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="2.97 - 3.63Vin, 5Vout"/>
<attribute name="VIN" value="2.97 - 3.63V"/>
<attribute name="VISO" value="1000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_177920511">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/177920511?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 177920511 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="1000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_177920521">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/177920521?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 177920521 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="1000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
<technology name="_177920531">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/177920531?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 177920531 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="no"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="1000V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L11.6W6H10.16" package="WPME-FISM_SIP-4_L11.6W6H10.16">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="_1779205311">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779205311?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779205311 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="1500V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_L11.6W7.55H10.16" package="WPME-FISM_SIP-4_L11.6W7.55H10.16">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="_1779405111">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779405111?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779405111 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="1500V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
<technology name="_1779405211">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779405211?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779405211 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="1500V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
<technology name="_1779405311">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779405311?ae"/>
<attribute name="HEIGHT" value="10.16mm"/>
<attribute name="LENGTH" value="11.6mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779405311 "/>
<attribute name="PO" value="2W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="21.6 - 26.4Vin, 5Vout"/>
<attribute name="VIN" value="21.6 - 26.4V"/>
<attribute name="VISO" value="1500V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="7.05mm"/>
</technology>
</technologies>
</device>
<device name="_1779205111" package="WPME-FISM_SIP-4_1779205111">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779205111?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779205111 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="4.5 - 5.5Vin, 5Vout"/>
<attribute name="VIN" value="4.5 - 5.5V"/>
<attribute name="VISO" value="1500V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
<device name="_1779205211" package="WPME-FISM_SIP-4_1779205211">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/1779205211?ae"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LENGTH" value="11.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 1779205211 "/>
<attribute name="PO" value="1W"/>
<attribute name="SHORT-CIRCUIT-PROTECTION" value="continuous"/>
<attribute name="SIZE" value="SIP-4"/>
<attribute name="TYPE-OF-INSULATION" value="Functional"/>
<attribute name="VALUE" value="10.8 - 13.2Vin, 5Vout"/>
<attribute name="VIN" value="10.8 - 13.2V"/>
<attribute name="VISO" value="1500V"/>
<attribute name="VOUT" value="5V"/>
<attribute name="WIDTH" value="6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
