<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Coaxial Connectors - WR-SMP &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-04-14&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="60114602122404">
<description>&lt;b&gt;WR-SMP Straight</description>
</package>
<package name="60114102122403">
<description>&lt;B&gt;WR-SMP Straight</description>
</package>
<package name="60114202122305">
<description>&lt;B&gt;WR-SMP SMT Edge Card Extended Solder Leg for PCB 1.6 mm Max.</description>
</package>
<package name="60114002122502">
<description>&lt;b&gt;WR-SMP Straight</description>
</package>
<package name="60123002122501">
<description>&lt;B&gt;WR-SMP Right Angle</description>
</package>
<package name="60124202122305">
<description>&lt;B&gt;WR-SMP SMT Edge Card Extended Solder Leg for PCB 1.6 mm Max.</description>
</package>
<package name="60124102122403">
<description>&lt;B&gt;WR-SMP Straight</description>
</package>
<package name="60124002122502">
<description>&lt;B&gt;WR-SMP Straight</description>
</package>
<package name="60124602122404">
<description>&lt;b&gt;WR-SMP Straight</description>
</package>
</packages>
<symbols>
<symbol name="PLUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="60114102122403" prefix="J">
<description>&lt;b&gt; WR-SMP Straight&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176648v209%20Family_WR-SMP_60114102122403.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176648v209%20Family_WR-SMP_60114102122403.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_SMT_STRAIGHT/"&gt;https://www.we-online.com/catalog/en/SMP_SMT_STRAIGHT/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114102122403">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60114102122403.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60114102122403"/>
<attribute name="VALUE" value="60114102122403"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114602122404" prefix="J">
<description>&lt;b&gt; WR-SMP Straight&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176649v209%20Family_WR-SMP_60114602122404.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176649v209%20Family_WR-SMP_60114602122404.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_THR_STRAIGHT/"&gt;https://www.we-online.com/catalog/en/SMP_THR_STRAIGHT/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-04-14&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114602122404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60114602122404.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60114602122404"/>
<attribute name="VALUE" value="60114602122404"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114202122305" prefix="J">
<description>&lt;b&gt; WR-SMP SMT Edge Card Extended Solder Leg for PCB 1.6 mm Max.  &lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176650v209%20Family_WR-SMP_60114202122305.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176650v209%20Family_WR-SMP_60114202122305.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_END_LAUNCH_EDGE_CARD/"&gt;hhttps://www.we-online.com/catalog/en/SMP_END_LAUNCH_EDGE_CARD/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-04-14&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114202122305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60114202122305 .pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60114202122305 "/>
<attribute name="VALUE" value="60114202122305 "/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60123002122501" prefix="J">
<description>&lt;b&gt; WR-SMP Right Angle&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Right Angle 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176646v209%20Family_WR-SMP_60123002122501.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176646v209%20Family_WR-SMP_60123002122501.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_PCB_RIGHT_ANGLE/"&gt;https://www.we-online.com/catalog/en/SMP_PCB_RIGHT_ANGLE/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60123002122501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60123002122501.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Right Angle"/>
<attribute name="PART-NUMBER" value="60123002122501"/>
<attribute name="VALUE" value="60123002122501"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60114002122502" prefix="J">
<description>&lt;b&gt; WR-SMP Straight&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176647v209%20Family_WR-SMP_60114002122502.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176647v209%20Family_WR-SMP_60114002122502.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_PCB_STRAIGHT/"&gt;https://www.we-online.com/catalog/en/SMP_PCB_STRAIGHT/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60114002122502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60114002122502.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60114002122502"/>
<attribute name="VALUE" value="60114002122502"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124202122305" prefix="J">
<description>&lt;b&gt; WR-SMP SMT Edge Card Extended Solder Leg for PCB 1.6 mm Max.  &lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176650v209%20Family_WR-SMP_60114202122305.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176650v209%20Family_WR-SMP_60114202122305.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_END_LAUNCH_EDGE_CARD/"&gt;hhttps://www.we-online.com/catalog/en/SMP_END_LAUNCH_EDGE_CARD/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2021-04-14&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124202122305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60124202122305.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60124202122305"/>
<attribute name="VALUE" value="60124202122305"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124102122403" prefix="J">
<description>&lt;b&gt; WR-SMP Straight&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176648v209%20Family_WR-SMP_60114102122403.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176648v209%20Family_WR-SMP_60114102122403.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_SMT_STRAIGHT/"&gt;https://www.we-online.com/catalog/en/SMP_SMT_STRAIGHT/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124102122403">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60124102122403.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60124102122403"/>
<attribute name="VALUE" value="60124102122403"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124002122502" prefix="J">
<description>&lt;b&gt; WR-SMP Straight&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material PTFE 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176647v209%20Family_WR-SMP_60114002122502.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176647v209%20Family_WR-SMP_60114002122502.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_PCB_STRAIGHT/"&gt;https://www.we-online.com/catalog/en/SMP_PCB_STRAIGHT/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2020-05-29&lt;br&gt;
2020(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124002122502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60124002122502.pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60124002122502"/>
<attribute name="VALUE" value="60124002122502"/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="60124602122404" prefix="J">
<description>&lt;b&gt; WR-SMP Straight&lt;/b&gt;
&lt;b&gt;&lt;br&gt;&lt;br&gt;
MATERIAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Insulator Material LCP 
&lt;br&gt;Center Contact Material Brass 
&lt;br&gt;Center Contact Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;Body Material Brass 
&lt;br&gt;Body Plating Gold, min. 0.127 μm over Nickel 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;KIND PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Interface MIL-STD-348 
&lt;br&gt;Connector Type SMP 
&lt;br&gt;Gender Plug 
&lt;br&gt;Orientation Type Straight 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;GENERAL INFORMATION 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Operating Temperature -65 up to +165 °C  
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;ELECTRICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;f DC~12 GHz 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;MECHANICAL PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Mating Cycle 500 Cycles; 1000 Cycles 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;PACKAGING PROPERTIES 
&lt;br&gt;&lt;br&gt;
&lt;/b&gt;Packaging Tray 
&lt;br&gt;
 &lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o176649v209%20Family_WR-SMP_60114602122404.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o176649v209%20Family_WR-SMP_60114602122404.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/SMP_THR_STRAIGHT/"&gt;https://www.we-online.com/catalog/en/SMP_THR_STRAIGHT/&lt;/a&gt;&lt;p&gt;
Updated by Ella Wu 2021-04-14&lt;br&gt;
2021(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="PLUG"/>
</gates>
<devices>
<device name="" package="60124602122404">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2 3 4 5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/60124602122404 .pdf"/>
<attribute name="GENDER" value="Plug"/>
<attribute name="INTERFACE" value="MIL-STD-348"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="ORIENTATION-TYPE" value="Straight"/>
<attribute name="PART-NUMBER" value="60124602122404 "/>
<attribute name="VALUE" value="60124602122404 "/>
<attribute name="Z" value="50Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
