<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Switches - Micro Switches - WS-MITV&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021b, 2021-03-12&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="463091691402">
<description>&lt;B&gt;WS-MITV THT Terminal with Actuator, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;12.8 x 5.8 mm Right Angle Operation, THT, 3pins</description>
</package>
<package name="463092691402">
<description>&lt;B&gt;WS-MITV THT Terminal with Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;12.8 x 5.8 mm Right Angle Operation, THT, 3pins</description>
</package>
<package name="463091370402">
<description>&lt;B&gt;WS-MITV&lt;/B&gt; &lt;BR&gt; THT Terminal with Actuator Micro Switch, 12.8 x 5.8 mm</description>
</package>
<package name="463093370402">
<description>&lt;B&gt;WS-MITV&lt;/B&gt; &lt;BR&gt;THT Terminal with Roller Lever Micro Switch, 12.8 x 5.8 mm</description>
</package>
<package name="463093691402">
<description>&lt;B&gt;WS-MITV THT Terminal with Roller Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;12.8 x 5.8 mm Right Angle Operation, THT, 3pins</description>
</package>
<package name="463092370402">
<description>&lt;B&gt;WS-MITV&lt;/B&gt;&lt;BR&gt; THT Terminal with Lever Micro Switch, 12.8 x 5.8 mm</description>
</package>
</packages>
<symbols>
<symbol name="WS-MITV-3">
<description>WS-MITV</description>
<pin name="NO" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WS-MITV-2">
<description>WS-MITV</description>
<pin name="NO" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WS-MITV-1">
<description>WS-MITV</description>
<pin name="NO" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WS-MITV">
<description>WS-MITV</description>
<pin name="NO" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="463091691402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Actuator, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material PBT 
&lt;BR&gt; Actuator Flammability Rating UL94 V-0 
&lt;BR&gt; Actuator Color White 
&lt;BR&gt; Frame Material PBT 
&lt;BR&gt; Frame Flammability Rating UL94 V-0 
&lt;BR&gt; Moveable Contact Material Silver 
&lt;BR&gt; Stationary Contact Material Silver 
&lt;BR&gt; Terminal Material Copper Alloy 
&lt;BR&gt; Terminal Plating Silver 
&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Mechanical Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Position 5.5 mm 
&lt;BR&gt;Pre-travel 0.5 mm 
&lt;BR&gt;Over travel 0.25 mm 
&lt;BR&gt;Movement Differential 0.12 mm 
&lt;BR&gt;Electrical Life 10000 Cycles 
&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging Tray 

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o320306v209%20Family_WS-MITV_463091691402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o320306v209%20Family_WS-MITV_463091691402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MITV_THT_TERMINAL_ACTUATOR_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8"&gt;https://www.we-online.com/catalog/en/MITV_THT_TERMINAL_ACTUATOR_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2021-03-12&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463091691402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/463091691402.pdf"/>
<attribute name="OPERATION-FORCE" value=" 150 "/>
<attribute name="PART-NUMBER" value="463091691402"/>
<attribute name="RELEASING-FORCE" value=" 20 "/>
<attribute name="VALUE" value="463091691402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463092691402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material PBT 
&lt;BR&gt; Actuator Flammability Rating UL94 V-0 
&lt;BR&gt; Actuator Color White 
&lt;BR&gt; Frame Material PBT 
&lt;BR&gt; Frame Flammability Rating UL94 V-0 
&lt;BR&gt; Moveable Contact Material Silver 
&lt;BR&gt; Stationary Contact Material Silver 
&lt;BR&gt; Terminal Material Copper Alloy 
&lt;BR&gt; Terminal Plating Silver 

&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Mechanical Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Position 6.8 mm 
&lt;BR&gt;Over travel 0.55 mm 
&lt;BR&gt;Movement Differential 0.5 mm 
&lt;BR&gt;Electrical Life 10000 Cycles 

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 
&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging Tray 

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o320310v209%20Family_WS-MITV_463092691402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o320310v209%20Family_WS-MITV_463092691402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MITV_THT_TERMINAL_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8"&gt;https://www.we-online.com/catalog/en/MITV_THT_TERMINAL_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2021-03-12&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463092691402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/463092691402.pdf"/>
<attribute name="OPERATION-FORCE" value=" 80 "/>
<attribute name="PART-NUMBER" value="463092691402"/>
<attribute name="RELEASING-FORCE" value=" 5 "/>
<attribute name="VALUE" value="463092691402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463091370402" prefix="S">
<description>&lt;b&gt;WS-MITV WS-MITV THT Terminal with Actuator Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Mechanical Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operation Force:250 g
&lt;BR&gt;Releasing Force:20 g
&lt;br&gt;Operating Position:5.5 mm
&lt;br&gt;Pre-travel (Value):0.5 mm
&lt;br&gt;Over travel (Value):0.25 mm
&lt;br&gt;Movement Differential:0.12 mm
&lt;br&gt;Electrical Life:10000 Cycles
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Flammability Rating:UL94 V-0
&lt;br&gt;Actuator Color:White
&lt;br&gt;Frame Material:PBT
&lt;br&gt;Frame Flammability Rating:UL94 V-0
&lt;br&gt;Moveable Contact Material:Silver
&lt;br&gt;Stationary Contact:Silver
&lt;br&gt;Terminal Material:Copper Alloy
&lt;br&gt;Terminal Plating:Silver
&lt;br&gt;RISO:100 MΩ
&lt;br&gt;Schematic:SPDT
&lt;br&gt;Actuator Material:PBT

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tray&lt;BR&gt;&lt;br&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o144880v209%20Single_WE-MITV_463091370402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o144880v209%20Single_WE-MITV_463091370402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MITV_19_8X6_4_THT_ACTUATOR_LEFT_240GF/"&gt;https://www.we-online.com/catalog/en/MITV_19_8X6_4_THT_ACTUATOR_LEFT_240GF/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463091370402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/463091370402.pdf"/>
<attribute name="OPERATION-FORCE" value=" 150 "/>
<attribute name="PART-NUMBER" value="463091370402"/>
<attribute name="QTY" value=" 100 "/>
<attribute name="SCHEMATIC" value="SPDT"/>
<attribute name="VALUE" value="463091370402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463093370402" prefix="S">
<description>&lt;b&gt;WS-MITV WS-MITV THT Terminal with Roller Lever Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Mechanical Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Releasing Force:5 g
&lt;BR&gt; Operating Position:13 mm
&lt;BR&gt; Over travel (Value):0.55 mm
&lt;BR&gt; Movement Differential:0.5 mm
&lt;BR&gt; Electrical Life:10000 Cycles
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Flammability Rating:UL94 V-0
&lt;br&gt;Actuator Color:White
&lt;br&gt;Frame Material:PBT
&lt;br&gt;Frame Flammability Rating:UL94 V-0
&lt;br&gt;Moveable Contact Material:Silver
&lt;br&gt;Stationary Contact:Silver
&lt;br&gt;Terminal Material:Copper Alloy
&lt;br&gt;Terminal Plating:Silver
&lt;br&gt;RISO:100 MΩ
&lt;br&gt;Schematic:SPDT
&lt;br&gt;Actuator Material:PBT

&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tray&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o144911v209%20Single_WE-MITV_463092370402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o144911v209%20Single_WE-MITV_463092370402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MITV_19_8X6_4_THT_LEVER_RIGHT_55GF/"&gt;https://www.we-online.com/catalog/en/MITV_19_8X6_4_THT_LEVER_RIGHT_55GF/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463093370402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/463093370402.pdf"/>
<attribute name="OPERATION-FORCE" value=" 80 "/>
<attribute name="PART-NUMBER" value="463093370402"/>
<attribute name="QTY" value=" 70 "/>
<attribute name="SCHEMATIC" value="SPDT"/>
<attribute name="VALUE" value="463093370402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463093691402" prefix="S">
<description>&lt;b&gt;WS-MITV THT Terminal with Roller Lever, Right Angle Operation Micro Switch, 12.8 x 5.8 mm
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Material Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Material PBT 
&lt;BR&gt; Actuator Flammability Rating UL94 V-0 
&lt;BR&gt; Actuator Color White 
&lt;BR&gt; Frame Material PBT 
&lt;BR&gt; Frame Flammability Rating UL94 V-0 
&lt;BR&gt; Moveable Contact Material Silver 
&lt;BR&gt; Stationary Contact Material Silver 
&lt;BR&gt; Terminal Material Copper Alloy 
&lt;BR&gt; Terminal Plating Silver 

&lt;BR&gt;
&lt;br&gt;&lt;b&gt;Mechanical Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Operating Position 13 mm 
&lt;BR&gt;Over travel 0.55 mm 
&lt;BR&gt;Movement Differential 0.5 mm 
&lt;BR&gt;Electrical Life 10000 Cycles 


&lt;BR&gt;&lt;BR&gt;
&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature -40 up to +85 °C 

&lt;BR&gt;&lt;br&gt;
&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging Tray 

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o320308v209%20Family_WS-MITV_463093691402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o320308v209%20Family_WS-MITV_463093691402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MITV_THT_TERMINAL_ROLLER_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8"&gt;https://www.we-online.com/catalog/en/MITV_THT_TERMINAL_ROLLER_LEVER_RIGHT_ANGLE_MICRO_SWITCH_12_8X5_8&lt;/a&gt;&lt;p&gt;

Created by Ella Wu, 2021-03-12&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463093691402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/463093691402.pdf"/>
<attribute name="OPERATION-FORCE" value=" 80 "/>
<attribute name="PART-NUMBER" value="463093691402"/>
<attribute name="RELEASING-FORCE" value=" 5 "/>
<attribute name="VALUE" value="463093691402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="463092370402" prefix="S">
<description>&lt;b&gt;WS-MITV WS-MITV THT Terminal with Lever Micro Switch, 12.8 x 5.8 mm 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Mechanical Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Releasing Force:5 g
&lt;br&gt;Operating Position:6.8 mm
&lt;br&gt;Over travel (Value):0.55 mm
&lt;br&gt;Movement Differential:0.5 mm
&lt;br&gt;Electrical Life:10000 Cycles
&lt;BR&gt;

&lt;br&gt;&lt;b&gt;Properties
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Actuator Color:White
Frame Material:PBT
Frame Flammability Rating:UL94 V-0
Moveable Contact Material:Silver
Stationary Contact:Silver
Terminal Material:Copper Alloy
Terminal Plating:Silver
RISO:100 MΩ
Schematic:SPDT
Actuator Material:PBT
&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;Packaging Properties&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Packaging:Tray&lt;BR&gt;&lt;BR&gt;

&lt;b&gt;General Information&lt;/b&gt;&lt;BR&gt;
&lt;BR&gt;Operating Temperature:-40 up to +85 °C

&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o144915v209%20Single_WE-MITV_463093370402.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o144915v209%20Single_WE-MITV_463093370402.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/MITV_19_8X6_4_THT_ROLLER_LEVER_LEFT_55GF/"&gt;https://www.we-online.com/catalog/en/MITV_19_8X6_4_THT_ROLLER_LEVER_LEFT_55GF/&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu, 2021-02-08&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WS-MITV"/>
</gates>
<devices>
<device name="" package="463092370402">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NO" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/463092370402.pdf"/>
<attribute name="OPERATION-FORCE" value=" 80 "/>
<attribute name="PART-NUMBER" value="463092370402"/>
<attribute name="QTY" value=" 100 "/>
<attribute name="SCHEMATIC" value="SPDT"/>
<attribute name="VALUE" value="463092370402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
